<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_H6IccNfyEe-1u6dpesWcRg" mediniIdentifier="_H6IccNfyEe-1u6dpesWcRg" name="HARA F020 B 21.01.25">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YBEq0NfyEe-1u6dpesWcRg" mediniIdentifier="_YBEq0NfyEe-1u6dpesWcRg" id="HE71176" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YBEq0dfyEe-1u6dpesWcRg" mediniIdentifier="_YBEq0dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHIWMIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YBkaENfyEe-1u6dpesWcRg" mediniIdentifier="_YBkaENfyEe-1u6dpesWcRg" id="HE71179" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YBkaEdfyEe-1u6dpesWcRg" mediniIdentifier="_YBkaEdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHIWMIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YCzJINfyEe-1u6dpesWcRg" mediniIdentifier="_YCzJINfyEe-1u6dpesWcRg" id="HE71187" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YCzJIdfyEe-1u6dpesWcRg" mediniIdentifier="_YCzJIdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHIWMIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YC86INfyEe-1u6dpesWcRg" mediniIdentifier="_YC86INfyEe-1u6dpesWcRg" id="HE71188" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YC86IdfyEe-1u6dpesWcRg" mediniIdentifier="_YC86IdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHIWMIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YESW4NfyEe-1u6dpesWcRg" mediniIdentifier="_YESW4NfyEe-1u6dpesWcRg" id="HE71197" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YESW4dfyEe-1u6dpesWcRg" mediniIdentifier="_YESW4dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHIWMIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YFWG0NfyEe-1u6dpesWcRg" mediniIdentifier="_YFWG0NfyEe-1u6dpesWcRg" id="HE71204" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YFWG0dfyEe-1u6dpesWcRg" mediniIdentifier="_YFWG0dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHFS4IIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YFyLsNfyEe-1u6dpesWcRg" mediniIdentifier="_YFyLsNfyEe-1u6dpesWcRg" id="HE71207" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YFyLsdfyEe-1u6dpesWcRg" mediniIdentifier="_YFyLsdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHFS4IIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YG_soNfyEe-1u6dpesWcRg" mediniIdentifier="_YG_soNfyEe-1u6dpesWcRg" id="HE71215" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YG_sodfyEe-1u6dpesWcRg" mediniIdentifier="_YG_sodfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHFS4IIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YHJdoNfyEe-1u6dpesWcRg" mediniIdentifier="_YHJdoNfyEe-1u6dpesWcRg" id="HE71216" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YHJdodfyEe-1u6dpesWcRg" mediniIdentifier="_YHJdodfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHFS4IIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YIgvkNfyEe-1u6dpesWcRg" mediniIdentifier="_YIgvkNfyEe-1u6dpesWcRg" id="HE71225" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YIgvkdfyEe-1u6dpesWcRg" mediniIdentifier="_YIgvkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHFS4IIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YJlGkNfyEe-1u6dpesWcRg" mediniIdentifier="_YJlGkNfyEe-1u6dpesWcRg" id="HE71232" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YJlGkdfyEe-1u6dpesWcRg" mediniIdentifier="_YJlGkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHHvIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YKCZkNfyEe-1u6dpesWcRg" mediniIdentifier="_YKCZkNfyEe-1u6dpesWcRg" id="HE71235" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YKCZkdfyEe-1u6dpesWcRg" mediniIdentifier="_YKCZkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHHvIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YLZEcNfyEe-1u6dpesWcRg" mediniIdentifier="_YLZEcNfyEe-1u6dpesWcRg" id="HE71243" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YLZEcdfyEe-1u6dpesWcRg" mediniIdentifier="_YLZEcdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHHvIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YLjcgNfyEe-1u6dpesWcRg" mediniIdentifier="_YLjcgNfyEe-1u6dpesWcRg" id="HE71244" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YLjcgdfyEe-1u6dpesWcRg" mediniIdentifier="_YLjcgdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHHvIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YNG7sNfyEe-1u6dpesWcRg" mediniIdentifier="_YNG7sNfyEe-1u6dpesWcRg" id="HE71253" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YNG7sdfyEe-1u6dpesWcRg" mediniIdentifier="_YNG7sdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHHvIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YOMg0NfyEe-1u6dpesWcRg" mediniIdentifier="_YOMg0NfyEe-1u6dpesWcRg" id="HE71260" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YOMg0dfyEe-1u6dpesWcRg" mediniIdentifier="_YOMg0dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKycIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YOqa4NfyEe-1u6dpesWcRg" mediniIdentifier="_YOqa4NfyEe-1u6dpesWcRg" id="HE71263" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YOqa4dfyEe-1u6dpesWcRg" mediniIdentifier="_YOqa4dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKycIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YP2tsNfyEe-1u6dpesWcRg" mediniIdentifier="_YP2tsNfyEe-1u6dpesWcRg" id="HE71271" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YP2tsdfyEe-1u6dpesWcRg" mediniIdentifier="_YP2tsdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKycIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YQAesNfyEe-1u6dpesWcRg" mediniIdentifier="_YQAesNfyEe-1u6dpesWcRg" id="HE71272" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YQAesdfyEe-1u6dpesWcRg" mediniIdentifier="_YQAesdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKycIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YRXJkNfyEe-1u6dpesWcRg" mediniIdentifier="_YRXJkNfyEe-1u6dpesWcRg" id="HE71281" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YRXJkdfyEe-1u6dpesWcRg" mediniIdentifier="_YRXJkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKycIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YSd80NfyEe-1u6dpesWcRg" mediniIdentifier="_YSd80NfyEe-1u6dpesWcRg" id="HE71288" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YSd80dfyEe-1u6dpesWcRg" mediniIdentifier="_YSd80dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMAkIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YS724NfyEe-1u6dpesWcRg" mediniIdentifier="_YS724NfyEe-1u6dpesWcRg" id="HE71291" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YS724dfyEe-1u6dpesWcRg" mediniIdentifier="_YS724dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMAkIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YUJX0NfyEe-1u6dpesWcRg" mediniIdentifier="_YUJX0NfyEe-1u6dpesWcRg" id="HE71299" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YUJX0dfyEe-1u6dpesWcRg" mediniIdentifier="_YUJX0dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMAkIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YUShwNfyEe-1u6dpesWcRg" mediniIdentifier="_YUShwNfyEe-1u6dpesWcRg" id="HE71300" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YUShwdfyEe-1u6dpesWcRg" mediniIdentifier="_YUShwdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMAkIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YVpMoNfyEe-1u6dpesWcRg" mediniIdentifier="_YVpMoNfyEe-1u6dpesWcRg" id="HE71309" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YVpModfyEe-1u6dpesWcRg" mediniIdentifier="_YVpModfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMAkIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YWs8kNfyEe-1u6dpesWcRg" mediniIdentifier="_YWs8kNfyEe-1u6dpesWcRg" id="HE71316" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YWs8kdfyEe-1u6dpesWcRg" mediniIdentifier="_YWs8kdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHJkUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YXKPkNfyEe-1u6dpesWcRg" mediniIdentifier="_YXKPkNfyEe-1u6dpesWcRg" id="HE71319" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YXKPkdfyEe-1u6dpesWcRg" mediniIdentifier="_YXKPkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHJkUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YYXwgNfyEe-1u6dpesWcRg" mediniIdentifier="_YYXwgNfyEe-1u6dpesWcRg" id="HE71327" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YYXwgdfyEe-1u6dpesWcRg" mediniIdentifier="_YYXwgdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHJkUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YYhhgNfyEe-1u6dpesWcRg" mediniIdentifier="_YYhhgNfyEe-1u6dpesWcRg" id="HE71328" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YYhhgdfyEe-1u6dpesWcRg" mediniIdentifier="_YYhhgdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHJkUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YZ6BkNfyEe-1u6dpesWcRg" mediniIdentifier="_YZ6BkNfyEe-1u6dpesWcRg" id="HE71337" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YZ6BkdfyEe-1u6dpesWcRg" mediniIdentifier="_YZ6BkdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHJkUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YbFtUNfyEe-1u6dpesWcRg" mediniIdentifier="_YbFtUNfyEe-1u6dpesWcRg" id="HE71344" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_ja49UJHWEe-rf_mtY6CvyA"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YbFtUdfyEe-1u6dpesWcRg" mediniIdentifier="_YbFtUdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHGhAIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YbjAUNfyEe-1u6dpesWcRg" mediniIdentifier="_YbjAUNfyEe-1u6dpesWcRg" id="HE71347" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_ja49UJHWEe-rf_mtY6CvyA"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YbjAUdfyEe-1u6dpesWcRg" mediniIdentifier="_YbjAUdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHGhAIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Ycv6MNfyEe-1u6dpesWcRg" mediniIdentifier="_Ycv6MNfyEe-1u6dpesWcRg" id="HE71355" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_ja49UJHWEe-rf_mtY6CvyA"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Ycv6MdfyEe-1u6dpesWcRg" mediniIdentifier="_Ycv6MdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHGhAIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Yc5EINfyEe-1u6dpesWcRg" mediniIdentifier="_Yc5EINfyEe-1u6dpesWcRg" id="HE71356" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_ja49UJHWEe-rf_mtY6CvyA"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yc5EIdfyEe-1u6dpesWcRg" mediniIdentifier="_Yc5EIdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHGhAIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YeQ9INfyEe-1u6dpesWcRg" mediniIdentifier="_YeQ9INfyEe-1u6dpesWcRg" id="HE71365" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_ja49UJHWEe-rf_mtY6CvyA"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YeQ9IdfyEe-1u6dpesWcRg" mediniIdentifier="_YeQ9IdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHGhAIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YfUGANfyEe-1u6dpesWcRg" mediniIdentifier="_YfUGANfyEe-1u6dpesWcRg" id="HE71372" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YfUGAdfyEe-1u6dpesWcRg" mediniIdentifier="_YfUGAdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMnoIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Yfwx8NfyEe-1u6dpesWcRg" mediniIdentifier="_Yfwx8NfyEe-1u6dpesWcRg" id="HE71375" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yfwx8dfyEe-1u6dpesWcRg" mediniIdentifier="_Yfwx8dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMnoIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Yg9r0NfyEe-1u6dpesWcRg" mediniIdentifier="_Yg9r0NfyEe-1u6dpesWcRg" id="HE71383" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yg9r0dfyEe-1u6dpesWcRg" mediniIdentifier="_Yg9r0dfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMnoIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YhG1wNfyEe-1u6dpesWcRg" mediniIdentifier="_YhG1wNfyEe-1u6dpesWcRg" id="HE71384" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YhG1wdfyEe-1u6dpesWcRg" mediniIdentifier="_YhG1wdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMnoIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Yic5kNfyEe-1u6dpesWcRg" mediniIdentifier="_Yic5kNfyEe-1u6dpesWcRg" id="HE71393" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yic5kdfyEe-1u6dpesWcRg" mediniIdentifier="_Yic5kdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHMnoIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YjgpgNfyEe-1u6dpesWcRg" mediniIdentifier="_YjgpgNfyEe-1u6dpesWcRg" id="HE71400" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YjgpgdfyEe-1u6dpesWcRg" mediniIdentifier="_YjgpgdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKLYIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Yj9VcNfyEe-1u6dpesWcRg" mediniIdentifier="_Yj9VcNfyEe-1u6dpesWcRg" id="HE71403" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yj9VcdfyEe-1u6dpesWcRg" mediniIdentifier="_Yj9VcdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKLYIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YlK2YNfyEe-1u6dpesWcRg" mediniIdentifier="_YlK2YNfyEe-1u6dpesWcRg" id="HE71411" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YlK2YdfyEe-1u6dpesWcRg" mediniIdentifier="_YlK2YdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKLYIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YlUnYNfyEe-1u6dpesWcRg" mediniIdentifier="_YlUnYNfyEe-1u6dpesWcRg" id="HE71412" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YlUnYdfyEe-1u6dpesWcRg" mediniIdentifier="_YlUnYdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKLYIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YmsgYNfyEe-1u6dpesWcRg" mediniIdentifier="_YmsgYNfyEe-1u6dpesWcRg" id="HE71421" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;Assumption is battery protection circuit is protecting the critical faults, it's not cascading, dependant and dual point fialure is no applicable. The info is of voltage and current.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YmsgYdfyEe-1u6dpesWcRg" mediniIdentifier="_YmsgYdfyEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hHKLYIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
