<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_aDX40AX3Eeq4AMRV0u5rew" mediniIdentifier="_aDX40AX3Eeq4AMRV0u5rew" name="P-11 Table 51 - PLD: Signal Routing Capability">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_rEmy8AX8Eeq4AMRV0u5rew" mediniIdentifier="_rEmy8AX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.5.1" name="One-bit hardware redundancy" maxDC="LOW" notes="-"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_rEmy8QX8Eeq4AMRV0u5rew" mediniIdentifier="_rEmy8QX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.5.2" name="Multi-bit hardware redundancy (including ECC)" maxDC="MEDIUM" notes="Multi-bit redundancy can achieve high coverage by proper interleaving of data, address and control lines, and if combined with some complete redundancy e.g. for the arbiter."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_rEmy8gX8Eeq4AMRV0u5rew" mediniIdentifier="_rEmy8gX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.5.3" name="Complete hardware redundancy" maxDC="HIGH" notes="Common failure modes can reduce diagnostic coverage."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_rEmy8wX8Eeq4AMRV0u5rew" mediniIdentifier="_rEmy8wX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.5.4" name="Inspection using test patterns" maxDC="HIGH" notes="Depends on type of pattern"/>
</safety:MeasureCatalog>
