<?xml version="1.1" encoding="UTF-8"?>
<sysml:SysMLContainerPackage xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:sysml="http://www.ikv.de/medini/sysml/1.0" xmi:id="_Z3Gk4NL7Ee-Sld_1EWpoOA" mediniIdentifier="_Z3Gk4NL7Ee-Sld_1EWpoOA" name="MCAL">
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_f6TdcNL7Ee-Sld_1EWpoOA" mediniIdentifier="_f6TdcNL7Ee-Sld_1EWpoOA" typeCode="Component" user_kind="internal" user_circuit_block=""/>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_-M8VgNL7Ee-Sld_1EWpoOA" mediniIdentifier="_-M8VgNL7Ee-Sld_1EWpoOA" typeCode="Software Unit" name="MCAL" user_kind="internal" user_circuit_block="">
    <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_FNaHkNL8Ee-Sld_1EWpoOA" mediniIdentifier="_FNaHkNL8Ee-Sld_1EWpoOA" typeCode="Software Unit" name="MCU API Layer" the_relationship_of_source="_76Vu0NL9Ee-Sld_1EWpoOA _lyLZUNMHEe-Sld_1EWpoOA _HB_0MNMIEe-Sld_1EWpoOA" user_kind="internal" user_circuit_block="">
      <the_owned_elements xsi:type="sysml:SysMLPortUsage" xmi:id="_ibVaUNL8Ee-Sld_1EWpoOA" mediniIdentifier="_ibVaUNL8Ee-Sld_1EWpoOA" name="Application requests" the_relationship_of_source="_mXrUENL8Ee-Sld_1EWpoOA"/>
      <dependencies xsi:type="sysml:SysMLDependency" xmi:id="_lyLZUNMHEe-Sld_1EWpoOA" mediniIdentifier="_lyLZUNMHEe-Sld_1EWpoOA" the_source_element="_FNaHkNL8Ee-Sld_1EWpoOA" the_target_element="_QghlINL9Ee-Sld_1EWpoOA"/>
      <connectors xsi:type="sysml:SysMLConnector" xmi:id="_mXrUENL8Ee-Sld_1EWpoOA" mediniIdentifier="_mXrUENL8Ee-Sld_1EWpoOA" the_source_element="_ibVaUNL8Ee-Sld_1EWpoOA" the_target_element="_d6JHENL8Ee-Sld_1EWpoOA">
        <theConnectorEnd xmi:id="_mXrUEtL8Ee-Sld_1EWpoOA" mediniIdentifier="_mXrUEtL8Ee-Sld_1EWpoOA" role="_ibVaUNL8Ee-Sld_1EWpoOA"/>
        <theConnectorEnd xmi:id="_mXr7INL8Ee-Sld_1EWpoOA" mediniIdentifier="_mXr7INL8Ee-Sld_1EWpoOA" role="_d6JHENL8Ee-Sld_1EWpoOA"/>
      </connectors>
      <connectors xsi:type="sysml:SysMLConnector" xmi:id="_76Vu0NL9Ee-Sld_1EWpoOA" mediniIdentifier="_76Vu0NL9Ee-Sld_1EWpoOA" name="MCU_Init_Request" the_source_element="_FNaHkNL8Ee-Sld_1EWpoOA" the_target_element="_QghlINL9Ee-Sld_1EWpoOA">
        <theConnectorEnd xmi:id="_76Vu0tL9Ee-Sld_1EWpoOA" mediniIdentifier="_76Vu0tL9Ee-Sld_1EWpoOA" role="_FNaHkNL8Ee-Sld_1EWpoOA"/>
        <theConnectorEnd xmi:id="_76Vu09L9Ee-Sld_1EWpoOA" mediniIdentifier="_76Vu09L9Ee-Sld_1EWpoOA" role="_QghlINL9Ee-Sld_1EWpoOA"/>
      </connectors>
      <connectors xsi:type="sysml:SysMLConnector" xmi:id="_HB_0MNMIEe-Sld_1EWpoOA" mediniIdentifier="_HB_0MNMIEe-Sld_1EWpoOA" the_source_element="_FNaHkNL8Ee-Sld_1EWpoOA" the_target_element="_QghlINL9Ee-Sld_1EWpoOA">
        <theConnectorEnd xmi:id="_HCAbQNMIEe-Sld_1EWpoOA" mediniIdentifier="_HCAbQNMIEe-Sld_1EWpoOA" role="_FNaHkNL8Ee-Sld_1EWpoOA"/>
        <theConnectorEnd xmi:id="_HCAbQdMIEe-Sld_1EWpoOA" mediniIdentifier="_HCAbQdMIEe-Sld_1EWpoOA" role="_QghlINL9Ee-Sld_1EWpoOA"/>
      </connectors>
    </the_owned_elements>
    <the_owned_elements xsi:type="sysml:SysMLPortUsage" xmi:id="_d6JHENL8Ee-Sld_1EWpoOA" mediniIdentifier="_d6JHENL8Ee-Sld_1EWpoOA" name="Application requests" the_relationship_of_target="_mXrUENL8Ee-Sld_1EWpoOA"/>
    <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_QghlINL9Ee-Sld_1EWpoOA" mediniIdentifier="_QghlINL9Ee-Sld_1EWpoOA" typeCode="Software Unit" name="MCU_Init_Module" the_relationship_of_source="_Z7zBMNMHEe-Sld_1EWpoOA" the_relationship_of_target="_76Vu0NL9Ee-Sld_1EWpoOA _lyLZUNMHEe-Sld_1EWpoOA _HB_0MNMIEe-Sld_1EWpoOA" user_kind="internal" user_circuit_block="">
      <the_owned_elements xsi:type="sysml:SysMLActivity" xmi:id="_DcIsUNL-Ee-Sld_1EWpoOA" mediniIdentifier="_DcIsUNL-Ee-Sld_1EWpoOA" typeCode="function" name="ivec_mcuInit" description="This function initialises:&#xD;&#xA;&#x9;MCU driver&#xD;&#xA;&#x9;PLL and MCU specific clock options&#xD;&#xA;&#x9;Activates the PLL clock to the MCU clock distribution&#xD;&#xA;&#x9;Sets the MCU power mode&#xD;&#xA;&#x9;Platform settings based on user configuration&#xD;&#xA;&#x9;The configured interrupts at interrupt controller level&#xD;&#xA;&#x9;OSIF system timer" id="F027">
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_PwvcENL_Ee-Sld_1EWpoOA" mediniIdentifier="_PwvcENL_Ee-Sld_1EWpoOA" name="Call function &quot;Mcu_Init&quot;, void type so no need to check return" theIncomingEdge="_VHx8wNMAEe-Sld_1EWpoOA" theOutgoingEdge="_6fNGMNMAEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_6fNGMNMAEe-Sld_1EWpoOA" mediniIdentifier="_6fNGMNMAEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_PwvcENL_Ee-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_vRURcNMAEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLInitialNode" xmi:id="_T6RAwNMAEe-Sld_1EWpoOA" mediniIdentifier="_T6RAwNMAEe-Sld_1EWpoOA" theOutgoingEdge="_VHx8wNMAEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_VHx8wNMAEe-Sld_1EWpoOA" mediniIdentifier="_VHx8wNMAEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_T6RAwNMAEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_PwvcENL_Ee-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLObjectNode" xmi:id="_t_6T8NMAEe-Sld_1EWpoOA" mediniIdentifier="_t_6T8NMAEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_vRURcNMAEe-Sld_1EWpoOA" mediniIdentifier="_vRURcNMAEe-Sld_1EWpoOA" name="Call function &quot;Mcu_InitClock&quot; with apt Clock configuration, void type so no need to check return" theIncomingEdge="_6fNGMNMAEe-Sld_1EWpoOA" theOutgoingEdge="_Xm1jsNMBEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_Xm1jsNMBEe-Sld_1EWpoOA" mediniIdentifier="_Xm1jsNMBEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_vRURcNMAEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_KmR3cNMBEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_KmR3cNMBEe-Sld_1EWpoOA" mediniIdentifier="_KmR3cNMBEe-Sld_1EWpoOA" name="Initialise local counter count_mcuPllLocked_u8 to 0." theIncomingEdge="_Xm1jsNMBEe-Sld_1EWpoOA" theOutgoingEdge="_oBGPUNMEEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_oBGPUNMEEe-Sld_1EWpoOA" mediniIdentifier="_oBGPUNMEEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_KmR3cNMBEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_FNnM0NMFEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_ZgB58NMBEe-Sld_1EWpoOA" mediniIdentifier="_ZgB58NMBEe-Sld_1EWpoOA" name="Mcu_GetPllStatus "/>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_HfyyMNMCEe-Sld_1EWpoOA" mediniIdentifier="_HfyyMNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_TEN3oNMCEe-Sld_1EWpoOA" mediniIdentifier="_TEN3oNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_UNa7YNMCEe-Sld_1EWpoOA" mediniIdentifier="_UNa7YNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLForkJoin" xmi:id="_V2cHoNMCEe-Sld_1EWpoOA" mediniIdentifier="_V2cHoNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLStructuredActivity" xmi:id="_XlMIcNMCEe-Sld_1EWpoOA" mediniIdentifier="_XlMIcNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_ZjfoMNMCEe-Sld_1EWpoOA" mediniIdentifier="_ZjfoMNMCEe-Sld_1EWpoOA"/>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_oA_hoNMEEe-Sld_1EWpoOA" mediniIdentifier="_oA_hoNMEEe-Sld_1EWpoOA" name="Mcu_GetPllStatus != MCU_PLL_LOCKED&#xD;&#xA;" theIncomingEdge="_HySwENMFEe-Sld_1EWpoOA" theOutgoingEdge="_8CdE0NMEEe-Sld_1EWpoOA __KAroNMEEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_8CdE0NMEEe-Sld_1EWpoOA" mediniIdentifier="_8CdE0NMEEe-Sld_1EWpoOA" name="NO" theNodeOfTheOutgoingEdge="_oA_hoNMEEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_4gFxUNMEEe-Sld_1EWpoOA"/>
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="__KAroNMEEe-Sld_1EWpoOA" mediniIdentifier="__KAroNMEEe-Sld_1EWpoOA" name="YES" theNodeOfTheOutgoingEdge="_oA_hoNMEEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_3MKrUNMEEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_3MKrUNMEEe-Sld_1EWpoOA" mediniIdentifier="_3MKrUNMEEe-Sld_1EWpoOA" name="Call function &quot;Mcu_DistributePllClock&quot;, void type so no need to check return" theIncomingEdge="__KAroNMEEe-Sld_1EWpoOA" theOutgoingEdge="_FCpdgNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_FCpdgNMGEe-Sld_1EWpoOA" mediniIdentifier="_FCpdgNMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_3MKrUNMEEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_xaSW0NMFEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_4gFxUNMEEe-Sld_1EWpoOA" mediniIdentifier="_4gFxUNMEEe-Sld_1EWpoOA" name="Increment count_mcuPllLocked_u8" theIncomingEdge="_8CdE0NMEEe-Sld_1EWpoOA" theOutgoingEdge="_jjwr4NMFEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_jjwr4NMFEe-Sld_1EWpoOA" mediniIdentifier="_jjwr4NMFEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_4gFxUNMEEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_ZVIUsNMFEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_FNnM0NMFEe-Sld_1EWpoOA" mediniIdentifier="_FNnM0NMFEe-Sld_1EWpoOA" name="Call function &quot;Mcu_GetPllStatus&quot;" theIncomingEdge="_oBGPUNMEEe-Sld_1EWpoOA _ld3BENMFEe-Sld_1EWpoOA" theOutgoingEdge="_HySwENMFEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_HySwENMFEe-Sld_1EWpoOA" mediniIdentifier="_HySwENMFEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_FNnM0NMFEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_oA_hoNMEEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLDecisionMerge" xmi:id="_ZVIUsNMFEe-Sld_1EWpoOA" mediniIdentifier="_ZVIUsNMFEe-Sld_1EWpoOA" name="count_mcuPllLocked_u8 &lt;&#xD;&#xA;MCU_PLL_LOCKED_COUNT_U8" theIncomingEdge="_jjwr4NMFEe-Sld_1EWpoOA" theOutgoingEdge="_ld3BENMFEe-Sld_1EWpoOA _vlF6UNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_ld3BENMFEe-Sld_1EWpoOA" mediniIdentifier="_ld3BENMFEe-Sld_1EWpoOA" name="YES" theNodeOfTheOutgoingEdge="_ZVIUsNMFEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_FNnM0NMFEe-Sld_1EWpoOA"/>
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_vlF6UNMGEe-Sld_1EWpoOA" mediniIdentifier="_vlF6UNMGEe-Sld_1EWpoOA" name="NO" theNodeOfTheOutgoingEdge="_ZVIUsNMFEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_ooWxsNMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_xaSW0NMFEe-Sld_1EWpoOA" mediniIdentifier="_xaSW0NMFEe-Sld_1EWpoOA" name="Call function &quot;Mcu_SetMode&quot; with apt configuration, void type so no need to check return" theIncomingEdge="_FCpdgNMGEe-Sld_1EWpoOA" theOutgoingEdge="_cQakoNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_cQakoNMGEe-Sld_1EWpoOA" mediniIdentifier="_cQakoNMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_xaSW0NMFEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_IJboQNMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_IJboQNMGEe-Sld_1EWpoOA" mediniIdentifier="_IJboQNMGEe-Sld_1EWpoOA" name="Call function &quot;Platform_Init&quot;, void type so no need to check return" theIncomingEdge="_cQakoNMGEe-Sld_1EWpoOA" theOutgoingEdge="_c1iq8NMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_c1iq8NMGEe-Sld_1EWpoOA" mediniIdentifier="_c1iq8NMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_IJboQNMGEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_O7o74NMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_O7o74NMGEe-Sld_1EWpoOA" mediniIdentifier="_O7o74NMGEe-Sld_1EWpoOA" name="Call function &quot;OsIf_Init&quot;, void type so no need to check return" theIncomingEdge="_c1iq8NMGEe-Sld_1EWpoOA" theOutgoingEdge="_d7MrcNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_d7MrcNMGEe-Sld_1EWpoOA" mediniIdentifier="_d7MrcNMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_O7o74NMGEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_UqYnYNMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_UqYnYNMGEe-Sld_1EWpoOA" mediniIdentifier="_UqYnYNMGEe-Sld_1EWpoOA" name="Call function &quot;IntCtrl_Ip_Init&quot; with apt configuration, void type so no need to check return" theIncomingEdge="_d7MrcNMGEe-Sld_1EWpoOA" theOutgoingEdge="_tHf2gNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_tHf2gNMGEe-Sld_1EWpoOA" mediniIdentifier="_tHf2gNMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_UqYnYNMGEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_qkJwANMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLFinalNode" xmi:id="_n0RpYNMGEe-Sld_1EWpoOA" mediniIdentifier="_n0RpYNMGEe-Sld_1EWpoOA" finalNodeKind="FINAL_FLOW_NODE"/>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_ooWxsNMGEe-Sld_1EWpoOA" mediniIdentifier="_ooWxsNMGEe-Sld_1EWpoOA" name="Return failure enum" theIncomingEdge="_vlF6UNMGEe-Sld_1EWpoOA" theOutgoingEdge="_ygR5ENMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_ygR5ENMGEe-Sld_1EWpoOA" mediniIdentifier="_ygR5ENMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_ooWxsNMGEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_xVfg8NMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLAction" xmi:id="_qkJwANMGEe-Sld_1EWpoOA" mediniIdentifier="_qkJwANMGEe-Sld_1EWpoOA" name="Return success enum" theIncomingEdge="_tHf2gNMGEe-Sld_1EWpoOA" theOutgoingEdge="_zbPFcNMGEe-Sld_1EWpoOA">
          <the_owned_elements xsi:type="sysml:SysMLActivityEdge" xmi:id="_zbPFcNMGEe-Sld_1EWpoOA" mediniIdentifier="_zbPFcNMGEe-Sld_1EWpoOA" theNodeOfTheOutgoingEdge="_qkJwANMGEe-Sld_1EWpoOA" theNodeOfTheIncomingEdge="_xVfg8NMGEe-Sld_1EWpoOA"/>
        </the_owned_elements>
        <the_owned_elements xsi:type="sysml:SysMLFinalNode" xmi:id="_xVfg8NMGEe-Sld_1EWpoOA" mediniIdentifier="_xVfg8NMGEe-Sld_1EWpoOA" theIncomingEdge="_ygR5ENMGEe-Sld_1EWpoOA _zbPFcNMGEe-Sld_1EWpoOA" finalNodeKind="FINAL_FLOW_NODE"/>
      </the_owned_elements>
      <dependencies xsi:type="sysml:SysMLDependency" xmi:id="_Z7zBMNMHEe-Sld_1EWpoOA" mediniIdentifier="_Z7zBMNMHEe-Sld_1EWpoOA" the_source_element="_QghlINL9Ee-Sld_1EWpoOA" the_target_element="_RXdooNMHEe-Sld_1EWpoOA"/>
    </the_owned_elements>
    <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_LKgXINMHEe-Sld_1EWpoOA" mediniIdentifier="_LKgXINMHEe-Sld_1EWpoOA" typeCode="Component" name="RTD Module" user_kind="internal" user_circuit_block=""/>
    <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_RXdooNMHEe-Sld_1EWpoOA" mediniIdentifier="_RXdooNMHEe-Sld_1EWpoOA" typeCode="Software Unit" name="NXP RTD Module" the_relationship_of_target="_Z7zBMNMHEe-Sld_1EWpoOA" user_kind="internal" user_circuit_block=""/>
  </the_owned_elements>
</sysml:SysMLContainerPackage>
