<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_8FCBAOUhEemDKMXKazwdEA" mediniIdentifier="_8FCBAOUhEemDKMXKazwdEA" name="P-11 Table 38 - Analogue/Mixed Signal: Analogue I/O">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Aql24OUiEemDKMXKazwdEA" mediniIdentifier="_Aql24OUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.1" name="Resistive pull up/down" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically used on input signals to avoid floating conditions due to pin failure or external pin interconnect failure."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_At8s4OUiEemDKMXKazwdEA" mediniIdentifier="_At8s4OUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.8" name="Filter" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Analogue or digital circuit, typically used to suppress high frequency signal variation, like an output from analogue over &amp; under voltage monitoring circuit."/>
</safety:MeasureCatalog>
