<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_UOiVEKKDEe-wZbFTjxBvsA" mediniIdentifier="_UOiVEKKDEe-wZbFTjxBvsA" name="VEC EV Trucks and Buses 22/11/24">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QwvwgKjOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwgKjOEe-HzbH5H-6a6w" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_QwvwgajOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwgajOEe-HzbH5H-6a6w" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant and Any traffic density" ISO26262_itemUsage="Service " user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QwvwgqjOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwgqjOEe-HzbH5H-6a6w" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Breakdowns are anticipated to occur occasionally, resulting in an E2 exposure as the likelihood of hazardous events is low but not negligible, with infrequent occurrence during operational scenarios." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Qwvwg6jOEe-HzbH5H-6a6w" mediniIdentifier="_Qwvwg6jOEe-HzbH5H-6a6w" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Breakdown" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QwvwhKjOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwhKjOEe-HzbH5H-6a6w" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_QwvwhajOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwhajOEe-HzbH5H-6a6w" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QwvwhqjOEe-HzbH5H-6a6w" mediniIdentifier="_QwvwhqjOEe-HzbH5H-6a6w" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Breakdowns are anticipated to occur occasionally, resulting in an E2 exposure as the likelihood of hazardous events is low but not negligible, with infrequent occurrence during operational scenarios." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Qwvwh6jOEe-HzbH5H-6a6w" mediniIdentifier="_Qwvwh6jOEe-HzbH5H-6a6w" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Breakdown" user_speed="Not Moving"/>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
