<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_kdchIOUgEemDKMXKazwdEA" mediniIdentifier="_kdchIOUgEemDKMXKazwdEA" name="P-11 Table 37 - Analogue/Mixed Signal: Power Supply">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_7o1psOUgEemDKMXKazwdEA" mediniIdentifier="_7o1psOUgEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.2" name="Over and under voltage monitoring" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit with an output latched in a digital core"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_7sk6MOUgEemDKMXKazwdEA" mediniIdentifier="_7sk6MOUgEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.3" name="Voltage clamp (limiter)" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically used to suppress voltage transients or spikes."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_7xAHMOUgEemDKMXKazwdEA" mediniIdentifier="_7xAHMOUgEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.4" name="Over-current monitoring" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit with an output latched in digital core."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_71zusOUgEemDKMXKazwdEA" mediniIdentifier="_71zusOUgEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.5" name="Current limiting" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit with feedback to an analogue control loop (e.g. to disable regulator main pass element)."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_D6QtUOUhEemDKMXKazwdEA" mediniIdentifier="_D6QtUOUhEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.6" name="Power on reset" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Functional block which keeps the circuit in a known initialized state until power supply rails and/or the clock signal are stable."/>
</safety:MeasureCatalog>
