<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_S4KakOUiEemDKMXKazwdEA" mediniIdentifier="_S4KakOUiEemDKMXKazwdEA" name="P-11 Table 39 - Analogue/Mixed Signal: Misc analogue components">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_dxtXAOUiEemDKMXKazwdEA" mediniIdentifier="_dxtXAOUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.7" name="Analogue watchdog" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically a monostable circuit used to monitor proper operation of an oscillator."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_d1iHEOUiEemDKMXKazwdEA" mediniIdentifier="_d1iHEOUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.9" name="Thermal monitor" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit with an output latched in digital core, or feedback to an analogue circuit control loop (e.g. to disable affected circuit)."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_d5uqkOUiEemDKMXKazwdEA" mediniIdentifier="_d5uqkOUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.11" name="ADC monitoring" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="An analogue circuit typically controlled and evaluated by a digital circuit."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_d9xdEOUiEemDKMXKazwdEA" mediniIdentifier="_d9xdEOUiEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.10" name="Analogue BIST" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit controlled by a digital circuit that verifies correct functionality of analogue safety mechanisms like under/over voltage monitoring, current limit protection and thermal protection circuits."/>
</safety:MeasureCatalog>
