<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_tdr4kE9BEeC1A4_enB0KXA" mediniIdentifier="_tdr4kE9BEeC1A4_enB0KXA" name="P-5 Table D.9 - Sensors">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wESHYk9BEeC1A4_enB0KXA" mediniIdentifier="_wESHYk9BEeC1A4_enB0KXA" id="ISO26262-5: D.2.1.1" name="Failure detection by on-line monitoring" maxDC="LOW" notes="Depends on diagnostic coverage of failure detection"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wESHY09BEeC1A4_enB0KXA" mediniIdentifier="_wESHY09BEeC1A4_enB0KXA" id="ISO26262-5: D.2.4.1" name="Test pattern" maxDC="HIGH" notes="-"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wEbRUE9BEeC1A4_enB0KXA" mediniIdentifier="_wEbRUE9BEeC1A4_enB0KXA" id="ISO26262-5: D.2.4.5" name="Input comparison/voting (1oo2, 2oo3 or better redundancy)" maxDC="HIGH" notes="Only if dataflow changes within diagnostic test interval"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wEbRUU9BEeC1A4_enB0KXA" mediniIdentifier="_wEbRUU9BEeC1A4_enB0KXA" id="ISO26262-5: D.2.8.1" name="Sensor Valid Range" maxDC="LOW" notes="Detects shorts to ground or power and some open circuits"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wEbRUk9BEeC1A4_enB0KXA" mediniIdentifier="_wEbRUk9BEeC1A4_enB0KXA" id="ISO26262-5: D.2.8.2" name="Sensor Correlation" maxDC="HIGH" notes="Detects in range failures"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_wEbRU09BEeC1A4_enB0KXA" mediniIdentifier="_wEbRU09BEeC1A4_enB0KXA" id="ISO26262-5: D.2.8.3" name="Sensor Rationality Check" maxDC="MEDIUM" notes="-"/>
</safety:MeasureCatalog>
