<?xml version="1.1" encoding="UTF-8"?>
<sysml:SysMLContainerPackage xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:failureratecatalogs="http://www.ikv.de/medini/failureratecatalogs/1.0" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmlns:sysml="http://www.ikv.de/medini/sysml/1.0" xmi:id="_6CABgJ0OEfC3WfcdpN7glw" mediniIdentifier="_6CABgJ0OEfC3WfcdpN7glw" name="HW Architecture">
  <eAnnotations xmi:id="_N2dqgJ0PEfC3WfcdpN7glw" source="baseline_file">
    <references href="../.project.medini#_N2b1UJ0PEfC3WfcdpN7glw"/>
  </eAnnotations>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEkJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEkJ0PEfC3WfcdpN7glw" name="BR-1225A_COIN CELL" description="BT1" partNumber="BR-1225A/FAN" user_kind="internal" user_circuit_block="Master controller"/>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEkZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEkZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvpQ0J0PEfC3WfcdpN7glw" mediniIdentifier="_NvpQ0J0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvp34J0PEfC3WfcdpN7glw" mediniIdentifier="_Nvp34J0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvqe8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nvqe8J0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvqe8Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw7DNp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DNp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DN50PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DN50PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DOJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DOJ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DOZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DOZ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw7DO50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw7DMJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DMZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DMZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DMp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DMp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DM50PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DM50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw7DNZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw6cJZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cJp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cJp0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cJ50PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cJ50PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cKJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cKJ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw6cKp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw51Fp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw51Fp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cIJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cIJ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cIZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cIZ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw6cIp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw6cIp0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw6cJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw51EJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw51EJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw51EZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw51EZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw51Ep0PEfC3WfcdpN7glw" mediniIdentifier="_Nw51Ep0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw51E50PEfC3WfcdpN7glw" mediniIdentifier="_Nw51E50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw51FZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw5OAJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw5OAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw5OAZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw5OAZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw5OAp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw5OAp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw5OA50PEfC3WfcdpN7glw" mediniIdentifier="_Nw5OA50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw5OBZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw4m8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nw4m8J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw4m8Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nw4m8Z0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw4m8p0PEfC3WfcdpN7glw" mediniIdentifier="_Nw4m8p0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw4m850PEfC3WfcdpN7glw" mediniIdentifier="_Nw4m850PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw4m9Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw3_5p0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_5p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_550PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_550PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_6J0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_6J0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_6Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_6Z0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw3_650PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw3_4J0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_4Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_4Z0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_4p0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_4p0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3_450PEfC3WfcdpN7glw" mediniIdentifier="_Nw3_450PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw3_5Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw3Y0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3Y0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3Y0Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3Y0Z0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3Y0p0PEfC3WfcdpN7glw" mediniIdentifier="_Nw3Y0p0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw3Y050PEfC3WfcdpN7glw" mediniIdentifier="_Nw3Y050PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw3Y1Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw2xwJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2xwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2xwZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2xwZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2xwp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2xwp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2xw50PEfC3WfcdpN7glw" mediniIdentifier="_Nw2xw50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw2xxZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw2KsJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2KsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2KsZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2KsZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2Ksp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw2Ksp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw2Ks50PEfC3WfcdpN7glw" mediniIdentifier="_Nw2Ks50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw2KtZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw1joJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw1joJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw1joZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw1joZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw1jop0PEfC3WfcdpN7glw" mediniIdentifier="_Nw1jop0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw1jo50PEfC3WfcdpN7glw" mediniIdentifier="_Nw1jo50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw1jpZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw08lp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08lp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08l50PEfC3WfcdpN7glw" mediniIdentifier="_Nw08l50PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08mJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08mJ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08mZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08mZ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw08m50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw08kJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08kJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08kZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08kZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08kp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw08kp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw08k50PEfC3WfcdpN7glw" mediniIdentifier="_Nw08k50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw08lZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw0VgJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw0VgJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw0VgZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw0VgZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw0Vgp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw0Vgp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw0Vg50PEfC3WfcdpN7glw" mediniIdentifier="_Nw0Vg50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw0VhZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwzucJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwzucJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwzucZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwzucZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwzucp0PEfC3WfcdpN7glw" mediniIdentifier="_Nwzucp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwzuc50PEfC3WfcdpN7glw" mediniIdentifier="_Nwzuc50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwzudZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwzHYp0PEfC3WfcdpN7glw" mediniIdentifier="_NwzHYp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwzHY50PEfC3WfcdpN7glw" mediniIdentifier="_NwzHY50PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwzHZJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwzHZJ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwzHZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwzHZZ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwzHZ50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwygVp0PEfC3WfcdpN7glw" mediniIdentifier="_NwygVp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygV50PEfC3WfcdpN7glw" mediniIdentifier="_NwygV50PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygWJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwygWJ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygWZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwygWZ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwzHYZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwygUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwygUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwygUZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygUp0PEfC3WfcdpN7glw" mediniIdentifier="_NwygUp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwygU50PEfC3WfcdpN7glw" mediniIdentifier="_NwygU50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwygVZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwx5Rp0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5Rp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5R50PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5R50PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5SJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5SJ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5SZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5SZ0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwx5S50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwx5QJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5QJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5QZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5QZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5Qp0PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5Qp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwx5Q50PEfC3WfcdpN7glw" mediniIdentifier="_Nwx5Q50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwx5RZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwxSMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwxSMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwxSMZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwxSMZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwxSMp0PEfC3WfcdpN7glw" mediniIdentifier="_NwxSMp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwxSM50PEfC3WfcdpN7glw" mediniIdentifier="_NwxSM50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwxSNZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwwrIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwwrIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwrIZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwwrIZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwrIp0PEfC3WfcdpN7glw" mediniIdentifier="_NwwrIp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwrI50PEfC3WfcdpN7glw" mediniIdentifier="_NwwrI50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwwrJZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwwEEJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwwEEJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwEEZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwwEEZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwEEp0PEfC3WfcdpN7glw" mediniIdentifier="_NwwEEp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwwEE50PEfC3WfcdpN7glw" mediniIdentifier="_NwwEE50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwwEFZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwu18J0PEfC3WfcdpN7glw" mediniIdentifier="_Nwu18J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwu18Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nwu18Z0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwu18p0PEfC3WfcdpN7glw" mediniIdentifier="_Nwu18p0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwu1850PEfC3WfcdpN7glw" mediniIdentifier="_Nwu1850PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwu19Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwtn1p0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn1p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn150PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn150PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn2J0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn2J0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn2Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn2Z0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwtn250PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwtn0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn0Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn0Z0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn0p0PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn0p0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwtn050PEfC3WfcdpN7glw" mediniIdentifier="_Nwtn050PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwtn1Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwtAwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwtAwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwtAwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwtAwZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwtAwp0PEfC3WfcdpN7glw" mediniIdentifier="_NwtAwp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwtAw50PEfC3WfcdpN7glw" mediniIdentifier="_NwtAw50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwtAxZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwsZsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwsZsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwsZsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwsZsZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwsZsp0PEfC3WfcdpN7glw" mediniIdentifier="_NwsZsp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwsZs50PEfC3WfcdpN7glw" mediniIdentifier="_NwsZs50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwsZtZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwryoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwryoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwryoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwryoZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwryop0PEfC3WfcdpN7glw" mediniIdentifier="_Nwryop0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwryo50PEfC3WfcdpN7glw" mediniIdentifier="_Nwryo50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwrypZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwrLkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwrLkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwrLkZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwrLkZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwrLkp0PEfC3WfcdpN7glw" mediniIdentifier="_NwrLkp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwrLk50PEfC3WfcdpN7glw" mediniIdentifier="_NwrLk50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwrLlZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nwp9cJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwp9cJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwp9cZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nwp9cZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwp9cp0PEfC3WfcdpN7glw" mediniIdentifier="_Nwp9cp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nwp9c50PEfC3WfcdpN7glw" mediniIdentifier="_Nwp9c50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nwp9dZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwpWYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwpWYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwpWYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwpWYZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwpWYp0PEfC3WfcdpN7glw" mediniIdentifier="_NwpWYp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwpWY50PEfC3WfcdpN7glw" mediniIdentifier="_NwpWY50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwpWZZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwovUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwovUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwovUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwovUZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwovUp0PEfC3WfcdpN7glw" mediniIdentifier="_NwovUp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwovU50PEfC3WfcdpN7glw" mediniIdentifier="_NwovU50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwovVZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwoIQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwoIQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwoIQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwoIQZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwoIQp0PEfC3WfcdpN7glw" mediniIdentifier="_NwoIQp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwoIQ50PEfC3WfcdpN7glw" mediniIdentifier="_NwoIQ50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwoIRZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwnhMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwnhMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwnhMZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwnhMZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwnhMp0PEfC3WfcdpN7glw" mediniIdentifier="_NwnhMp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwnhM50PEfC3WfcdpN7glw" mediniIdentifier="_NwnhM50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwnhNZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwlsAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwlsAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwlsAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwlsAZ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwlsAp0PEfC3WfcdpN7glw" mediniIdentifier="_NwlsAp0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwlsA50PEfC3WfcdpN7glw" mediniIdentifier="_NwlsA50PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwmTEZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NwT_MJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwT_MJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047uF_100V_0603" alias="C_0.047uF_100V_0603" description="C1-C33,C35-C41" failureRateMode="FROM_CATALOG" partNumber="GCG188R92A473KA01D" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwVNUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwVNUJ0PEfC3WfcdpN7glw" id="FM004" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owo5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwVNUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwVNUZ0PEfC3WfcdpN7glw" id="FM005" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwVNUp0PEfC3WfcdpN7glw" mediniIdentifier="_NwVNUp0PEfC3WfcdpN7glw" id="FM006" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwpZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwV0YZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owopq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEkp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEkp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_1200PF_50V_0603" alias="C_1200PF_50V_0603" description="C34,C142,C168,C174,C175" failureRateMode="FROM_CATALOG" partNumber="GCM1885C1H122JA16J" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvrtEZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvrtEZ0PEfC3WfcdpN7glw" id="FM007" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owp5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvrtEp0PEfC3WfcdpN7glw" mediniIdentifier="_NvrtEp0PEfC3WfcdpN7glw" id="FM008" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvsUIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvsUIJ0PEfC3WfcdpN7glw" id="FM009" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvs7MJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owppq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw8RVp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RVp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_1200PF_50V_0603" alias="C_1200PF_50V_0603" description="C34,C142,C168,C174,C175" failureRateMode="FROM_CATALOG" partNumber="GCM1885C1H122JA16J" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RV50PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RV50PEfC3WfcdpN7glw" id="FM007" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owp5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RWJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RWJ0PEfC3WfcdpN7glw" id="FM008" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RWZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RWZ0PEfC3WfcdpN7glw" id="FM009" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw84YZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owppq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw8RUJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_1200PF_50V_0603" alias="C_1200PF_50V_0603" description="C34,C142,C168,C174,C175" failureRateMode="FROM_CATALOG" partNumber="GCM1885C1H122JA16J" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RUZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RUZ0PEfC3WfcdpN7glw" id="FM007" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owp5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RUp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RUp0PEfC3WfcdpN7glw" id="FM008" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw8RU50PEfC3WfcdpN7glw" mediniIdentifier="_Nw8RU50PEfC3WfcdpN7glw" id="FM009" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw8RVZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owppq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw7qQJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7qQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_1200PF_50V_0603" alias="C_1200PF_50V_0603" description="C34,C142,C168,C174,C175" failureRateMode="FROM_CATALOG" partNumber="GCM1885C1H122JA16J" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7qQZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7qQZ0PEfC3WfcdpN7glw" id="FM007" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owp5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7qQp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7qQp0PEfC3WfcdpN7glw" id="FM008" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7qQ50PEfC3WfcdpN7glw" mediniIdentifier="_Nw7qQ50PEfC3WfcdpN7glw" id="FM009" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw7qRZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owppq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw7DPJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DPJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_1200PF_50V_0603" alias="C_1200PF_50V_0603" description="C34,C142,C168,C174,C175" failureRateMode="FROM_CATALOG" partNumber="GCM1885C1H122JA16J" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DPZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DPZ0PEfC3WfcdpN7glw" id="FM007" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owp5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DPp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DPp0PEfC3WfcdpN7glw" id="FM008" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw7DP50PEfC3WfcdpN7glw" mediniIdentifier="_Nw7DP50PEfC3WfcdpN7glw" id="FM009" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwqZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw7DQZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owppq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEk50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEk50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu_wkJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu_wkJ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvAXoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvAXoJ0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvA-sJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxDmEJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxDmEJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxDmEZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxDmEZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxDmEp0PEfC3WfcdpN7glw" mediniIdentifier="_NxDmEp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxDmFJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxCX8p0PEfC3WfcdpN7glw" mediniIdentifier="_NxCX8p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxCX850PEfC3WfcdpN7glw" mediniIdentifier="_NxCX850PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxCX9J0PEfC3WfcdpN7glw" mediniIdentifier="_NxCX9J0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxCX9p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxBw4J0PEfC3WfcdpN7glw" mediniIdentifier="_NxBw4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxBw4Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxBw4Z0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxBw4p0PEfC3WfcdpN7glw" mediniIdentifier="_NxBw4p0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxCX8Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxBJ0J0PEfC3WfcdpN7glw" mediniIdentifier="_NxBJ0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxBJ0Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxBJ0Z0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxBJ0p0PEfC3WfcdpN7glw" mediniIdentifier="_NxBJ0p0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxBJ1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxAixZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxAixZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxAixp0PEfC3WfcdpN7glw" mediniIdentifier="_NxAixp0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxAix50PEfC3WfcdpN7glw" mediniIdentifier="_NxAix50PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxAiyZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxAiwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxAiwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxAiwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxAiwZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxAiwp0PEfC3WfcdpN7glw" mediniIdentifier="_NxAiwp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxAixJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw_7sJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_7sJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_7sZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_7sZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_7sp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_7sp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw_7tJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw_UpZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_UpZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_Upp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_Upp0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_Up50PEfC3WfcdpN7glw" mediniIdentifier="_Nw_Up50PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw_UqZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw_UoJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_UoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_UoZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_UoZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw_Uop0PEfC3WfcdpN7glw" mediniIdentifier="_Nw_Uop0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw_UpJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw-tlZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tlZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-tlp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tlp0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-tl50PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tl50PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw-tmZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw-tkJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-tkZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tkZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-tkp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-tkp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw-tlJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw-GgJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-GgJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-GgZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-GgZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw-Ggp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw-Ggp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw-GhJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw9fdZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fdZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw9fdp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fdp0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw9fd50PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fd50PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw9feZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw9fcJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fcJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw9fcZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fcZ0PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw9fcp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw9fcp0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw9fdJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nw84Yp0PEfC3WfcdpN7glw" mediniIdentifier="_Nw84Yp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.047UF_50V_0603" alias="C_0.047UF_50V_0603" description="C42-C57" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H473K080AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw84Y50PEfC3WfcdpN7glw" mediniIdentifier="_Nw84Y50PEfC3WfcdpN7glw" id="FM010" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owq5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nw84ZJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nw84ZJ0PEfC3WfcdpN7glw" id="FM011" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nw84Zp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owqpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUElJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUElJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv2sMJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv2sMJ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv3TQJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv3TQJ0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv3TQZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxKTxZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxKTxZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxKTxp0PEfC3WfcdpN7glw" mediniIdentifier="_NxKTxp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxKTx50PEfC3WfcdpN7glw" mediniIdentifier="_NxKTx50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxKTyZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxKTwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxKTwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxKTwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxKTwZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxKTwp0PEfC3WfcdpN7glw" mediniIdentifier="_NxKTwp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxKTxJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxJstZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxJstZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJstp0PEfC3WfcdpN7glw" mediniIdentifier="_NxJstp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJst50PEfC3WfcdpN7glw" mediniIdentifier="_NxJst50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxJsuZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxJssJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxJssJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJssZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxJssZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJssp0PEfC3WfcdpN7glw" mediniIdentifier="_NxJssp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxJstJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxJFoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxJFoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJFoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxJFoZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxJFop0PEfC3WfcdpN7glw" mediniIdentifier="_NxJFop0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxJFpJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxIekJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxIekJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxIekZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxIekZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxIekp0PEfC3WfcdpN7glw" mediniIdentifier="_NxIekp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxIelJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxH3hZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxH3hZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxH3hp0PEfC3WfcdpN7glw" mediniIdentifier="_NxH3hp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxH3h50PEfC3WfcdpN7glw" mediniIdentifier="_NxH3h50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxH3iZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxH3gJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxH3gJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxH3gZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxH3gZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxH3gp0PEfC3WfcdpN7glw" mediniIdentifier="_NxH3gp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxH3hJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxHQep0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQep0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQe50PEfC3WfcdpN7glw" mediniIdentifier="_NxHQe50PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQfJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQfJ0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxHQfp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxHQdZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQdZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQdp0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQdp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQd50PEfC3WfcdpN7glw" mediniIdentifier="_NxHQd50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxHQeZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxHQcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQcJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQcZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxHQcp0PEfC3WfcdpN7glw" mediniIdentifier="_NxHQcp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxHQdJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxGpZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGpZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGpZp0PEfC3WfcdpN7glw" mediniIdentifier="_NxGpZp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGpZ50PEfC3WfcdpN7glw" mediniIdentifier="_NxGpZ50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxGpaZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxGpYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGpYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGpYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGpYZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGpYp0PEfC3WfcdpN7glw" mediniIdentifier="_NxGpYp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxGpZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxGCVZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGCVZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGCVp0PEfC3WfcdpN7glw" mediniIdentifier="_NxGCVp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGCV50PEfC3WfcdpN7glw" mediniIdentifier="_NxGCV50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxGCWZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxGCUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGCUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGCUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxGCUZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxGCUp0PEfC3WfcdpN7glw" mediniIdentifier="_NxGCUp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxGCVJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxFbRZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxFbRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxFbRp0PEfC3WfcdpN7glw" mediniIdentifier="_NxFbRp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxFbR50PEfC3WfcdpN7glw" mediniIdentifier="_NxFbR50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxFbSZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxFbQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxFbQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxFbQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxFbQZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxFbQp0PEfC3WfcdpN7glw" mediniIdentifier="_NxFbQp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxFbRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxE0Mp0PEfC3WfcdpN7glw" mediniIdentifier="_NxE0Mp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxE0M50PEfC3WfcdpN7glw" mediniIdentifier="_NxE0M50PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxE0NJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxE0NJ0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxE0Np0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxENJZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxENJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxENJp0PEfC3WfcdpN7glw" mediniIdentifier="_NxENJp0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxENJ50PEfC3WfcdpN7glw" mediniIdentifier="_NxENJ50PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxE0MZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxENIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxENIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1uF_50V_0603" alias="C_0.1uF_50V_0603" description="C59,C60,C64-C66,C80,C81,C85,C86,C93,C130,C132,C137,C139,C141,C157,C160,C162,C165,C169,C170" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R1H104K080AA" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxENIZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxENIZ0PEfC3WfcdpN7glw" id="FM012" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owrpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxENIp0PEfC3WfcdpN7glw" mediniIdentifier="_NxENIp0PEfC3WfcdpN7glw" id="FM013" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owr5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxENJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwrZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUElZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUElZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.22uF_50V_0603" alias="C_0.22uF_50V_0603" description="C61,C75,C150" failureRateMode="FROM_CATALOG" partNumber="GCM188R71H224KA64D" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvTSkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvTSkJ0PEfC3WfcdpN7glw" id="FM014" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvT5oJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvT5oJ0PEfC3WfcdpN7glw" id="FM015" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owspq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvUgsJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxK61Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxK61Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.22uF_50V_0603" alias="C_0.22uF_50V_0603" description="C61,C75,C150" failureRateMode="FROM_CATALOG" partNumber="GCM188R71H224KA64D" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxK61p0PEfC3WfcdpN7glw" mediniIdentifier="_NxK61p0PEfC3WfcdpN7glw" id="FM014" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxK6150PEfC3WfcdpN7glw" mediniIdentifier="_NxK6150PEfC3WfcdpN7glw" id="FM015" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owspq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxK62Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxK60J0PEfC3WfcdpN7glw" mediniIdentifier="_NxK60J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.22uF_50V_0603" alias="C_0.22uF_50V_0603" description="C61,C75,C150" failureRateMode="FROM_CATALOG" partNumber="GCM188R71H224KA64D" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxK60Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxK60Z0PEfC3WfcdpN7glw" id="FM014" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxK60p0PEfC3WfcdpN7glw" mediniIdentifier="_NxK60p0PEfC3WfcdpN7glw" id="FM015" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owspq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxK61J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwsJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUElp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUElp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvPoMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvPoMJ0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvQPQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvQPQJ0PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvQ2UJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxMwAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxMwAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMwAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxMwAZ0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMwAp0PEfC3WfcdpN7glw" mediniIdentifier="_NxMwAp0PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxMwBJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxMI9Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxMI9Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMI9p0PEfC3WfcdpN7glw" mediniIdentifier="_NxMI9p0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMI950PEfC3WfcdpN7glw" mediniIdentifier="_NxMI950PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxMI-Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxMI8J0PEfC3WfcdpN7glw" mediniIdentifier="_NxMI8J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMI8Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxMI8Z0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMI8p0PEfC3WfcdpN7glw" mediniIdentifier="_NxMI8p0PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxMI9J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxLh5Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxLh5Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxLh5p0PEfC3WfcdpN7glw" mediniIdentifier="_NxLh5p0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxLh550PEfC3WfcdpN7glw" mediniIdentifier="_NxLh550PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxLh6Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxLh4J0PEfC3WfcdpN7glw" mediniIdentifier="_NxLh4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_25V_0402" alias="C_0.1UF_25V_0402" description="C62,C68-C70,C78,C79" failureRateMode="FROM_CATALOG" partNumber="CGA2B3X7R1E104K050BB" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxLh4Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxLh4Z0PEfC3WfcdpN7glw" id="FM016" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxLh4p0PEfC3WfcdpN7glw" mediniIdentifier="_NxLh4p0PEfC3WfcdpN7glw" id="FM017" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwtZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxLh5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ows5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEl50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEl50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_10uF_16V_0805" alias="C_10uF_16V_0805" description="C73,C74" failureRateMode="FROM_CATALOG" partNumber="CGA4J1X7S1C106M125AC" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvs7MZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nvs7MZ0PEfC3WfcdpN7glw" id="FM018" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owt5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvtiQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvtiQJ0PEfC3WfcdpN7glw" id="FM019" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwuJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvtiQZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owtpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxMwBZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxMwBZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_10uF_16V_0805" alias="C_10uF_16V_0805" description="C73,C74" failureRateMode="FROM_CATALOG" partNumber="CGA4J1X7S1C106M125AC" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMwBp0PEfC3WfcdpN7glw" mediniIdentifier="_NxMwBp0PEfC3WfcdpN7glw" id="FM018" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owt5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxMwB50PEfC3WfcdpN7glw" mediniIdentifier="_NxMwB50PEfC3WfcdpN7glw" id="FM019" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwuJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxNXEZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owtpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEmJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEmJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_12pF_50V_0402" alias="C_12pF_50V_0402" description="C76,C77" failureRateMode="FROM_CATALOG" partNumber="GCM1555C1H120JA16D" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvmNgZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvmNgZ0PEfC3WfcdpN7glw" id="FM020" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owupq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvnboJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvnboJ0PEfC3WfcdpN7glw" id="FM021" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owu5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvoCsJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwuZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxNXEp0PEfC3WfcdpN7glw" mediniIdentifier="_NxNXEp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_12pF_50V_0402" alias="C_12pF_50V_0402" description="C76,C77" failureRateMode="FROM_CATALOG" partNumber="GCM1555C1H120JA16D" user_kind="internal" user_circuit_block="Master Controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxNXE50PEfC3WfcdpN7glw" mediniIdentifier="_NxNXE50PEfC3WfcdpN7glw" id="FM020" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owupq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxNXFJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxNXFJ0PEfC3WfcdpN7glw" id="FM021" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owu5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxNXFp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwuZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEmZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEmZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_22UF_25V_1210" alias="C_22UF_25V_1210" description="C88,C105,C113,C119,C120" failureRateMode="FROM_CATALOG" partNumber="CGA6P3X7R1E226M250AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvlmcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvlmcJ0PEfC3WfcdpN7glw" id="FM022" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvlmcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvlmcZ0PEfC3WfcdpN7glw" id="FM023" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owvpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvmNgJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxPMQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPMQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_22UF_25V_1210" alias="C_22UF_25V_1210" description="C88,C105,C113,C119,C120" failureRateMode="FROM_CATALOG" partNumber="CGA6P3X7R1E226M250AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPMQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPMQZ0PEfC3WfcdpN7glw" id="FM022" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPMQp0PEfC3WfcdpN7glw" mediniIdentifier="_NxPMQp0PEfC3WfcdpN7glw" id="FM023" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owvpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxPMRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxOlMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxOlMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_22UF_25V_1210" alias="C_22UF_25V_1210" description="C88,C105,C113,C119,C120" failureRateMode="FROM_CATALOG" partNumber="CGA6P3X7R1E226M250AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxOlMZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxOlMZ0PEfC3WfcdpN7glw" id="FM022" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxOlMp0PEfC3WfcdpN7glw" mediniIdentifier="_NxOlMp0PEfC3WfcdpN7glw" id="FM023" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owvpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxOlNJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxN-IJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxN-IJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_22UF_25V_1210" alias="C_22UF_25V_1210" description="C88,C105,C113,C119,C120" failureRateMode="FROM_CATALOG" partNumber="CGA6P3X7R1E226M250AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxN-IZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxN-IZ0PEfC3WfcdpN7glw" id="FM022" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxN-Ip0PEfC3WfcdpN7glw" mediniIdentifier="_NxN-Ip0PEfC3WfcdpN7glw" id="FM023" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owvpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxN-JJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxNXF50PEfC3WfcdpN7glw" mediniIdentifier="_NxNXF50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_22UF_25V_1210" alias="C_22UF_25V_1210" description="C88,C105,C113,C119,C120" failureRateMode="FROM_CATALOG" partNumber="CGA6P3X7R1E226M250AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxNXGJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxNXGJ0PEfC3WfcdpN7glw" id="FM022" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxNXGZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxNXGZ0PEfC3WfcdpN7glw" id="FM023" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owvpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxNXG50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwvJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEmp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEmp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NupyUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NupyUJ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuqZYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuqZYJ0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NurngJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxRohZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxRohZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRohp0PEfC3WfcdpN7glw" mediniIdentifier="_NxRohp0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRoh50PEfC3WfcdpN7glw" mediniIdentifier="_NxRoh50PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxRoiZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxRogJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxRogJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRogZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxRogZ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRogp0PEfC3WfcdpN7glw" mediniIdentifier="_NxRogp0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxRohJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxRBcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxRBcJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRBcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxRBcZ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxRBcp0PEfC3WfcdpN7glw" mediniIdentifier="_NxRBcp0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxRBdJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxQaaZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaaZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaap0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaap0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaa50PEfC3WfcdpN7glw" mediniIdentifier="_NxQaa50PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxQabZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxQaZJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaZJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaZZ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaZp0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaZp0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxQaaJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxPzVZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPzVZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaYJ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxQaYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxQaYZ0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxQaY50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxPzUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPzUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPzUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPzUZ0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPzUp0PEfC3WfcdpN7glw" mediniIdentifier="_NxPzUp0PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxPzVJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxPMRZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxPMRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_56pF_100V_0603" alias="C_56pF_100V_0603" description="C107,C108,C110-C112,C131,C133,C134,C136" failureRateMode="FROM_CATALOG" partNumber="GCM1885C2A560JA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPMRp0PEfC3WfcdpN7glw" mediniIdentifier="_NxPMRp0PEfC3WfcdpN7glw" id="FM024" name="Short Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxPMR50PEfC3WfcdpN7glw" mediniIdentifier="_NxPMR50PEfC3WfcdpN7glw" id="FM025" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwwZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxPMSZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owv5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEm50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEm50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_4700pF_50V_0603" alias="C_4700pF_50V_0603" description="C109,C135" failureRateMode="FROM_CATALOG" partNumber="C0603C472J5GACAUTO" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvrGAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvrGAJ0PEfC3WfcdpN7glw" id="FM026" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Oww5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvrGAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvrGAZ0PEfC3WfcdpN7glw" id="FM027" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwxJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvrtEJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owwpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxSPkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_4700pF_50V_0603" alias="C_4700pF_50V_0603" description="C109,C135" failureRateMode="FROM_CATALOG" partNumber="C0603C472J5GACAUTO" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPkZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPkZ0PEfC3WfcdpN7glw" id="FM026" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Oww5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPkp0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPkp0PEfC3WfcdpN7glw" id="FM027" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwxJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxSPlJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owwpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEnJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEnJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_2.2UF_100V_0805" alias="C_2.2UF_100V_0805" description="C115,C116,C149" failureRateMode="FROM_CATALOG" partNumber="CGA4J1X7R2A225K125AC" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvwlkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvwlkJ0PEfC3WfcdpN7glw" id="FM028" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owxpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvxMoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvxMoJ0PEfC3WfcdpN7glw" id="FM029" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owx5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvxzsJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwxZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxSPmp0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPmp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_2.2UF_100V_0805" alias="C_2.2UF_100V_0805" description="C115,C116,C149" failureRateMode="FROM_CATALOG" partNumber="CGA4J1X7R2A225K125AC" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPm50PEfC3WfcdpN7glw" mediniIdentifier="_NxSPm50PEfC3WfcdpN7glw" id="FM028" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owxpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPnJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPnJ0PEfC3WfcdpN7glw" id="FM029" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owx5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxS2oZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwxZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxSPlZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPlZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_2.2UF_100V_0805" alias="C_2.2UF_100V_0805" description="C115,C116,C149" failureRateMode="FROM_CATALOG" partNumber="CGA4J1X7R2A225K125AC" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPlp0PEfC3WfcdpN7glw" mediniIdentifier="_NxSPlp0PEfC3WfcdpN7glw" id="FM028" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owxpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxSPl50PEfC3WfcdpN7glw" mediniIdentifier="_NxSPl50PEfC3WfcdpN7glw" id="FM029" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owx5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxSPmZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwxZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEnZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEnZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_2200PF_50V_0603" alias="C_2200PF_50V_0603" description="C117" failureRateMode="FROM_CATALOG" partNumber="C0603C222K5RACTU" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvW88J0PEfC3WfcdpN7glw" mediniIdentifier="_NvW88J0PEfC3WfcdpN7glw" id="FM030" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwyZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvXkAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvXkAJ0PEfC3WfcdpN7glw" id="FM031" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owypq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvXkAZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwyJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEnp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEnp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_3300PF_100V_0603" alias="C_3300PF_100V_0603" description="C118" failureRateMode="FROM_CATALOG" partNumber="CGA3E2X7R2A332K080AA" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NusOkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NusOkJ0PEfC3WfcdpN7glw" id="FM032" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwzJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NusOkZ0PEfC3WfcdpN7glw" mediniIdentifier="_NusOkZ0PEfC3WfcdpN7glw" id="FM033" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OwzZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nus1oJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owy5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEn50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEn50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_100V_0603" alias="C_0.1UF_100V_0603" description="C121,C122,C126" failureRateMode="FROM_CATALOG" partNumber="CGA3E3X7S2A104K080AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvYyIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvYyIJ0PEfC3WfcdpN7glw" id="FM034" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owz5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvYyIZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvYyIZ0PEfC3WfcdpN7glw" id="FM035" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow0Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvZZMJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owzpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxTdsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxTdsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_100V_0603" alias="C_0.1UF_100V_0603" description="C121,C122,C126" failureRateMode="FROM_CATALOG" partNumber="CGA3E3X7S2A104K080AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxTdsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxTdsZ0PEfC3WfcdpN7glw" id="FM034" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owz5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxTdsp0PEfC3WfcdpN7glw" mediniIdentifier="_NxTdsp0PEfC3WfcdpN7glw" id="FM035" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow0Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxTdtJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owzpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxS2op0PEfC3WfcdpN7glw" mediniIdentifier="_NxS2op0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_0.1UF_100V_0603" alias="C_0.1UF_100V_0603" description="C121,C122,C126" failureRateMode="FROM_CATALOG" partNumber="CGA3E3X7S2A104K080AB" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxS2o50PEfC3WfcdpN7glw" mediniIdentifier="_NxS2o50PEfC3WfcdpN7glw" id="FM034" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owz5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxS2pJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxS2pJ0PEfC3WfcdpN7glw" id="FM035" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow0Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxS2pp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Owzpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEoJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_390PF_100V_0603" alias="C_390PF_100V_0603" description="C127" failureRateMode="FROM_CATALOG" partNumber="GRT1885C2A391JA02J" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NuT0EJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuT0EJ0PEfC3WfcdpN7glw" id="FM036" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow0pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuYFgJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuYFgJ0PEfC3WfcdpN7glw" id="FM037" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow05q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NuYskJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow0Zq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEoZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEoZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_6pF_50V_0402" alias="C_6pF_50V_0402" description="C172,C173" failureRateMode="FROM_CATALOG" partNumber="GCM1555C1H6R0FA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvdqoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvdqoJ0PEfC3WfcdpN7glw" id="FM038" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvdqoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvdqoZ0PEfC3WfcdpN7glw" id="FM039" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NveRsJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxTdtZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxTdtZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="C_6pF_50V_0402" alias="C_6pF_50V_0402" description="C172,C173" failureRateMode="FROM_CATALOG" partNumber="GCM1555C1H6R0FA16D" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxTdtp0PEfC3WfcdpN7glw" mediniIdentifier="_NxTdtp0PEfC3WfcdpN7glw" id="FM038" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxTdt50PEfC3WfcdpN7glw" mediniIdentifier="_NxTdt50PEfC3WfcdpN7glw" id="FM039" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxTduZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow1Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEop0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEop0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TVS_TPSMF4L78A" alias="DIODE_TVS_TPSMF4L78A" description="D1" failureRateMode="FROM_CATALOG" partNumber="TPSMF4L78A" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NuezMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuezMJ0PEfC3WfcdpN7glw" id="FM040" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow2Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NugBUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NugBUJ0PEfC3WfcdpN7glw" id="FM041" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow2pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NuhPcJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow2Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEo50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEo50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TPSMB12CA_SMB" alias="DIODE_TPSMB12CA_SMB" description="D9,D11,D13,D14" failureRateMode="FROM_CATALOG" partNumber="TPSMB12CA" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv-A8p0PEfC3WfcdpN7glw" mediniIdentifier="_Nv-A8p0PEfC3WfcdpN7glw" id="FM042" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv-oAJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv-oAJ0PEfC3WfcdpN7glw" id="FM043" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv-oAZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow25q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxUEyp0PEfC3WfcdpN7glw" mediniIdentifier="_NxUEyp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TPSMB12CA_SMB" alias="DIODE_TPSMB12CA_SMB" description="D9,D11,D13,D14" failureRateMode="FROM_CATALOG" partNumber="TPSMB12CA" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUEy50PEfC3WfcdpN7glw" mediniIdentifier="_NxUEy50PEfC3WfcdpN7glw" id="FM042" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUEzJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxUEzJ0PEfC3WfcdpN7glw" id="FM043" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxUEzp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow25q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxUExZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxUExZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TPSMB12CA_SMB" alias="DIODE_TPSMB12CA_SMB" description="D9,D11,D13,D14" failureRateMode="FROM_CATALOG" partNumber="TPSMB12CA" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUExp0PEfC3WfcdpN7glw" mediniIdentifier="_NxUExp0PEfC3WfcdpN7glw" id="FM042" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUEx50PEfC3WfcdpN7glw" mediniIdentifier="_NxUEx50PEfC3WfcdpN7glw" id="FM043" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxUEyZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow25q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxUEwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxUEwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TPSMB12CA_SMB" alias="DIODE_TPSMB12CA_SMB" description="D9,D11,D13,D14" failureRateMode="FROM_CATALOG" partNumber="TPSMB12CA" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUEwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxUEwZ0PEfC3WfcdpN7glw" id="FM042" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUEwp0PEfC3WfcdpN7glw" mediniIdentifier="_NxUEwp0PEfC3WfcdpN7glw" id="FM043" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxUExJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow25q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEpJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEpJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" alias="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" description="D10,D36,D44" failureRateMode="FROM_CATALOG" partNumber="BAT46WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NujrsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NujrsJ0PEfC3WfcdpN7glw" id="FM044" name="Short circuit (reverse degradation)" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow35q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NujrsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NujrsZ0PEfC3WfcdpN7glw" id="FM045" name="Open circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow4Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nuk50J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3pq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxUr1Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxUr1Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" alias="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" description="D10,D36,D44" failureRateMode="FROM_CATALOG" partNumber="BAT46WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUr1p0PEfC3WfcdpN7glw" mediniIdentifier="_NxUr1p0PEfC3WfcdpN7glw" id="FM044" name="Short circuit (reverse degradation)" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow35q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUr150PEfC3WfcdpN7glw" mediniIdentifier="_NxUr150PEfC3WfcdpN7glw" id="FM045" name="Open circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow4Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxUr2Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3pq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxUr0J0PEfC3WfcdpN7glw" mediniIdentifier="_NxUr0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" alias="DIODE_100V_150mA_BAT46WQ-7-F_SOD123" description="D10,D36,D44" failureRateMode="FROM_CATALOG" partNumber="BAT46WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUr0Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxUr0Z0PEfC3WfcdpN7glw" id="FM044" name="Short circuit (reverse degradation)" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow35q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxUr0p0PEfC3WfcdpN7glw" mediniIdentifier="_NxUr0p0PEfC3WfcdpN7glw" id="FM045" name="Open circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow4Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxUr1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow3pq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEpZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEpZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_TVS__12.8V_TPSMB15CA-VR_DO214A" alias="DIODE_TVS__12.8V_TPSMB15CA-VR_DO214A" description="D33" failureRateMode="FROM_CATALOG" partNumber="TPSMB15CA-VR" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv6WkJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv6WkJ0PEfC3WfcdpN7glw" id="FM046" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow4pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv69oJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv69oJ0PEfC3WfcdpN7glw" id="FM047" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow45q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv69oZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow4Zq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEpp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEpp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" alias="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" description="D39-D41" failureRateMode="FROM_CATALOG" partNumber="PMEG10010ELR-QX" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvBlwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvBlwJ0PEfC3WfcdpN7glw" id="FM048" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvCM0J0PEfC3WfcdpN7glw" mediniIdentifier="_NvCM0J0PEfC3WfcdpN7glw" id="FM049" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvCz4J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxV58J0PEfC3WfcdpN7glw" mediniIdentifier="_NxV58J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" alias="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" description="D39-D41" failureRateMode="FROM_CATALOG" partNumber="PMEG10010ELR-QX" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV58Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxV58Z0PEfC3WfcdpN7glw" id="FM048" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV58p0PEfC3WfcdpN7glw" mediniIdentifier="_NxV58p0PEfC3WfcdpN7glw" id="FM049" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxV59J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxVS4J0PEfC3WfcdpN7glw" mediniIdentifier="_NxVS4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" alias="DIODE_SCH_100v_1A_PMEG10010ELR-QX_SOD123" description="D39-D41" failureRateMode="FROM_CATALOG" partNumber="PMEG10010ELR-QX" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxVS4Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxVS4Z0PEfC3WfcdpN7glw" id="FM048" name="Short Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxVS4p0PEfC3WfcdpN7glw" mediniIdentifier="_NxVS4p0PEfC3WfcdpN7glw" id="FM049" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxVS5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow5Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEp50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEp50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PTC_0ZCJ0010FF2E" alias="PTC_0ZCJ0010FF2E" description="F1-F4" failureRateMode="FROM_CATALOG" partNumber="0ZCJ0010FF2E" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NutcsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NutcsJ0PEfC3WfcdpN7glw" id="FM121" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDeZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuuDwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuuDwJ0PEfC3WfcdpN7glw" id="FM122" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDepq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nuuq0J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow6Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxV5_50PEfC3WfcdpN7glw" mediniIdentifier="_NxV5_50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PTC_0ZCJ0010FF2E" alias="PTC_0ZCJ0010FF2E" description="F1-F4" failureRateMode="FROM_CATALOG" partNumber="0ZCJ0010FF2E" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV6AJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxV6AJ0PEfC3WfcdpN7glw" id="FM121" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDeZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV6AZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxV6AZ0PEfC3WfcdpN7glw" id="FM122" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDepq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxV6A50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow6Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxV5-p0PEfC3WfcdpN7glw" mediniIdentifier="_NxV5-p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PTC_0ZCJ0010FF2E" alias="PTC_0ZCJ0010FF2E" description="F1-F4" failureRateMode="FROM_CATALOG" partNumber="0ZCJ0010FF2E" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV5-50PEfC3WfcdpN7glw" mediniIdentifier="_NxV5-50PEfC3WfcdpN7glw" id="FM121" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDeZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV5_J0PEfC3WfcdpN7glw" mediniIdentifier="_NxV5_J0PEfC3WfcdpN7glw" id="FM122" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDepq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxV5_p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow6Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxV59Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxV59Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PTC_0ZCJ0010FF2E" alias="PTC_0ZCJ0010FF2E" description="F1-F4" failureRateMode="FROM_CATALOG" partNumber="0ZCJ0010FF2E" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV59p0PEfC3WfcdpN7glw" mediniIdentifier="_NxV59p0PEfC3WfcdpN7glw" id="FM121" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDeZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxV5950PEfC3WfcdpN7glw" mediniIdentifier="_NxV5950PEfC3WfcdpN7glw" id="FM122" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDepq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxV5-Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow6Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEqJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEqJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PTC_RESET_FUSE_60V_100MA_0ZCH0010FF2E" alias="PTC_RESET_FUSE_60V_100MA_0ZCH0010FF2E" description="F6" failureRateMode="FROM_CATALOG" partNumber="0ZCH0010FF2E" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NumvAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NumvAJ0PEfC3WfcdpN7glw" id="FM123" name="Short Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDfJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nun9IJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nun9IJ0PEfC3WfcdpN7glw" id="FM124" name="Open Circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDfZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NuokMJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow6Zq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEqZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEqZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_BAT_CTRL_MC33774ASP1AE" alias="IC_BAT_CTRL_MC33774ASP1AE" description="IC1" failureRateMode="FROM_CATALOG" partNumber="MC33774ASP1AE" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NubI0J0PEfC3WfcdpN7glw" mediniIdentifier="_NubI0J0PEfC3WfcdpN7glw" id="FM050" name="Input/output fixed to 1" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow7Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nuc-AJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nuc-AJ0PEfC3WfcdpN7glw" id="FM051" name="Input/output fixed to 0" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow7Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NueMIJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow65q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEqp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEqp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_MICRO_S32K342EHT0MPAST_100QFP_NXP" alias="IC_MICRO_S32K342EHT0MPAST_100QFP_NXP" description="IC2" failureRateMode="FROM_CATALOG" partNumber="S32K342EHT0MPAST" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvUgsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvUgsZ0PEfC3WfcdpN7glw" id="FM052" name="Input/output fixed to 1" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow75q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvVHwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvVHwJ0PEfC3WfcdpN7glw" id="FM053" name="Input/output fixed to 0" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow8Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvVu0J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow7pq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEq50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEq50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_DGTL_ISOLTR_5KV_ISO6721QDWVRQ1_8SOIC" alias="IC_DGTL_ISOLTR_5KV_ISO6721QDWVRQ1_8SOIC" description="IC5" failureRateMode="FROM_CATALOG" partNumber="ISO6721QDWVRQ1" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwCSYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwCSYJ0PEfC3WfcdpN7glw" id="FM054" name="Input/output fixed to 1" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow8pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwCSYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwCSYZ0PEfC3WfcdpN7glw" id="FM055" name="Input/output fixed to 0" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow85q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwC5cJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow8Zq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUErJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUErJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="Automotive CAN FD Transceivers TCAN1044ADRQ1" alias="Automotive CAN FD Transceivers TCAN1044ADRQ1" description="IC6" failureRateMode="FROM_CATALOG" partNumber="TCAN1044ADRQ1" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvKvsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvKvsJ0PEfC3WfcdpN7glw" id="FM056" name="Input/output fixed to 1" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow9Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvLWwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvLWwJ0PEfC3WfcdpN7glw" id="FM057" name="Input/output fixed to 0" failureRateDistribution="50.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow9pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvL90J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow9Jq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUErZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUErZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_INA228AQDGSRQ1 _10VSSOP" alias="IC_INA228AQDGSRQ1 _10VSSOP" description="IC7" failureRateMode="FROM_CATALOG" partNumber="INA228AQDGSRQ1" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvvXcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvvXcJ0PEfC3WfcdpN7glw" id="FM058" name="Input/output fixed to 1" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow-Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvvXcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvvXcZ0PEfC3WfcdpN7glw" id="FM059" name="Input/output fixed to 0" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow-Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvvXcp0PEfC3WfcdpN7glw" mediniIdentifier="_NvvXcp0PEfC3WfcdpN7glw" id="FM060" name="Open circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow-pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvv-gJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow95q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUErp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUErp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_FLASH_W25Q128JVSIQ" alias="IC_FLASH_W25Q128JVSIQ" description="IC12" failureRateMode="FROM_CATALOG" partNumber="W25Q128JVSIQ" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nve4wJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nve4wJ0PEfC3WfcdpN7glw" id="FM061" name="Input/output fixed to 1" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow_Jq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nve4wZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nve4wZ0PEfC3WfcdpN7glw" id="FM062" name="Input/output fixed to 0" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow_Zq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvff0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nvff0J0PEfC3WfcdpN7glw" id="FM063" name="Open circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow_pq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvff0Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow-5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEr50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEr50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="IC_MCP7940NT-E_SN_8SOIC" alias="IC_MCP7940NT-E_SN_8SOIC" description="IC13" failureRateMode="FROM_CATALOG" partNumber="MCP7940NT-E_SN" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv_PEJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv_PEJ0PEfC3WfcdpN7glw" id="FM064" name="Input/output fixed to 1" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxAJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv_2IJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv_2IJ0PEfC3WfcdpN7glw" id="FM065" name="Input/output fixed to 0" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxAZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv_2IZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv_2IZ0PEfC3WfcdpN7glw" id="FM066" name="Open circuit" failureRateDistribution="90.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxApq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwAdMJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6Ow_5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEsJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="MOLEX_43045-2200" alias="MOLEX_43045-2200" description="J1" failureRateMode="FROM_CATALOG" partNumber="43045-2200" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv36UJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv36UJ0PEfC3WfcdpN7glw" id="FM125" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDmZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv4hYJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv4hYJ0PEfC3WfcdpN7glw" id="FM126" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDmpq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv4hYZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEsZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEsZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="HEADER2x7_RA_3mm_430451400" alias="HEADER2x7_RA_3mm_430451400" description="J2" failureRateMode="FROM_CATALOG" partNumber="430451400" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwGj0J0PEfC3WfcdpN7glw" mediniIdentifier="_NwGj0J0PEfC3WfcdpN7glw" id="FM127" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDnJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwGj0Z0PEfC3WfcdpN7glw" mediniIdentifier="_NwGj0Z0PEfC3WfcdpN7glw" id="FM128" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDnZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwHK4J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEsp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEsp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CONN_4POS_5023520400_SMD" alias="CONN_4POS_5023520400_SMD" description="J3-J7" failureRateMode="FROM_CATALOG" partNumber="5023520400" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nuh2gJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nuh2gJ0PEfC3WfcdpN7glw" id="FM129" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDn5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuidkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuidkJ0PEfC3WfcdpN7glw" id="FM130" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDoJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NujEoJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxYWNZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxYWNZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CONN_4POS_5023520400_SMD" alias="CONN_4POS_5023520400_SMD" description="J3-J7" failureRateMode="FROM_CATALOG" partNumber="5023520400" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxYWNp0PEfC3WfcdpN7glw" mediniIdentifier="_NxYWNp0PEfC3WfcdpN7glw" id="FM129" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDn5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxYWN50PEfC3WfcdpN7glw" mediniIdentifier="_NxYWN50PEfC3WfcdpN7glw" id="FM130" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDoJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxYWOZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxYWMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxYWMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CONN_4POS_5023520400_SMD" alias="CONN_4POS_5023520400_SMD" description="J3-J7" failureRateMode="FROM_CATALOG" partNumber="5023520400" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxYWMZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxYWMZ0PEfC3WfcdpN7glw" id="FM129" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDn5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxYWMp0PEfC3WfcdpN7glw" mediniIdentifier="_NxYWMp0PEfC3WfcdpN7glw" id="FM130" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDoJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxYWNJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxXvIp0PEfC3WfcdpN7glw" mediniIdentifier="_NxXvIp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CONN_4POS_5023520400_SMD" alias="CONN_4POS_5023520400_SMD" description="J3-J7" failureRateMode="FROM_CATALOG" partNumber="5023520400" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxXvI50PEfC3WfcdpN7glw" mediniIdentifier="_NxXvI50PEfC3WfcdpN7glw" id="FM129" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDn5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxXvJJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxXvJJ0PEfC3WfcdpN7glw" id="FM130" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDoJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxXvJp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxXIEJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxXIEJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CONN_4POS_5023520400_SMD" alias="CONN_4POS_5023520400_SMD" description="J3-J7" failureRateMode="FROM_CATALOG" partNumber="5023520400" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxXIEZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxXIEZ0PEfC3WfcdpN7glw" id="FM129" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDn5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxXIEp0PEfC3WfcdpN7glw" mediniIdentifier="_NxXIEp0PEfC3WfcdpN7glw" id="FM130" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDoJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxXvIZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxBpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEs50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEs50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="LED_ORANGE_SMD_0603" alias="LED_ORANGE_SMD_0603" description="LED1" failureRateMode="FROM_CATALOG" partNumber="TLMO1000-GS08" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwEHkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwEHkJ0PEfC3WfcdpN7glw" id="FM131" name="Short circuit (forward degradation)" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDo5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwEuoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwEuoJ0PEfC3WfcdpN7glw" id="FM132" name="Open circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDpJq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwFVsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwFVsJ0PEfC3WfcdpN7glw" id="FM133" name="Optical coupling, or fibre" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rDpZq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwF8wJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxCJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEtJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEtJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NTC_10K_0402_NTCS0402E3103JHT" alias="NTC_10K_0402_NTCS0402E3103JHT" description="NTC1,NTC2,NTC3,NTC4" failureRateMode="FROM_CATALOG" partNumber="NTCS0402E3103JHT" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NuvR4J0PEfC3WfcdpN7glw" mediniIdentifier="_NuvR4J0PEfC3WfcdpN7glw" id="FM067" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxC5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuwgAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuwgAJ0PEfC3WfcdpN7glw" id="FM068" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuxHEJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuxHEJ0PEfC3WfcdpN7glw" id="FM069" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NuxuIJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxCpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxZkUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NTC_10K_0402_NTCS0402E3103JHT" alias="NTC_10K_0402_NTCS0402E3103JHT" description="NTC1,NTC2,NTC3,NTC4" failureRateMode="FROM_CATALOG" partNumber="NTCS0402E3103JHT" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkUZ0PEfC3WfcdpN7glw" id="FM067" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxC5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkUp0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkUp0PEfC3WfcdpN7glw" id="FM068" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkU50PEfC3WfcdpN7glw" mediniIdentifier="_NxZkU50PEfC3WfcdpN7glw" id="FM069" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxZkVZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxCpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxY9Rp0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9Rp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NTC_10K_0402_NTCS0402E3103JHT" alias="NTC_10K_0402_NTCS0402E3103JHT" description="NTC1,NTC2,NTC3,NTC4" failureRateMode="FROM_CATALOG" partNumber="NTCS0402E3103JHT" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9R50PEfC3WfcdpN7glw" mediniIdentifier="_NxY9R50PEfC3WfcdpN7glw" id="FM067" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxC5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9SJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9SJ0PEfC3WfcdpN7glw" id="FM068" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9SZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9SZ0PEfC3WfcdpN7glw" id="FM069" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxY9S50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxCpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxY9QJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9QJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NTC_10K_0402_NTCS0402E3103JHT" alias="NTC_10K_0402_NTCS0402E3103JHT" description="NTC1,NTC2,NTC3,NTC4" failureRateMode="FROM_CATALOG" partNumber="NTCS0402E3103JHT" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9QZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9QZ0PEfC3WfcdpN7glw" id="FM067" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxC5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9Qp0PEfC3WfcdpN7glw" mediniIdentifier="_NxY9Qp0PEfC3WfcdpN7glw" id="FM068" name="Open Circuit" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxY9Q50PEfC3WfcdpN7glw" mediniIdentifier="_NxY9Q50PEfC3WfcdpN7glw" id="FM069" name="Drift" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxDZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxY9RZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxCpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEtZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEtZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="TRANS_NPN_100V_3A_PWRSO8_PHPT61003NYX" alias="TRANS_NPN_100V_3A_PWRSO8_PHPT61003NYX" description="Q1" failureRateMode="FROM_CATALOG" partNumber="PHPT61003NYX" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvzo4J0PEfC3WfcdpN7glw" mediniIdentifier="_Nvzo4J0PEfC3WfcdpN7glw" id="FM070" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxEJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv0P8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nv0P8J0PEfC3WfcdpN7glw" id="FM071" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxEZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv0P8Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxD5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEtp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEtp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PMOS_40V_5.8A_SOT89_HSK4101" alias="PMOS_40V_5.8A_SOT89_HSK4101" description="Q2" failureRateMode="FROM_CATALOG" partNumber="HSK4101" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvxzsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvxzsZ0PEfC3WfcdpN7glw" id="FM072" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxE5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvyawJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvyawJ0PEfC3WfcdpN7glw" id="FM073" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvzB0J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxEpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEt50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEt50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NMOS_100V_BSS123WQ-7-F_SOT23_3" alias="NMOS_100V_BSS123WQ-7-F_SOT23_3" description="Q3,Q24,Q25,Q21,Q22" failureRateMode="FROM_CATALOG" partNumber="BSS123WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv9Z4J0PEfC3WfcdpN7glw" mediniIdentifier="_Nv9Z4J0PEfC3WfcdpN7glw" id="FM074" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv-A8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nv-A8J0PEfC3WfcdpN7glw" id="FM075" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxF5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv-A8Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxaLZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaLZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NMOS_100V_BSS123WQ-7-F_SOT23_3" alias="NMOS_100V_BSS123WQ-7-F_SOT23_3" description="Q3,Q24,Q25,Q21,Q22" failureRateMode="FROM_CATALOG" partNumber="BSS123WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxaLZp0PEfC3WfcdpN7glw" mediniIdentifier="_NxaLZp0PEfC3WfcdpN7glw" id="FM074" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxaLZ50PEfC3WfcdpN7glw" mediniIdentifier="_NxaLZ50PEfC3WfcdpN7glw" id="FM075" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxF5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxaLaZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxaLYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaLYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NMOS_100V_BSS123WQ-7-F_SOT23_3" alias="NMOS_100V_BSS123WQ-7-F_SOT23_3" description="Q3,Q24,Q25,Q21,Q22" failureRateMode="FROM_CATALOG" partNumber="BSS123WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxaLYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaLYZ0PEfC3WfcdpN7glw" id="FM074" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxaLYp0PEfC3WfcdpN7glw" mediniIdentifier="_NxaLYp0PEfC3WfcdpN7glw" id="FM075" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxF5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxaLZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxZkW50PEfC3WfcdpN7glw" mediniIdentifier="_NxZkW50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NMOS_100V_BSS123WQ-7-F_SOT23_3" alias="NMOS_100V_BSS123WQ-7-F_SOT23_3" description="Q3,Q24,Q25,Q21,Q22" failureRateMode="FROM_CATALOG" partNumber="BSS123WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkXJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkXJ0PEfC3WfcdpN7glw" id="FM074" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkXZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkXZ0PEfC3WfcdpN7glw" id="FM075" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxF5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxZkX50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxZkVp0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkVp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="NMOS_100V_BSS123WQ-7-F_SOT23_3" alias="NMOS_100V_BSS123WQ-7-F_SOT23_3" description="Q3,Q24,Q25,Q21,Q22" failureRateMode="FROM_CATALOG" partNumber="BSS123WQ-7-F" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkV50PEfC3WfcdpN7glw" mediniIdentifier="_NxZkV50PEfC3WfcdpN7glw" id="FM074" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxZkWJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxZkWJ0PEfC3WfcdpN7glw" id="FM075" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxF5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxZkWp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxFZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEuJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEuJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="PMOS_20V_2.8A_SI2301Q-TPAU_SOT23" alias="PMOS_20V_2.8A_SI2301Q-TPAU_SOT23" description="Q23" failureRateMode="FROM_CATALOG" partNumber="SI2301Q-TPAU" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvoCsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvoCsZ0PEfC3WfcdpN7glw" id="FM076" name="Short Circuit" failureRateDistribution="85.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxGZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvopwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvopwJ0PEfC3WfcdpN7glw" id="FM077" name="Open Circuit" failureRateDistribution="15.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxGpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvopwZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxGJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEuZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEuZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10_OHM_1%_0603" alias="R_10_OHM_1%_0603" description="R1" failureRateMode="FROM_CATALOG" partNumber="ERJ-3EKF10R0V" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv03AJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv03AJ0PEfC3WfcdpN7glw" id="FM078" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxHZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv1eEJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv1eEJ0PEfC3WfcdpN7glw" id="FM079" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxHpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv2FIJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxHJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEup0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEup0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvjKMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvjKMJ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvjxQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvjxQJ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvjxQZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxnmxZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxnmxZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxnmxp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxnmxp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxnmx50PEfC3WfcdpN7glw" mediniIdentifier="_Nxnmx50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxnmyZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxnmwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxnmwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxnmwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxnmwZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxnmwp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxnmwp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxnmxJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxm_tZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_tZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxm_tp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_tp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxm_t50PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_t50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxm_uZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxm_sJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_sJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxm_sZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_sZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxm_sp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxm_sp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxm_tJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxmYpZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxmYpZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxmYpp0PEfC3WfcdpN7glw" mediniIdentifier="_NxmYpp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxmYp50PEfC3WfcdpN7glw" mediniIdentifier="_NxmYp50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxmYqZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxmYoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxmYoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxmYoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxmYoZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxmYop0PEfC3WfcdpN7glw" mediniIdentifier="_NxmYop0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxmYpJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxlxlZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlxlZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxlxlp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxlxlp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxlxl50PEfC3WfcdpN7glw" mediniIdentifier="_Nxlxl50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxlxmZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxlxkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlxkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxlxkZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlxkZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxlxkp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxlxkp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxlxlJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxlKhZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlKhZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxlKhp0PEfC3WfcdpN7glw" mediniIdentifier="_NxlKhp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxlKh50PEfC3WfcdpN7glw" mediniIdentifier="_NxlKh50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxlKiZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxlKgJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlKgJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxlKgZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxlKgZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxlKgp0PEfC3WfcdpN7glw" mediniIdentifier="_NxlKgp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxlKhJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxkjcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxkjcJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxkjcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxkjcZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxkjcp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxkjcp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxkjdJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxj8ZZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8ZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxj8Zp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8Zp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxj8Z50PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8Z50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxj8aZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxj8YJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8YJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxj8YZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8YZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxj8Yp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxj8Yp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxj8ZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxjVV50PEfC3WfcdpN7glw" mediniIdentifier="_NxjVV50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxjVWJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxjVWJ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxjVWZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxjVWZ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxjVW50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxjVUp0PEfC3WfcdpN7glw" mediniIdentifier="_NxjVUp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxjVU50PEfC3WfcdpN7glw" mediniIdentifier="_NxjVU50PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxjVVJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxjVVJ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxjVVp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxiuSp0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuSp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuS50PEfC3WfcdpN7glw" mediniIdentifier="_NxiuS50PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuTJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuTJ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxjVUZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxiuRZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuRp0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuRp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuR50PEfC3WfcdpN7glw" mediniIdentifier="_NxiuR50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxiuSZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxiuQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuQZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiuQp0PEfC3WfcdpN7glw" mediniIdentifier="_NxiuQp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxiuRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxiHNZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiHNZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiHNp0PEfC3WfcdpN7glw" mediniIdentifier="_NxiHNp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiHN50PEfC3WfcdpN7glw" mediniIdentifier="_NxiHN50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxiHOZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxiHMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiHMJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiHMZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxiHMZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxiHMp0PEfC3WfcdpN7glw" mediniIdentifier="_NxiHMp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxiHNJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxhgJZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxhgJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxhgJp0PEfC3WfcdpN7glw" mediniIdentifier="_NxhgJp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxhgJ50PEfC3WfcdpN7glw" mediniIdentifier="_NxhgJ50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxhgKZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxhgIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxhgIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxhgIZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxhgIZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxhgIp0PEfC3WfcdpN7glw" mediniIdentifier="_NxhgIp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxhgJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxg5FZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5FZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxg5Fp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5Fp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxg5F50PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5F50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxg5GZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxg5EJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5EJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxg5EZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5EZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxg5Ep0PEfC3WfcdpN7glw" mediniIdentifier="_Nxg5Ep0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxg5FJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxgSBZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxgSBZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxgSBp0PEfC3WfcdpN7glw" mediniIdentifier="_NxgSBp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxgSB50PEfC3WfcdpN7glw" mediniIdentifier="_NxgSB50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxgSCZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxgSAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxgSAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxgSAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxgSAZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxgSAp0PEfC3WfcdpN7glw" mediniIdentifier="_NxgSAp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxgSBJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxfq_50PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq_50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfrAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxfrAJ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfrAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxfrAZ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxfrA50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxfq-p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq-p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq-50PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq-50PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq_J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq_J0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxfq_p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxfq9Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq9Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq9p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq9p0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq950PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq950PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxfq-Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxfq8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq8J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq8Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq8Z0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxfq8p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxfq8p0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxfq9J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxfD5Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxfD5Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfD5p0PEfC3WfcdpN7glw" mediniIdentifier="_NxfD5p0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfD550PEfC3WfcdpN7glw" mediniIdentifier="_NxfD550PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxfD6Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxfD4J0PEfC3WfcdpN7glw" mediniIdentifier="_NxfD4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfD4Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxfD4Z0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxfD4p0PEfC3WfcdpN7glw" mediniIdentifier="_NxfD4p0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxfD5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxec1Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxec1Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxec1p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxec1p0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxec150PEfC3WfcdpN7glw" mediniIdentifier="_Nxec150PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxec2Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxec0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxec0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxec0Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxec0Z0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxec0p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxec0p0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxec1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxd1xZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1xZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxd1xp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1xp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxd1x50PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1x50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxd1yZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxd1wJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1wJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxd1wZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1wZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxd1wp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxd1wp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxd1xJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxdOup0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOup0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOu50PEfC3WfcdpN7glw" mediniIdentifier="_NxdOu50PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOvJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOvJ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxdOvp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxdOtZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOtZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOtp0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOtp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOt50PEfC3WfcdpN7glw" mediniIdentifier="_NxdOt50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxdOuZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxdOsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOsZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxdOsp0PEfC3WfcdpN7glw" mediniIdentifier="_NxdOsp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxdOtJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxcnoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxcnoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxcnoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxcnoZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxcnop0PEfC3WfcdpN7glw" mediniIdentifier="_Nxcnop0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxcnpJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxcAkJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxcAkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxcAkZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxcAkZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxcAkp0PEfC3WfcdpN7glw" mediniIdentifier="_NxcAkp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxcAlJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxayep0PEfC3WfcdpN7glw" mediniIdentifier="_Nxayep0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxaye50PEfC3WfcdpN7glw" mediniIdentifier="_Nxaye50PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxayfJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxayfJ0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxayfp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxaydZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaydZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxaydp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxaydp0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxayd50PEfC3WfcdpN7glw" mediniIdentifier="_Nxayd50PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxayeZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxaycJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaycJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0603" alias="R_10K_1%_0603" description="R2-R4,R7-R10,R12,R13,R17,R21,R25,R33,R37,R41,R47,R52,R56,R57,R61,R67,R72,R77,R81,R86,R90,R91,R102,R117,R135,R142,R145-R148,R184,R205,R207-R209,R213-R216,R231" failureRateMode="FROM_CATALOG" partNumber="CRCW060310K0FKEA" user_kind="internal" user_circuit_block="PDU">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxaycZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxaycZ0PEfC3WfcdpN7glw" id="FM080" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxaycp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxaycp0PEfC3WfcdpN7glw" id="FM081" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxaydJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxH5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEu50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEu50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvaAQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvaAQJ0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvaAQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvaAQZ0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvanUJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxqqEJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxqqEJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxqqEZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxqqEZ0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxqqEp0PEfC3WfcdpN7glw" mediniIdentifier="_NxqqEp0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxqqFJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxqDAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxqDAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxqDAZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxqDAZ0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxqDAp0PEfC3WfcdpN7glw" mediniIdentifier="_NxqDAp0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxqDBJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxpb9Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb9Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxpb9p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb9p0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxpb950PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb950PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxpb-Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxpb8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb8J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxpb8Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb8Z0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxpb8p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxpb8p0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxpb9J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxo04J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxo04J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxo04Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxo04Z0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxo04p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxo04p0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxo05J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxoN0J0PEfC3WfcdpN7glw" mediniIdentifier="_NxoN0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_4.99K_1%_0603" alias="R_4.99K_1%_0603" description="R5,R92-R97" failureRateMode="FROM_CATALOG" partNumber="RMCF0603FT4K99" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxoN0Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxoN0Z0PEfC3WfcdpN7glw" id="FM082" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxI5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxoN0p0PEfC3WfcdpN7glw" mediniIdentifier="_NxoN0p0PEfC3WfcdpN7glw" id="FM083" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxoN1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxIpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEvJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEvJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwHx8J0PEfC3WfcdpN7glw" mediniIdentifier="_NwHx8J0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwIZAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwIZAJ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwJAEJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx8W5Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W5Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx8W5p0PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W5p0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx8W550PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W550PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx8W6Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx8W4J0PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx8W4Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W4Z0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx8W4p0PEfC3WfcdpN7glw" mediniIdentifier="_Nx8W4p0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx8W5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx7v0p0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7v0p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7v050PEfC3WfcdpN7glw" mediniIdentifier="_Nx7v050PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7v1J0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7v1J0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx7v1p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx7IxZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7IxZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7Ixp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7Ixp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7Ix50PEfC3WfcdpN7glw" mediniIdentifier="_Nx7Ix50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx7v0Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx7IwJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7IwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7IwZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7IwZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx7Iwp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx7Iwp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx7IxJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx6htZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx6htZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx6htp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx6htp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx6ht50PEfC3WfcdpN7glw" mediniIdentifier="_Nx6ht50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx6huZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx6hsJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx6hsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx6hsZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx6hsZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx6hsp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx6hsp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx6htJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx56pZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx56pZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx56pp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx56pp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx56p50PEfC3WfcdpN7glw" mediniIdentifier="_Nx56p50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx56qZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx56oJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx56oJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx56oZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx56oZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx56op0PEfC3WfcdpN7glw" mediniIdentifier="_Nx56op0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx56pJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx5TkJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx5TkJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx5TkZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx5TkZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx5Tkp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx5Tkp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx5TlJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx4sgJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4sgJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4sgZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4sgZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4sgp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4sgp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx4shJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx4Fd50PEfC3WfcdpN7glw" mediniIdentifier="_Nx4Fd50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4FeJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4FeJ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4FeZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4FeZ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx4Fe50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx4Fcp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4Fcp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4Fc50PEfC3WfcdpN7glw" mediniIdentifier="_Nx4Fc50PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx4FdJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx4FdJ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx4Fdp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx3eZZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx3eZp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eZp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx3eZ50PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eZ50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx4FcZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx3eYJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx3eYZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eYZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx3eYp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx3eYp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx3eZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx23VZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx23VZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx23Vp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx23Vp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx23V50PEfC3WfcdpN7glw" mediniIdentifier="_Nx23V50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx23WZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx23UJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx23UJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx23UZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx23UZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx23Up0PEfC3WfcdpN7glw" mediniIdentifier="_Nx23Up0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx23VJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx2QRZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx2QRp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QRp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx2QR50PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QR50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx2QSZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx2QQJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx2QQZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QQZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx2QQp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx2QQp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx2QRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx1pOZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pOZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pOp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pOp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pO50PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pO50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx1pPZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx1pNJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pNJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pNZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pNZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pNp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pNp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx1pOJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx1CKp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CKp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pMJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pMJ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1pMZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1pMZ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx1pM50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx1CJZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1CJp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CJp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1CJ50PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CJ50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx1CKZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx1CIJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1CIZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CIZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx1CIp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx1CIp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx1CJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx0bFZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bFZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx0bFp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bFp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx0bF50PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bF50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx0bGZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx0bEJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bEJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx0bEZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bEZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx0bEp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx0bEp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx0bFJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxz0AJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxz0AJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxz0AZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxz0AZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxz0Ap0PEfC3WfcdpN7glw" mediniIdentifier="_Nxz0Ap0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxz0BJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxzM-Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM-Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM-p0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM-p0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM-50PEfC3WfcdpN7glw" mediniIdentifier="_NxzM-50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxzM_Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxzM9J0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM9J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM9Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM9Z0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM9p0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM9p0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxzM-J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxyl750PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl750PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM8J0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM8J0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxzM8Z0PEfC3WfcdpN7glw" mediniIdentifier="_NxzM8Z0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxzM850PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxyl6p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl6p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl650PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl650PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl7J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl7J0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxyl7p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxyl5Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl5Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl5p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl5p0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl550PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl550PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxyl6Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxyl4J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl4Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl4Z0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxyl4p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxyl4p0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxyl5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxx-1Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-1Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxx-1p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-1p0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxx-150PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-150PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxx-2Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxx-0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxx-0Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-0Z0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxx-0p0PEfC3WfcdpN7glw" mediniIdentifier="_Nxx-0p0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxx-1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxxXxZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxxXxZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxxXxp0PEfC3WfcdpN7glw" mediniIdentifier="_NxxXxp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxxXx50PEfC3WfcdpN7glw" mediniIdentifier="_NxxXx50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxxXyZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxxXwJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxxXwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxxXwZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxxXwZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxxXwp0PEfC3WfcdpN7glw" mediniIdentifier="_NxxXwp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxxXxJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxwwtZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwwtZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxwwtp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxwwtp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxwwt50PEfC3WfcdpN7glw" mediniIdentifier="_Nxwwt50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxwwuZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxwwsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwwsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxwwsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwwsZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxwwsp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxwwsp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxwwtJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxwJpZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwJpZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxwJpp0PEfC3WfcdpN7glw" mediniIdentifier="_NxwJpp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxwJp50PEfC3WfcdpN7glw" mediniIdentifier="_NxwJp50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxwJqZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxwJoJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwJoJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxwJoZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxwJoZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxwJop0PEfC3WfcdpN7glw" mediniIdentifier="_NxwJop0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxwJpJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxvikp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxvikp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxvik50PEfC3WfcdpN7glw" mediniIdentifier="_Nxvik50PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxvilJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxvilJ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxvilp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxu7iZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7iZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7ip0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7ip0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7i50PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7i50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxvikZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxu7hJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7hJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7hZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7hZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7hp0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7hp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxu7iJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxuUdZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxuUdZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7gJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7gJ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxu7gZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nxu7gZ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxu7g50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxuUcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxuUcJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxuUcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxuUcZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxuUcp0PEfC3WfcdpN7glw" mediniIdentifier="_NxuUcp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxuUdJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nxttap0PEfC3WfcdpN7glw" mediniIdentifier="_Nxttap0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nxtta50PEfC3WfcdpN7glw" mediniIdentifier="_Nxtta50PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxttbJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxttbJ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nxttbp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxttZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxttZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxttZp0PEfC3WfcdpN7glw" mediniIdentifier="_NxttZp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxttZ50PEfC3WfcdpN7glw" mediniIdentifier="_NxttZ50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxttaZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxttYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxttYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxttYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxttYZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxttYp0PEfC3WfcdpN7glw" mediniIdentifier="_NxttYp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxttZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxtGVZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxtGVZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxtGVp0PEfC3WfcdpN7glw" mediniIdentifier="_NxtGVp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxtGV50PEfC3WfcdpN7glw" mediniIdentifier="_NxtGV50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxtGWZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxtGUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxtGUJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxtGUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxtGUZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxtGUp0PEfC3WfcdpN7glw" mediniIdentifier="_NxtGUp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxtGVJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxsfRZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxsfRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxsfRp0PEfC3WfcdpN7glw" mediniIdentifier="_NxsfRp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxsfR50PEfC3WfcdpN7glw" mediniIdentifier="_NxsfR50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxsfSZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxsfQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxsfQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxsfQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxsfQZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxsfQp0PEfC3WfcdpN7glw" mediniIdentifier="_NxsfQp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxsfRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxrRKp0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRKp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRK50PEfC3WfcdpN7glw" mediniIdentifier="_NxrRK50PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRLJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRLJ0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxrRLp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxrRJZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRJp0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRJp0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRJ50PEfC3WfcdpN7glw" mediniIdentifier="_NxrRJ50PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxrRKZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NxrRIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_33_OHM_1%_1206" alias="R_33_OHM_1%_1206" description="R6,R11,R14-R16,R18-R20,R22-R24,R26-R32,R34-R36,R38-R40,R42-R46,R48-R51,R53-R55,R58-R60,R62-R64,R68-R70,R74-R76,R78-R80,R83-R85,R87-R89" failureRateMode="FROM_CATALOG" partNumber="ESR18EZPF33R0" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRIZ0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRIZ0PEfC3WfcdpN7glw" id="FM084" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NxrRIp0PEfC3WfcdpN7glw" mediniIdentifier="_NxrRIp0PEfC3WfcdpN7glw" id="FM085" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJ5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NxrRJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxJZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEvZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEvZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu3NsJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu3NsJ0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu30wJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu30wJ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nu4b0J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyAoUp0PEfC3WfcdpN7glw" mediniIdentifier="_NyAoUp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyAoU50PEfC3WfcdpN7glw" mediniIdentifier="_NyAoU50PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyAoVJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyAoVJ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyAoVp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyABRZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyABRZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyABRp0PEfC3WfcdpN7glw" mediniIdentifier="_NyABRp0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyABR50PEfC3WfcdpN7glw" mediniIdentifier="_NyABR50PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyAoUZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyABQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyABQJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyABQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyABQZ0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyABQp0PEfC3WfcdpN7glw" mediniIdentifier="_NyABQp0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyABRJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx_aN50PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aN50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx_aOJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aOJ0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx_aOZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aOZ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx_aO50PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx_aMp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aMp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx_aM50PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aM50PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx_aNJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx_aNJ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx_aNp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx-zKp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zKp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zK50PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zK50PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zLJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zLJ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx_aMZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx-zJZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zJZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zJp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zJp0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zJ50PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zJ50PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx-zKZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx-zIJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zIJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zIZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zIZ0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx-zIp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx-zIp0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx-zJJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx9lCp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lCp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lC50PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lC50PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lDJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lDJ0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx9lDp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx9lBZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lBZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lBp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lBp0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lB50PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lB50PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx9lCZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx9lAJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lAJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lAZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lAZ0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx9lAp0PEfC3WfcdpN7glw" mediniIdentifier="_Nx9lAp0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx9lBJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_Nx898J0PEfC3WfcdpN7glw" mediniIdentifier="_Nx898J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100_Ohm_1%_0603" alias="R_100_Ohm_1%_0603" description="R65,R66,R71,R73,R101,R138,R140,R210-R212,R217,R218,R232" failureRateMode="FROM_CATALOG" partNumber="ERA3AEB101V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx898Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nx898Z0PEfC3WfcdpN7glw" id="FM086" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nx898p0PEfC3WfcdpN7glw" mediniIdentifier="_Nx898p0PEfC3WfcdpN7glw" id="FM087" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nx899J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxKJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEvp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEvp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_14_Ohm_1%_0603" alias="R_14_Ohm_1%_0603" description="R82" failureRateMode="FROM_CATALOG" partNumber="RK73H1JTTD14R0F" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu5p8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nu5p8J0PEfC3WfcdpN7glw" id="FM088" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu7fIJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu7fIJ0PEfC3WfcdpN7glw" id="FM089" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nu8GMJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxK5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEv50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEv50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0402" alias="R_10K_1%_0402" description="R98,R100,R104-R106" failureRateMode="FROM_CATALOG" partNumber="ERJ2RKF1002X" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv8y0J0PEfC3WfcdpN7glw" mediniIdentifier="_Nv8y0J0PEfC3WfcdpN7glw" id="FM090" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxL5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv8y0Z0PEfC3WfcdpN7glw" mediniIdentifier="_Nv8y0Z0PEfC3WfcdpN7glw" id="FM091" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv8y0p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyB2dZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyB2dZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0402" alias="R_10K_1%_0402" description="R98,R100,R104-R106" failureRateMode="FROM_CATALOG" partNumber="ERJ2RKF1002X" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyB2dp0PEfC3WfcdpN7glw" mediniIdentifier="_NyB2dp0PEfC3WfcdpN7glw" id="FM090" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxL5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyB2d50PEfC3WfcdpN7glw" mediniIdentifier="_NyB2d50PEfC3WfcdpN7glw" id="FM091" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyB2eZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyB2cJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyB2cJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0402" alias="R_10K_1%_0402" description="R98,R100,R104-R106" failureRateMode="FROM_CATALOG" partNumber="ERJ2RKF1002X" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyB2cZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyB2cZ0PEfC3WfcdpN7glw" id="FM090" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxL5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyB2cp0PEfC3WfcdpN7glw" mediniIdentifier="_NyB2cp0PEfC3WfcdpN7glw" id="FM091" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyB2dJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyBPZZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyBPZZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0402" alias="R_10K_1%_0402" description="R98,R100,R104-R106" failureRateMode="FROM_CATALOG" partNumber="ERJ2RKF1002X" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyBPZp0PEfC3WfcdpN7glw" mediniIdentifier="_NyBPZp0PEfC3WfcdpN7glw" id="FM090" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxL5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyBPZ50PEfC3WfcdpN7glw" mediniIdentifier="_NyBPZ50PEfC3WfcdpN7glw" id="FM091" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyBPaZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyBPYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyBPYJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0402" alias="R_10K_1%_0402" description="R98,R100,R104-R106" failureRateMode="FROM_CATALOG" partNumber="ERJ2RKF1002X" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyBPYZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyBPYZ0PEfC3WfcdpN7glw" id="FM090" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxL5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyBPYp0PEfC3WfcdpN7glw" mediniIdentifier="_NyBPYp0PEfC3WfcdpN7glw" id="FM091" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyBPZJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxLpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEwJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEwJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_60.4Ohm_1%_0603" alias="R_60.4Ohm_1%_0603" description="R121,R124,R136,R139" failureRateMode="FROM_CATALOG" partNumber="ERJ3EKF60R4V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvDa8J0PEfC3WfcdpN7glw" mediniIdentifier="_NvDa8J0PEfC3WfcdpN7glw" id="FM092" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvF3MJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvF3MJ0PEfC3WfcdpN7glw" id="FM093" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxM5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvGeQJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyCdip0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdip0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_60.4Ohm_1%_0603" alias="R_60.4Ohm_1%_0603" description="R121,R124,R136,R139" failureRateMode="FROM_CATALOG" partNumber="ERJ3EKF60R4V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdi50PEfC3WfcdpN7glw" mediniIdentifier="_NyCdi50PEfC3WfcdpN7glw" id="FM092" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdjJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdjJ0PEfC3WfcdpN7glw" id="FM093" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxM5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyDEkZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyCdhZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdhZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_60.4Ohm_1%_0603" alias="R_60.4Ohm_1%_0603" description="R121,R124,R136,R139" failureRateMode="FROM_CATALOG" partNumber="ERJ3EKF60R4V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdhp0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdhp0PEfC3WfcdpN7glw" id="FM092" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdh50PEfC3WfcdpN7glw" mediniIdentifier="_NyCdh50PEfC3WfcdpN7glw" id="FM093" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxM5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyCdiZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyCdgJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdgJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_60.4Ohm_1%_0603" alias="R_60.4Ohm_1%_0603" description="R121,R124,R136,R139" failureRateMode="FROM_CATALOG" partNumber="ERJ3EKF60R4V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdgZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdgZ0PEfC3WfcdpN7glw" id="FM092" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyCdgp0PEfC3WfcdpN7glw" mediniIdentifier="_NyCdgp0PEfC3WfcdpN7glw" id="FM093" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxM5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyCdhJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxMZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEwZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEwZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_1R_1%_0603" alias="R_1R_1%_0603" description="R125" failureRateMode="FROM_CATALOG" partNumber="ERJU03F1R00V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwMqcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwMqcJ0PEfC3WfcdpN7glw" id="FM094" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxNZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwMqcZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwMqcZ0PEfC3WfcdpN7glw" id="FM095" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxNpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwMqcp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxNJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEwp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEwp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_453K_1%_0603" alias="R_453K_1%_0603" description="R126,R128" failureRateMode="FROM_CATALOG" partNumber="AC0603FR-07453KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvgt8J0PEfC3WfcdpN7glw" mediniIdentifier="_Nvgt8J0PEfC3WfcdpN7glw" id="FM096" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxOJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvhVAJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvhVAJ0PEfC3WfcdpN7glw" id="FM097" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxOZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvh8EJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxN5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyDEkp0PEfC3WfcdpN7glw" mediniIdentifier="_NyDEkp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_453K_1%_0603" alias="R_453K_1%_0603" description="R126,R128" failureRateMode="FROM_CATALOG" partNumber="AC0603FR-07453KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyDEk50PEfC3WfcdpN7glw" mediniIdentifier="_NyDEk50PEfC3WfcdpN7glw" id="FM096" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxOJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyDElJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyDElJ0PEfC3WfcdpN7glw" id="FM097" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxOZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyDroZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxN5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEw50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEw50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_102K_1%_0402" alias="R_102K_1%_0402" description="R129" failureRateMode="FROM_CATALOG" partNumber="CRCW0402102KFKED" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvRdYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvRdYJ0PEfC3WfcdpN7glw" id="FM098" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxO5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvSEcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvSEcJ0PEfC3WfcdpN7glw" id="FM099" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxPJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvSEcZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxOpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUExJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUExJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_330K_1%_0603_1" alias="R_330K_1%_0603_1" description="R130" failureRateMode="FROM_CATALOG" partNumber="AC0603FR-07330KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv5IcJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv5IcJ0PEfC3WfcdpN7glw" id="FM100" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxPpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv5IcZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv5IcZ0PEfC3WfcdpN7glw" id="FM101" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxP5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv5Icp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxPZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUExZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUExZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_49.9K_1%_0603" alias="R_49.9K_1%_0603" description="R131" failureRateMode="FROM_CATALOG" partNumber="ERJ3EKF4992V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwJnIJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwJnIJ0PEfC3WfcdpN7glw" id="FM102" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxQZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwKOMJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwKOMJ0PEfC3WfcdpN7glw" id="FM103" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxQpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwKOMZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxQJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUExp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUExp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100K_1%_0603" alias="R_100K_1%_0603" description="R132,R134" failureRateMode="FROM_CATALOG" partNumber="AC0603FR-07100KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvHsYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvHsYJ0PEfC3WfcdpN7glw" id="FM104" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxRJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvITcJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvITcJ0PEfC3WfcdpN7glw" id="FM105" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxRZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvKIoJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxQ5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyDrop0PEfC3WfcdpN7glw" mediniIdentifier="_NyDrop0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_100K_1%_0603" alias="R_100K_1%_0603" description="R132,R134" failureRateMode="FROM_CATALOG" partNumber="AC0603FR-07100KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyDro50PEfC3WfcdpN7glw" mediniIdentifier="_NyDro50PEfC3WfcdpN7glw" id="FM104" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxRJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyDrpJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyDrpJ0PEfC3WfcdpN7glw" id="FM105" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxRZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyDrpp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxQ5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEx50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEx50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_10K_1%_0805" alias="R_10K_1%_0805" description="R222" failureRateMode="FROM_CATALOG" partNumber="ERJHP6F1002V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwLcUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwLcUJ0PEfC3WfcdpN7glw" id="FM106" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxR5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwMDYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwMDYJ0PEfC3WfcdpN7glw" id="FM107" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwMDYZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxRpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEyJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEyJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv7ksJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv7ksJ0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nv7ksZ0PEfC3WfcdpN7glw" mediniIdentifier="_Nv7ksZ0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nv8LwJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyFg2p0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg2p0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg250PEfC3WfcdpN7glw" mediniIdentifier="_NyFg250PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg3J0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg3J0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyFg3p0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyFg1Z0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg1Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg1p0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg1p0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg150PEfC3WfcdpN7glw" mediniIdentifier="_NyFg150PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyFg2Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyFg0J0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg0Z0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg0Z0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyFg0p0PEfC3WfcdpN7glw" mediniIdentifier="_NyFg0p0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyFg1J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyE5yp0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5yp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5y50PEfC3WfcdpN7glw" mediniIdentifier="_NyE5y50PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5zJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5zJ0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyE5zp0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyE5xZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5xZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5xp0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5xp0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5x50PEfC3WfcdpN7glw" mediniIdentifier="_NyE5x50PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyE5yZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyE5wJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5wJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5wZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5wZ0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyE5wp0PEfC3WfcdpN7glw" mediniIdentifier="_NyE5wp0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyE5xJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyESsJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyESsJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_249K_0.1%_0805" alias="R_249K_0.1%_0805" description="R237-R244" failureRateMode="FROM_CATALOG" partNumber="AT0805BRD07249KL" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyESsZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyESsZ0PEfC3WfcdpN7glw" id="FM108" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyESsp0PEfC3WfcdpN7glw" mediniIdentifier="_NyESsp0PEfC3WfcdpN7glw" id="FM109" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxS5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyEStJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxSZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEyZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEyZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_200K_0.1%_0805" alias="R_200K_0.1%_0805" description="R245,R246" failureRateMode="FROM_CATALOG" partNumber="RT0805BRD07200KL" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvkYUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvkYUJ0PEfC3WfcdpN7glw" id="FM110" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvkYUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvkYUZ0PEfC3WfcdpN7glw" id="FM111" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nvk_YJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyGH4J0PEfC3WfcdpN7glw" mediniIdentifier="_NyGH4J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_200K_0.1%_0805" alias="R_200K_0.1%_0805" description="R245,R246" failureRateMode="FROM_CATALOG" partNumber="RT0805BRD07200KL" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGH4Z0PEfC3WfcdpN7glw" mediniIdentifier="_NyGH4Z0PEfC3WfcdpN7glw" id="FM110" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGH4p0PEfC3WfcdpN7glw" mediniIdentifier="_NyGH4p0PEfC3WfcdpN7glw" id="FM111" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyGH5J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxTJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEyp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEyp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_1K_0.25W_0.1%_0805" alias="R_1K_0.25W_0.1%_0805" description="R247,R248" failureRateMode="FROM_CATALOG" partNumber="RNCF0805BKE1K00" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvuJUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvuJUJ0PEfC3WfcdpN7glw" id="FM112" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvuwYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvuwYJ0PEfC3WfcdpN7glw" id="FM113" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvuwYZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxT5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyGH5Z0PEfC3WfcdpN7glw" mediniIdentifier="_NyGH5Z0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_1K_0.25W_0.1%_0805" alias="R_1K_0.25W_0.1%_0805" description="R247,R248" failureRateMode="FROM_CATALOG" partNumber="RNCF0805BKE1K00" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGH5p0PEfC3WfcdpN7glw" mediniIdentifier="_NyGH5p0PEfC3WfcdpN7glw" id="FM112" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGH550PEfC3WfcdpN7glw" mediniIdentifier="_NyGH550PEfC3WfcdpN7glw" id="FM113" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyGH6Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxT5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEy50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEy50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_1K_0.1%%_0805" alias="R_1K_0.1%%_0805" description="R249,R250" failureRateMode="FROM_CATALOG" partNumber="ERA6AEB102V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NwBEQJ0PEfC3WfcdpN7glw" mediniIdentifier="_NwBEQJ0PEfC3WfcdpN7glw" id="FM114" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxU5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NwBEQZ0PEfC3WfcdpN7glw" mediniIdentifier="_NwBEQZ0PEfC3WfcdpN7glw" id="FM115" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxVJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NwBrUJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyGu8J0PEfC3WfcdpN7glw" mediniIdentifier="_NyGu8J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_1K_0.1%%_0805" alias="R_1K_0.1%%_0805" description="R249,R250" failureRateMode="FROM_CATALOG" partNumber="ERA6AEB102V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGu8Z0PEfC3WfcdpN7glw" mediniIdentifier="_NyGu8Z0PEfC3WfcdpN7glw" id="FM114" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxU5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyGu8p0PEfC3WfcdpN7glw" mediniIdentifier="_NyGu8p0PEfC3WfcdpN7glw" id="FM115" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxVJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyGu9J0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxUpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEzJ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEzJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="R_127K_0.1%_0805" alias="R_127K_0.1%_0805" description="R251" failureRateMode="FROM_CATALOG" partNumber="ERA6KEB1273V" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nuy8QJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nuy8QJ0PEfC3WfcdpN7glw" id="FM116" name="Open Circuit" failureRateDistribution="40.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxVpq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NuzjUJ0PEfC3WfcdpN7glw" mediniIdentifier="_NuzjUJ0PEfC3WfcdpN7glw" id="FM117" name="Drift" failureRateDistribution="60.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxV5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nu2moJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxVZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEzZ0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEzZ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="Switch_SKRPABE010_SMD" alias="Switch_SKRPABE010_SMD" description="SW1,SW2" failureRateMode="FROM_CATALOG" partNumber="SKRPABE010" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nvb1cJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nvb1cJ0PEfC3WfcdpN7glw" id="FM134" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD95q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvccgJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvccgJ0PEfC3WfcdpN7glw" id="FM135" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD-Jq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvdDkJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxWZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_NyH9EJ0PEfC3WfcdpN7glw" mediniIdentifier="_NyH9EJ0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="Switch_SKRPABE010_SMD" alias="Switch_SKRPABE010_SMD" description="SW1,SW2" failureRateMode="FROM_CATALOG" partNumber="SKRPABE010" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NyH9EZ0PEfC3WfcdpN7glw" mediniIdentifier="_NyH9EZ0PEfC3WfcdpN7glw" id="FM134" name="Open Circuit" failureRateDistribution="80.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD95q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NyH9Ep0PEfC3WfcdpN7glw" mediniIdentifier="_NyH9Ep0PEfC3WfcdpN7glw" id="FM135" name="Short Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD-Jq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NyH9FJ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxWZq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEzp0PEfC3WfcdpN7glw" mediniIdentifier="_JDUEzp0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CRYSTAL_AA-16.000MALE-T_SMD2" alias="CRYSTAL_AA-16.000MALE-T_SMD2" description="Y1" failureRateMode="FROM_CATALOG" partNumber="AA-16.000MALE-T" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvMk4J0PEfC3WfcdpN7glw" mediniIdentifier="_NvMk4J0PEfC3WfcdpN7glw" id="FM136" name="Short Circuit" failureRateDistribution="95.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD-5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvNL8J0PEfC3WfcdpN7glw" mediniIdentifier="_NvNL8J0PEfC3WfcdpN7glw" id="FM137" name="Open Circuit" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD_Jq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvNL8Z0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxW5q2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUEz50PEfC3WfcdpN7glw" mediniIdentifier="_JDUEz50PEfC3WfcdpN7glw" typeCode="Hardware Part" name="CRYSTAL_ABS07AIG-32_768KHZ-7-D-T_SMD" alias="CRYSTAL_ABS07AIG-32_768KHZ-7-D-T_SMD" description="Y2" failureRateMode="FROM_CATALOG" partNumber="ABS07AIG-32_768KHZ-7-D-T" user_kind="internal" user_circuit_block="Master controller">
    <failures xsi:type="safety:FailureMode" xmi:id="_NvanUZ0PEfC3WfcdpN7glw" mediniIdentifier="_NvanUZ0PEfC3WfcdpN7glw" id="FM138" name="Short Circuit" failureRateDistribution="95.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD_pq3EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_NvbOYJ0PEfC3WfcdpN7glw" mediniIdentifier="_NvbOYJ0PEfC3WfcdpN7glw" id="FM139" name="Open Circuit" failureRateDistribution="5.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_M4rD_5q3EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_NvbOYZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxXJq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
  <the_owned_elements xsi:type="sysml:SysMLPart" xmi:id="_JDUE0J0PEfC3WfcdpN7glw" mediniIdentifier="_JDUE0J0PEfC3WfcdpN7glw" typeCode="Hardware Part" name="DIODE_ZENER_82V_SOD123_MMSZ5268BT1G" alias="DIODE_ZENER_82V_SOD123_MMSZ5268BT1G" description="Z1" failureRateMode="FROM_CATALOG" partNumber="MMSZ5268BT1G" user_kind="internal" user_circuit_block="Cell Sensing Module">
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu8tQJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu8tQJ0PEfC3WfcdpN7glw" id="FM118" name="Short Circuit" failureRateDistribution="70.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxX5q2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu9UUJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu9UUJ0PEfC3WfcdpN7glw" id="FM119" name="Open Circuit" failureRateDistribution="20.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxYJq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failures xsi:type="safety:FailureMode" xmi:id="_Nu97YJ0PEfC3WfcdpN7glw" mediniIdentifier="_Nu97YJ0PEfC3WfcdpN7glw" id="FM120" name="Drift" failureRateDistribution="10.0">
      <represents href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxYZq2EfCSa_wJ-_IumQ"/>
    </failures>
    <failureRateData xsi:type="failureratecatalogs:FailureRateData" xmi:id="_Nu97YZ0PEfC3WfcdpN7glw"/>
    <theType xsi:type="sysml:SysMLBlock" href="_s6RM4Jq2EfCSa_wJ-_IumQ.sysml#_s6OxXpq2EfCSa_wJ-_IumQ"/>
  </the_owned_elements>
</sysml:SysMLContainerPackage>
