<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_CW0j8AX3Eeq4AMRV0u5rew" mediniIdentifier="_CW0j8AX3Eeq4AMRV0u5rew" name="P-11 Table 51 - PLD: Digital I/O and Analogue I/O">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjYAX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjYAX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.1.1" name="Failure detection by on-line monitoring (Digital I/O) (Digital I/O can be periodic)" maxDC="LOW" notes="Depends on diagnostic coverage of failure detection"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjYQX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjYQX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.4.1" name="Test pattern" maxDC="HIGH" notes="Depends on type of pattern"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjYgX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjYgX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.4.2" name="Code protection for digital I/O" maxDC="MEDIUM" notes="Depends on type of coding"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjYwX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjYwX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.4.3" name="Multi-channel parallel output" maxDC="HIGH" notes="-"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjZAX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjZAX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.4.4" name="Monitored outputs" maxDC="HIGH" notes="Only if dataflow changes within diagnostic test interval"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_a7zjZQX8Eeq4AMRV0u5rew" mediniIdentifier="_a7zjZQX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.4.5" name="Input comparison/voting (1oo2, 2oo3 or better redundancy) " maxDC="HIGH" notes="Only if dataflow changes within diagnostic test interval"/>
</safety:MeasureCatalog>
