<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_x0ezAAX2Eeq4AMRV0u5rew" mediniIdentifier="_x0ezAAX2Eeq4AMRV0u5rew" name="P-11 Table 51 - PLD: Power Supply">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_XShvkAX8Eeq4AMRV0u5rew" mediniIdentifier="_XShvkAX8Eeq4AMRV0u5rew" id="ISO26262-11: Table 51" name="Separate voltage planes" description="No default typical DC given in ISO26262" notes="Voltage plane means electrically isolated voltage supply plane regions with each plane region being connectable to an external supply voltage."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_XShvkQX8Eeq4AMRV0u5rew" mediniIdentifier="_XShvkQX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.6.1" name="Voltage or current control (input)" maxDC="LOW" notes="-"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_XShvkgX8Eeq4AMRV0u5rew" mediniIdentifier="_XShvkgX8Eeq4AMRV0u5rew" id="ISO26262-5: D.2.6.2" name="Voltage or current control (output) " maxDC="HIGH" notes="-"/>
</safety:MeasureCatalog>
