<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_iH9ZENfjEe-PcMaFbaEkQg" mediniIdentifier="_iH9ZENfjEe-PcMaFbaEkQg" name="HARA F017 B 21.01.25">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8wRzINfxEe-1u6dpesWcRg" mediniIdentifier="_8wRzINfxEe-1u6dpesWcRg" id="HE70784" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8wRzIdfxEe-1u6dpesWcRg" mediniIdentifier="_8wRzIdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8weAYNfxEe-1u6dpesWcRg" mediniIdentifier="_8weAYNfxEe-1u6dpesWcRg" id="HE70785" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8weAYdfxEe-1u6dpesWcRg" mediniIdentifier="_8weAYdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8wo_gNfxEe-1u6dpesWcRg" mediniIdentifier="_8wo_gNfxEe-1u6dpesWcRg" id="HE70786" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8wo_gdfxEe-1u6dpesWcRg" mediniIdentifier="_8wo_gdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8wz-oNfxEe-1u6dpesWcRg" mediniIdentifier="_8wz-oNfxEe-1u6dpesWcRg" id="HE70787" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8wz-odfxEe-1u6dpesWcRg" mediniIdentifier="_8wz-odfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8w-9wNfxEe-1u6dpesWcRg" mediniIdentifier="_8w-9wNfxEe-1u6dpesWcRg" id="HE70788" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8w-9wdfxEe-1u6dpesWcRg" mediniIdentifier="_8w-9wdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8xJ84NfxEe-1u6dpesWcRg" mediniIdentifier="_8xJ84NfxEe-1u6dpesWcRg" id="HE70789" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8xJ84dfxEe-1u6dpesWcRg" mediniIdentifier="_8xJ84dfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8xTt4NfxEe-1u6dpesWcRg" mediniIdentifier="_8xTt4NfxEe-1u6dpesWcRg" id="HE70790" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8xTt4dfxEe-1u6dpesWcRg" mediniIdentifier="_8xTt4dfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8xeF8NfxEe-1u6dpesWcRg" mediniIdentifier="_8xeF8NfxEe-1u6dpesWcRg" id="HE70791" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8xeF8dfxEe-1u6dpesWcRg" mediniIdentifier="_8xeF8dfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8xn28NfxEe-1u6dpesWcRg" mediniIdentifier="_8xn28NfxEe-1u6dpesWcRg" id="HE70792" ISO26262_severity="S2" ISO26262_severityComment="The severity is high due to the potential for a collision with other high-speed moving vehicles, leading to catastrophic consequences." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8xn28dfxEe-1u6dpesWcRg" mediniIdentifier="_8xn28dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8xyPANfxEe-1u6dpesWcRg" mediniIdentifier="_8xyPANfxEe-1u6dpesWcRg" id="HE70793" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8xyPAdfxEe-1u6dpesWcRg" mediniIdentifier="_8xyPAdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8x8AANfxEe-1u6dpesWcRg" mediniIdentifier="_8x8AANfxEe-1u6dpesWcRg" id="HE70794" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8x8AAdfxEe-1u6dpesWcRg" mediniIdentifier="_8x8AAdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8yFxANfxEe-1u6dpesWcRg" mediniIdentifier="_8yFxANfxEe-1u6dpesWcRg" id="HE70795" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8yFxAdfxEe-1u6dpesWcRg" mediniIdentifier="_8yFxAdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8yPiANfxEe-1u6dpesWcRg" mediniIdentifier="_8yPiANfxEe-1u6dpesWcRg" id="HE70796" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur while working on the vehicle" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8yPiAdfxEe-1u6dpesWcRg" mediniIdentifier="_8yPiAdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8yZTANfxEe-1u6dpesWcRg" mediniIdentifier="_8yZTANfxEe-1u6dpesWcRg" id="HE70797" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8yZTAdfxEe-1u6dpesWcRg" mediniIdentifier="_8yZTAdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8yic8NfxEe-1u6dpesWcRg" mediniIdentifier="_8yic8NfxEe-1u6dpesWcRg" id="HE70798" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8yic8dfxEe-1u6dpesWcRg" mediniIdentifier="_8yic8dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8yrm4NfxEe-1u6dpesWcRg" mediniIdentifier="_8yrm4NfxEe-1u6dpesWcRg" id="HE70799" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8yrm4dfxEe-1u6dpesWcRg" mediniIdentifier="_8yrm4dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8y1X4NfxEe-1u6dpesWcRg" mediniIdentifier="_8y1X4NfxEe-1u6dpesWcRg" id="HE70800" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8y1X4dfxEe-1u6dpesWcRg" mediniIdentifier="_8y1X4dfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8y_I4NfxEe-1u6dpesWcRg" mediniIdentifier="_8y_I4NfxEe-1u6dpesWcRg" id="HE70801" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8y_I4dfxEe-1u6dpesWcRg" mediniIdentifier="_8y_I4dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8zIS0NfxEe-1u6dpesWcRg" mediniIdentifier="_8zIS0NfxEe-1u6dpesWcRg" id="HE70802" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8zIS0dfxEe-1u6dpesWcRg" mediniIdentifier="_8zIS0dfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8zSD0NfxEe-1u6dpesWcRg" mediniIdentifier="_8zSD0NfxEe-1u6dpesWcRg" id="HE70803" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8zSD0dfxEe-1u6dpesWcRg" mediniIdentifier="_8zSD0dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8zbNwNfxEe-1u6dpesWcRg" mediniIdentifier="_8zbNwNfxEe-1u6dpesWcRg" id="HE70804" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8zbNwdfxEe-1u6dpesWcRg" mediniIdentifier="_8zbNwdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8zk-wNfxEe-1u6dpesWcRg" mediniIdentifier="_8zk-wNfxEe-1u6dpesWcRg" id="HE70805" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8zk-wdfxEe-1u6dpesWcRg" mediniIdentifier="_8zk-wdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8zuvwNfxEe-1u6dpesWcRg" mediniIdentifier="_8zuvwNfxEe-1u6dpesWcRg" id="HE70806" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8zuvwdfxEe-1u6dpesWcRg" mediniIdentifier="_8zuvwdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8z35sNfxEe-1u6dpesWcRg" mediniIdentifier="_8z35sNfxEe-1u6dpesWcRg" id="HE70807" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8z35sdfxEe-1u6dpesWcRg" mediniIdentifier="_8z35sdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80BqsNfxEe-1u6dpesWcRg" mediniIdentifier="_80BqsNfxEe-1u6dpesWcRg" id="HE70808" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80BqsdfxEe-1u6dpesWcRg" mediniIdentifier="_80BqsdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80LbsNfxEe-1u6dpesWcRg" mediniIdentifier="_80LbsNfxEe-1u6dpesWcRg" id="HE70809" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80LbsdfxEe-1u6dpesWcRg" mediniIdentifier="_80LbsdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80VMsNfxEe-1u6dpesWcRg" mediniIdentifier="_80VMsNfxEe-1u6dpesWcRg" id="HE70810" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80VMsdfxEe-1u6dpesWcRg" mediniIdentifier="_80VMsdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80eWoNfxEe-1u6dpesWcRg" mediniIdentifier="_80eWoNfxEe-1u6dpesWcRg" id="HE70811" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80eWodfxEe-1u6dpesWcRg" mediniIdentifier="_80eWodfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Vh4O8Nl7Ee-4oP6igVcfAA" mediniIdentifier="_Vh4O8Nl7Ee-4oP6igVcfAA" id="HE72615" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Vh4O8dl7Ee-4oP6igVcfAA" mediniIdentifier="_Vh4O8dl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_X5Og0Nl7Ee-4oP6igVcfAA" mediniIdentifier="_X5Og0Nl7Ee-4oP6igVcfAA" id="HE72617" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_X5Og0dl7Ee-4oP6igVcfAA" mediniIdentifier="_X5Og0dl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YXjbkNl7Ee-4oP6igVcfAA" mediniIdentifier="_YXjbkNl7Ee-4oP6igVcfAA" id="HE72618" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_YXjbkdl7Ee-4oP6igVcfAA" mediniIdentifier="_YXjbkdl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG2CUIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80oHoNfxEe-1u6dpesWcRg" mediniIdentifier="_80oHoNfxEe-1u6dpesWcRg" id="HE70812" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80oHodfxEe-1u6dpesWcRg" mediniIdentifier="_80oHodfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_80x4oNfxEe-1u6dpesWcRg" mediniIdentifier="_80x4oNfxEe-1u6dpesWcRg" id="HE70813" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_80x4odfxEe-1u6dpesWcRg" mediniIdentifier="_80x4odfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_807poNfxEe-1u6dpesWcRg" mediniIdentifier="_807poNfxEe-1u6dpesWcRg" id="HE70814" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_807podfxEe-1u6dpesWcRg" mediniIdentifier="_807podfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81EzkNfxEe-1u6dpesWcRg" mediniIdentifier="_81EzkNfxEe-1u6dpesWcRg" id="HE70815" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81EzkdfxEe-1u6dpesWcRg" mediniIdentifier="_81EzkdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81OkkNfxEe-1u6dpesWcRg" mediniIdentifier="_81OkkNfxEe-1u6dpesWcRg" id="HE70816" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81OkkdfxEe-1u6dpesWcRg" mediniIdentifier="_81OkkdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81XugNfxEe-1u6dpesWcRg" mediniIdentifier="_81XugNfxEe-1u6dpesWcRg" id="HE70817" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81XugdfxEe-1u6dpesWcRg" mediniIdentifier="_81XugdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81hfgNfxEe-1u6dpesWcRg" mediniIdentifier="_81hfgNfxEe-1u6dpesWcRg" id="HE70818" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81hfgdfxEe-1u6dpesWcRg" mediniIdentifier="_81hfgdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81rQgNfxEe-1u6dpesWcRg" mediniIdentifier="_81rQgNfxEe-1u6dpesWcRg" id="HE70819" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81rQgdfxEe-1u6dpesWcRg" mediniIdentifier="_81rQgdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_811BgNfxEe-1u6dpesWcRg" mediniIdentifier="_811BgNfxEe-1u6dpesWcRg" id="HE70820" ISO26262_severity="S2" ISO26262_severityComment="The severity is high due to the potential for a collision with other high-speed moving vehicles, leading to catastrophic consequences." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_811BgdfxEe-1u6dpesWcRg" mediniIdentifier="_811BgdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_81-LcNfxEe-1u6dpesWcRg" mediniIdentifier="_81-LcNfxEe-1u6dpesWcRg" id="HE70821" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_81-LcdfxEe-1u6dpesWcRg" mediniIdentifier="_81-LcdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_82H8cNfxEe-1u6dpesWcRg" mediniIdentifier="_82H8cNfxEe-1u6dpesWcRg" id="HE70822" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_82H8cdfxEe-1u6dpesWcRg" mediniIdentifier="_82H8cdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_82RtcNfxEe-1u6dpesWcRg" mediniIdentifier="_82RtcNfxEe-1u6dpesWcRg" id="HE70823" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_82RtcdfxEe-1u6dpesWcRg" mediniIdentifier="_82RtcdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_82becNfxEe-1u6dpesWcRg" mediniIdentifier="_82becNfxEe-1u6dpesWcRg" id="HE70824" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur while working on the vehicle" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_82becdfxEe-1u6dpesWcRg" mediniIdentifier="_82becdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_82koYNfxEe-1u6dpesWcRg" mediniIdentifier="_82koYNfxEe-1u6dpesWcRg" id="HE70825" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_82koYdfxEe-1u6dpesWcRg" mediniIdentifier="_82koYdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_82uZYNfxEe-1u6dpesWcRg" mediniIdentifier="_82uZYNfxEe-1u6dpesWcRg" id="HE70826" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_82uZYdfxEe-1u6dpesWcRg" mediniIdentifier="_82uZYdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_824xcNfxEe-1u6dpesWcRg" mediniIdentifier="_824xcNfxEe-1u6dpesWcRg" id="HE70827" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_824xcdfxEe-1u6dpesWcRg" mediniIdentifier="_824xcdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83B7YNfxEe-1u6dpesWcRg" mediniIdentifier="_83B7YNfxEe-1u6dpesWcRg" id="HE70828" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83B7YdfxEe-1u6dpesWcRg" mediniIdentifier="_83B7YdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83LsYNfxEe-1u6dpesWcRg" mediniIdentifier="_83LsYNfxEe-1u6dpesWcRg" id="HE70829" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83LsYdfxEe-1u6dpesWcRg" mediniIdentifier="_83LsYdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83U2UNfxEe-1u6dpesWcRg" mediniIdentifier="_83U2UNfxEe-1u6dpesWcRg" id="HE70830" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83U2UdfxEe-1u6dpesWcRg" mediniIdentifier="_83U2UdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83eAQNfxEe-1u6dpesWcRg" mediniIdentifier="_83eAQNfxEe-1u6dpesWcRg" id="HE70831" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83eAQdfxEe-1u6dpesWcRg" mediniIdentifier="_83eAQdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83nKMNfxEe-1u6dpesWcRg" mediniIdentifier="_83nKMNfxEe-1u6dpesWcRg" id="HE70832" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83nKMdfxEe-1u6dpesWcRg" mediniIdentifier="_83nKMdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_83w7MNfxEe-1u6dpesWcRg" mediniIdentifier="_83w7MNfxEe-1u6dpesWcRg" id="HE70833" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_83w7MdfxEe-1u6dpesWcRg" mediniIdentifier="_83w7MdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_836FINfxEe-1u6dpesWcRg" mediniIdentifier="_836FINfxEe-1u6dpesWcRg" id="HE70834" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_836FIdfxEe-1u6dpesWcRg" mediniIdentifier="_836FIdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84DPENfxEe-1u6dpesWcRg" mediniIdentifier="_84DPENfxEe-1u6dpesWcRg" id="HE70835" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84DPEdfxEe-1u6dpesWcRg" mediniIdentifier="_84DPEdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84MZANfxEe-1u6dpesWcRg" mediniIdentifier="_84MZANfxEe-1u6dpesWcRg" id="HE70836" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84MZAdfxEe-1u6dpesWcRg" mediniIdentifier="_84MZAdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84Vi8NfxEe-1u6dpesWcRg" mediniIdentifier="_84Vi8NfxEe-1u6dpesWcRg" id="HE70837" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84Vi8dfxEe-1u6dpesWcRg" mediniIdentifier="_84Vi8dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84fT8NfxEe-1u6dpesWcRg" mediniIdentifier="_84fT8NfxEe-1u6dpesWcRg" id="HE70838" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84fT8dfxEe-1u6dpesWcRg" mediniIdentifier="_84fT8dfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84od4NfxEe-1u6dpesWcRg" mediniIdentifier="_84od4NfxEe-1u6dpesWcRg" id="HE70839" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84od4dfxEe-1u6dpesWcRg" mediniIdentifier="_84od4dfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_JMC6sNl7Ee-4oP6igVcfAA" mediniIdentifier="_JMC6sNl7Ee-4oP6igVcfAA" id="HE72612" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_JMC6sdl7Ee-4oP6igVcfAA" mediniIdentifier="_JMC6sdl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Jphg4Nl7Ee-4oP6igVcfAA" mediniIdentifier="_Jphg4Nl7Ee-4oP6igVcfAA" id="HE72613" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Jphg4dl7Ee-4oP6igVcfAA" mediniIdentifier="_Jphg4dl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_KCBgcNl7Ee-4oP6igVcfAA" mediniIdentifier="_KCBgcNl7Ee-4oP6igVcfAA" id="HE72614" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_KCBgcdl7Ee-4oP6igVcfAA" mediniIdentifier="_KCBgcdl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG00MIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_84xn0NfxEe-1u6dpesWcRg" mediniIdentifier="_84xn0NfxEe-1u6dpesWcRg" id="HE70840" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_84xn0dfxEe-1u6dpesWcRg" mediniIdentifier="_84xn0dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_846xwNfxEe-1u6dpesWcRg" mediniIdentifier="_846xwNfxEe-1u6dpesWcRg" id="HE70841" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_846xwdfxEe-1u6dpesWcRg" mediniIdentifier="_846xwdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85EiwNfxEe-1u6dpesWcRg" mediniIdentifier="_85EiwNfxEe-1u6dpesWcRg" id="HE70842" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85EiwdfxEe-1u6dpesWcRg" mediniIdentifier="_85EiwdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85NssNfxEe-1u6dpesWcRg" mediniIdentifier="_85NssNfxEe-1u6dpesWcRg" id="HE70843" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85NssdfxEe-1u6dpesWcRg" mediniIdentifier="_85NssdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85W2oNfxEe-1u6dpesWcRg" mediniIdentifier="_85W2oNfxEe-1u6dpesWcRg" id="HE70844" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85W2odfxEe-1u6dpesWcRg" mediniIdentifier="_85W2odfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85gnoNfxEe-1u6dpesWcRg" mediniIdentifier="_85gnoNfxEe-1u6dpesWcRg" id="HE70845" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85gnodfxEe-1u6dpesWcRg" mediniIdentifier="_85gnodfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85pxkNfxEe-1u6dpesWcRg" mediniIdentifier="_85pxkNfxEe-1u6dpesWcRg" id="HE70846" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85pxkdfxEe-1u6dpesWcRg" mediniIdentifier="_85pxkdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_85zikNfxEe-1u6dpesWcRg" mediniIdentifier="_85zikNfxEe-1u6dpesWcRg" id="HE70847" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_85zikdfxEe-1u6dpesWcRg" mediniIdentifier="_85zikdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_858sgNfxEe-1u6dpesWcRg" mediniIdentifier="_858sgNfxEe-1u6dpesWcRg" id="HE70848" ISO26262_severity="S2" ISO26262_severityComment="The severity is high due to the potential for a collision with other high-speed moving vehicles, leading to catastrophic consequences." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_858sgdfxEe-1u6dpesWcRg" mediniIdentifier="_858sgdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_86GdgNfxEe-1u6dpesWcRg" mediniIdentifier="_86GdgNfxEe-1u6dpesWcRg" id="HE70849" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_86GdgdfxEe-1u6dpesWcRg" mediniIdentifier="_86GdgdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_86QOgNfxEe-1u6dpesWcRg" mediniIdentifier="_86QOgNfxEe-1u6dpesWcRg" id="HE70850" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_86QOgdfxEe-1u6dpesWcRg" mediniIdentifier="_86QOgdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_86Z_gNfxEe-1u6dpesWcRg" mediniIdentifier="_86Z_gNfxEe-1u6dpesWcRg" id="HE70851" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_86Z_gdfxEe-1u6dpesWcRg" mediniIdentifier="_86Z_gdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_86jwgNfxEe-1u6dpesWcRg" mediniIdentifier="_86jwgNfxEe-1u6dpesWcRg" id="HE70852" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur while working on the vehicle" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_86jwgdfxEe-1u6dpesWcRg" mediniIdentifier="_86jwgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_86thgNfxEe-1u6dpesWcRg" mediniIdentifier="_86thgNfxEe-1u6dpesWcRg" id="HE70853" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_86thgdfxEe-1u6dpesWcRg" mediniIdentifier="_86thgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_863SgNfxEe-1u6dpesWcRg" mediniIdentifier="_863SgNfxEe-1u6dpesWcRg" id="HE70854" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_863SgdfxEe-1u6dpesWcRg" mediniIdentifier="_863SgdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87BDgNfxEe-1u6dpesWcRg" mediniIdentifier="_87BDgNfxEe-1u6dpesWcRg" id="HE70855" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87BDgdfxEe-1u6dpesWcRg" mediniIdentifier="_87BDgdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87K0gNfxEe-1u6dpesWcRg" mediniIdentifier="_87K0gNfxEe-1u6dpesWcRg" id="HE70856" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87K0gdfxEe-1u6dpesWcRg" mediniIdentifier="_87K0gdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87UlgNfxEe-1u6dpesWcRg" mediniIdentifier="_87UlgNfxEe-1u6dpesWcRg" id="HE70857" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87UlgdfxEe-1u6dpesWcRg" mediniIdentifier="_87UlgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87eWgNfxEe-1u6dpesWcRg" mediniIdentifier="_87eWgNfxEe-1u6dpesWcRg" id="HE70858" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87eWgdfxEe-1u6dpesWcRg" mediniIdentifier="_87eWgdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87oHgNfxEe-1u6dpesWcRg" mediniIdentifier="_87oHgNfxEe-1u6dpesWcRg" id="HE70859" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87oHgdfxEe-1u6dpesWcRg" mediniIdentifier="_87oHgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_87x4gNfxEe-1u6dpesWcRg" mediniIdentifier="_87x4gNfxEe-1u6dpesWcRg" id="HE70860" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_87x4gdfxEe-1u6dpesWcRg" mediniIdentifier="_87x4gdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_877pgNfxEe-1u6dpesWcRg" mediniIdentifier="_877pgNfxEe-1u6dpesWcRg" id="HE70861" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_877pgdfxEe-1u6dpesWcRg" mediniIdentifier="_877pgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88FagNfxEe-1u6dpesWcRg" mediniIdentifier="_88FagNfxEe-1u6dpesWcRg" id="HE70862" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88FagdfxEe-1u6dpesWcRg" mediniIdentifier="_88FagdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88PLgNfxEe-1u6dpesWcRg" mediniIdentifier="_88PLgNfxEe-1u6dpesWcRg" id="HE70863" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88PLgdfxEe-1u6dpesWcRg" mediniIdentifier="_88PLgdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88YVcNfxEe-1u6dpesWcRg" mediniIdentifier="_88YVcNfxEe-1u6dpesWcRg" id="HE70864" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88YVcdfxEe-1u6dpesWcRg" mediniIdentifier="_88YVcdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88iGcNfxEe-1u6dpesWcRg" mediniIdentifier="_88iGcNfxEe-1u6dpesWcRg" id="HE70865" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88iGcdfxEe-1u6dpesWcRg" mediniIdentifier="_88iGcdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88rQYNfxEe-1u6dpesWcRg" mediniIdentifier="_88rQYNfxEe-1u6dpesWcRg" id="HE70866" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88rQYdfxEe-1u6dpesWcRg" mediniIdentifier="_88rQYdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_881BYNfxEe-1u6dpesWcRg" mediniIdentifier="_881BYNfxEe-1u6dpesWcRg" id="HE70867" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_881BYdfxEe-1u6dpesWcRg" mediniIdentifier="_881BYdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_mgJG4Nl7Ee-4oP6igVcfAA" mediniIdentifier="_mgJG4Nl7Ee-4oP6igVcfAA" id="HE72619" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_mgJG4dl7Ee-4oP6igVcfAA" mediniIdentifier="_mgJG4dl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nBT6QNl7Ee-4oP6igVcfAA" mediniIdentifier="_nBT6QNl7Ee-4oP6igVcfAA" id="HE72620" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nBT6Qdl7Ee-4oP6igVcfAA" mediniIdentifier="_nBT6Qdl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nMVegNl7Ee-4oP6igVcfAA" mediniIdentifier="_nMVegNl7Ee-4oP6igVcfAA" id="HE72621" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nMVegdl7Ee-4oP6igVcfAA" mediniIdentifier="_nMVegdl7Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG3QcIIYEe-aNNVRVoOGvw"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_88-LUNfxEe-1u6dpesWcRg" mediniIdentifier="_88-LUNfxEe-1u6dpesWcRg" id="HE70868" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_88-LUdfxEe-1u6dpesWcRg" mediniIdentifier="_88-LUdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_89JxgNfxEe-1u6dpesWcRg" mediniIdentifier="_89JxgNfxEe-1u6dpesWcRg" id="HE70869" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_89JxgdfxEe-1u6dpesWcRg" mediniIdentifier="_89JxgdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_89UwoNfxEe-1u6dpesWcRg" mediniIdentifier="_89UwoNfxEe-1u6dpesWcRg" id="HE70870" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_89UwodfxEe-1u6dpesWcRg" mediniIdentifier="_89UwodfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_89fvwNfxEe-1u6dpesWcRg" mediniIdentifier="_89fvwNfxEe-1u6dpesWcRg" id="HE70871" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_89fvwdfxEe-1u6dpesWcRg" mediniIdentifier="_89fvwdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_89qH0NfxEe-1u6dpesWcRg" mediniIdentifier="_89qH0NfxEe-1u6dpesWcRg" id="HE70872" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_89qH0dfxEe-1u6dpesWcRg" mediniIdentifier="_89qH0dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_890f4NfxEe-1u6dpesWcRg" mediniIdentifier="_890f4NfxEe-1u6dpesWcRg" id="HE70873" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_890f4dfxEe-1u6dpesWcRg" mediniIdentifier="_890f4dfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_89-38NfxEe-1u6dpesWcRg" mediniIdentifier="_89-38NfxEe-1u6dpesWcRg" id="HE70874" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_89-38dfxEe-1u6dpesWcRg" mediniIdentifier="_89-38dfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8-JQANfxEe-1u6dpesWcRg" mediniIdentifier="_8-JQANfxEe-1u6dpesWcRg" id="HE70875" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8-JQAdfxEe-1u6dpesWcRg" mediniIdentifier="_8-JQAdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8-TBANfxEe-1u6dpesWcRg" mediniIdentifier="_8-TBANfxEe-1u6dpesWcRg" id="HE70876" ISO26262_severity="S2" ISO26262_severityComment="The severity is high due to the potential for a collision with other high-speed moving vehicles, leading to catastrophic consequences." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8-TBAdfxEe-1u6dpesWcRg" mediniIdentifier="_8-TBAdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8-dZENfxEe-1u6dpesWcRg" mediniIdentifier="_8-dZENfxEe-1u6dpesWcRg" id="HE70877" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8-dZEdfxEe-1u6dpesWcRg" mediniIdentifier="_8-dZEdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8-nxINfxEe-1u6dpesWcRg" mediniIdentifier="_8-nxINfxEe-1u6dpesWcRg" id="HE70878" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8-nxIdfxEe-1u6dpesWcRg" mediniIdentifier="_8-nxIdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8-4P0NfxEe-1u6dpesWcRg" mediniIdentifier="_8-4P0NfxEe-1u6dpesWcRg" id="HE70879" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8-4P0dfxEe-1u6dpesWcRg" mediniIdentifier="_8-4P0dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_CA0NfxEe-1u6dpesWcRg" mediniIdentifier="_8_CA0NfxEe-1u6dpesWcRg" id="HE70880" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur while working on the vehicle" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_CA0dfxEe-1u6dpesWcRg" mediniIdentifier="_8_CA0dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_Lx0NfxEe-1u6dpesWcRg" mediniIdentifier="_8_Lx0NfxEe-1u6dpesWcRg" id="HE70881" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_Lx0dfxEe-1u6dpesWcRg" mediniIdentifier="_8_Lx0dfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_Vi0NfxEe-1u6dpesWcRg" mediniIdentifier="_8_Vi0NfxEe-1u6dpesWcRg" id="HE70882" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_Vi0dfxEe-1u6dpesWcRg" mediniIdentifier="_8_Vi0dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_f64NfxEe-1u6dpesWcRg" mediniIdentifier="_8_f64NfxEe-1u6dpesWcRg" id="HE70883" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_f64dfxEe-1u6dpesWcRg" mediniIdentifier="_8_f64dfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_q6ANfxEe-1u6dpesWcRg" mediniIdentifier="_8_q6ANfxEe-1u6dpesWcRg" id="HE70884" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_q6AdfxEe-1u6dpesWcRg" mediniIdentifier="_8_q6AdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8_1SENfxEe-1u6dpesWcRg" mediniIdentifier="_8_1SENfxEe-1u6dpesWcRg" id="HE70885" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8_1SEdfxEe-1u6dpesWcRg" mediniIdentifier="_8_1SEdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8__DENfxEe-1u6dpesWcRg" mediniIdentifier="_8__DENfxEe-1u6dpesWcRg" id="HE70886" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8__DEdfxEe-1u6dpesWcRg" mediniIdentifier="_8__DEdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9AI0ENfxEe-1u6dpesWcRg" mediniIdentifier="_9AI0ENfxEe-1u6dpesWcRg" id="HE70887" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9AI0EdfxEe-1u6dpesWcRg" mediniIdentifier="_9AI0EdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9AR-ANfxEe-1u6dpesWcRg" mediniIdentifier="_9AR-ANfxEe-1u6dpesWcRg" id="HE70888" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9AR-AdfxEe-1u6dpesWcRg" mediniIdentifier="_9AR-AdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9AbvANfxEe-1u6dpesWcRg" mediniIdentifier="_9AbvANfxEe-1u6dpesWcRg" id="HE70889" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9AbvAdfxEe-1u6dpesWcRg" mediniIdentifier="_9AbvAdfxEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9AlgANfxEe-1u6dpesWcRg" mediniIdentifier="_9AlgANfxEe-1u6dpesWcRg" id="HE70890" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9AlgAdfxEe-1u6dpesWcRg" mediniIdentifier="_9AlgAdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9AvRANfxEe-1u6dpesWcRg" mediniIdentifier="_9AvRANfxEe-1u6dpesWcRg" id="HE70891" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9AvRAdfxEe-1u6dpesWcRg" mediniIdentifier="_9AvRAdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9A5CANfxEe-1u6dpesWcRg" mediniIdentifier="_9A5CANfxEe-1u6dpesWcRg" id="HE70892" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9A5CAdfxEe-1u6dpesWcRg" mediniIdentifier="_9A5CAdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9BDaENfxEe-1u6dpesWcRg" mediniIdentifier="_9BDaENfxEe-1u6dpesWcRg" id="HE70893" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9BDaEdfxEe-1u6dpesWcRg" mediniIdentifier="_9BDaEdfxEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9BNLENfxEe-1u6dpesWcRg" mediniIdentifier="_9BNLENfxEe-1u6dpesWcRg" id="HE70894" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9BNLEdfxEe-1u6dpesWcRg" mediniIdentifier="_9BNLEdfxEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_9BXjINfxEe-1u6dpesWcRg" mediniIdentifier="_9BXjINfxEe-1u6dpesWcRg" id="HE70895" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_9BXjIdfxEe-1u6dpesWcRg" mediniIdentifier="_9BXjIdfxEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_5Rb4INl6Ee-4oP6igVcfAA" mediniIdentifier="_5Rb4INl6Ee-4oP6igVcfAA" id="HE72609" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_5Rb4Idl6Ee-4oP6igVcfAA" mediniIdentifier="_5Rb4Idl6Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_50DdANl6Ee-4oP6igVcfAA" mediniIdentifier="_50DdANl6Ee-4oP6igVcfAA" id="HE72610" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_50DdAdl6Ee-4oP6igVcfAA" mediniIdentifier="_50DdAdl6Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_6cWzINl6Ee-4oP6igVcfAA" mediniIdentifier="_6cWzINl6Ee-4oP6igVcfAA" id="HE72611" ISO26262_severity="S1" ISO26262_severityComment="Minor or negligible injuries may occur, due to sudden braking, but the vehicle remains under driver control." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_6cWzIdl6Ee-4oP6igVcfAA" mediniIdentifier="_6cWzIdl6Ee-4oP6igVcfAA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hG0NIIIYEe-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
