<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_R1GTUExwEe2Kw8YgMgGasw" mediniIdentifier="_R1GTUExwEe2Kw8YgMgGasw" name="HARA 1">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1R5gExwEe2Kw8YgMgGasw" mediniIdentifier="_R1R5gExwEe2Kw8YgMgGasw" id="HE106" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries (Case: 2 wheelers)" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1R5gUxwEe2Kw8YgMgGasw" mediniIdentifier="_R1R5gUxwEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_operationMode="" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_XPAuMO_KEe28G7cKH-sJBw" mediniIdentifier="_XPAuMO_KEe28G7cKH-sJBw" id="HE1003" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_XPCjYO_KEe28G7cKH-sJBw" mediniIdentifier="_XPCjYO_KEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_eSsPgO_OEe28G7cKH-sJBw" mediniIdentifier="_eSsPgO_OEe28G7cKH-sJBw" id="HE1004" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_eSsPge_OEe28G7cKH-sJBw" mediniIdentifier="_eSsPge_OEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_np-DwO_VEe28G7cKH-sJBw" mediniIdentifier="_np-DwO_VEe28G7cKH-sJBw" id="HE1005" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_np-Dwe_VEe28G7cKH-sJBw" mediniIdentifier="_np-Dwe_VEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_cdk1YGDeEe2ewte9LXS6jQ" mediniIdentifier="_cdk1YGDeEe2ewte9LXS6jQ" id="HE811" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_cdtYQGDeEe2ewte9LXS6jQ" mediniIdentifier="_cdtYQGDeEe2ewte9LXS6jQ" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_operationMode="" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_f57OwFA7Ee2Kw8YgMgGasw" mediniIdentifier="_f57OwFA7Ee2Kw8YgMgGasw" id="HE736" effect="Panic braking might lead to an accident " ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_f57OwVA7Ee2Kw8YgMgGasw" mediniIdentifier="_f57OwVA7Ee2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by road condition" ISO26262_trafficAndPeople="low-density traffic" ISO26262_operationMode="" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qZzzgExVEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ASUNgEx6Ee2Kw8YgMgGasw" mediniIdentifier="_ASUNgEx6Ee2Kw8YgMgGasw" id="HE161" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_AScwYEx6Ee2Kw8YgMgGasw" mediniIdentifier="_AScwYEx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_zlu1sO_WEe28G7cKH-sJBw" mediniIdentifier="_zlu1sO_WEe28G7cKH-sJBw" id="HE1006" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_zlu1se_WEe28G7cKH-sJBw" mediniIdentifier="_zlu1se_WEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_operationMode="" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_0n9HsO_WEe28G7cKH-sJBw" mediniIdentifier="_0n9HsO_WEe28G7cKH-sJBw" id="HE1007" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_0n9Hse_WEe28G7cKH-sJBw" mediniIdentifier="_0n9Hse_WEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_1NuHMO_WEe28G7cKH-sJBw" mediniIdentifier="_1NuHMO_WEe28G7cKH-sJBw" id="HE1008" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_1NuHMe_WEe28G7cKH-sJBw" mediniIdentifier="_1NuHMe_WEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_W4Ax0GHgEe2ewte9LXS6jQ" mediniIdentifier="_W4Ax0GHgEe2ewte9LXS6jQ" id="HE848" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_W4Ax0WHgEe2ewte9LXS6jQ" mediniIdentifier="_W4Ax0WHgEe2ewte9LXS6jQ" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_4YhEkFA7Ee2Kw8YgMgGasw" mediniIdentifier="_4YhEkFA7Ee2Kw8YgMgGasw" id="HE737" effect="Panic braking might lead to an accident " ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_4YhEkVA7Ee2Kw8YgMgGasw" mediniIdentifier="_4YhEkVA7Ee2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="no impact by traffic conditions" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_RXmTcEx6Ee2Kw8YgMgGasw" mediniIdentifier="_RXmTcEx6Ee2Kw8YgMgGasw" id="HE167" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_RXmTcUx6Ee2Kw8YgMgGasw" mediniIdentifier="_RXmTcUx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Ln91wGcWEe2SPNjxy79kZw" mediniIdentifier="_Ln91wGcWEe2SPNjxy79kZw" id="HE856" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Ln91wWcWEe2SPNjxy79kZw" mediniIdentifier="_Ln91wWcWEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MduiFBEEe2Kw8YgMgGasw" mediniIdentifier="__MduiFBEEe2Kw8YgMgGasw" id="HE744" effect="Panic braking might lead to accidents" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways&#xD;&#xA;&#xD;&#xA;Possible only if other temperature sensors also fail">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MduiVBEEe2Kw8YgMgGasw" mediniIdentifier="__MduiVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_vfyekO_XEe28G7cKH-sJBw" mediniIdentifier="_vfyekO_XEe28G7cKH-sJBw" id="HE1009" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_vfyeke_XEe28G7cKH-sJBw" mediniIdentifier="_vfyeke_XEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_wJRgcO_XEe28G7cKH-sJBw" mediniIdentifier="_wJRgcO_XEe28G7cKH-sJBw" id="HE1010" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_wJRgce_XEe28G7cKH-sJBw" mediniIdentifier="_wJRgce_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_wqiacO_XEe28G7cKH-sJBw" mediniIdentifier="_wqiacO_XEe28G7cKH-sJBw" id="HE1011" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_wqiace_XEe28G7cKH-sJBw" mediniIdentifier="_wqiace_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_YONEsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1UVwExwEe2Kw8YgMgGasw" mediniIdentifier="_R1UVwExwEe2Kw8YgMgGasw" id="HE107" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lifts, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1UVwUxwEe2Kw8YgMgGasw" mediniIdentifier="_R1UVwUxwEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_AIUSsGcCEe2SPNjxy79kZw" mediniIdentifier="_AIUSsGcCEe2SPNjxy79kZw" id="HE849" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_AIVg0GcCEe2SPNjxy79kZw" mediniIdentifier="_AIVg0GcCEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MdujFBEEe2Kw8YgMgGasw" mediniIdentifier="__MdujFBEEe2Kw8YgMgGasw" id="HE746" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MdujVBEEe2Kw8YgMgGasw" mediniIdentifier="__MdujVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_3jJ4EO_XEe28G7cKH-sJBw" mediniIdentifier="_3jJ4EO_XEe28G7cKH-sJBw" id="HE1012" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_3jJ4Ee_XEe28G7cKH-sJBw" mediniIdentifier="_3jJ4Ee_XEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_4Gw7cO_XEe28G7cKH-sJBw" mediniIdentifier="_4Gw7cO_XEe28G7cKH-sJBw" id="HE1013" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_4Gw7ce_XEe28G7cKH-sJBw" mediniIdentifier="_4Gw7ce_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_4xq5oO_XEe28G7cKH-sJBw" mediniIdentifier="_4xq5oO_XEe28G7cKH-sJBw" id="HE1014" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_4x0qoO_XEe28G7cKH-sJBw" mediniIdentifier="_4x0qoO_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_cnNsUD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_UZW0QEx6Ee2Kw8YgMgGasw" mediniIdentifier="_UZW0QEx6Ee2Kw8YgMgGasw" id="HE169" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_UZW0QUx6Ee2Kw8YgMgGasw" mediniIdentifier="_UZW0QUx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_K5sKkGcCEe2SPNjxy79kZw" mediniIdentifier="_K5sKkGcCEe2SPNjxy79kZw" id="HE850" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_K5sKkWcCEe2SPNjxy79kZw" mediniIdentifier="_K5sKkWcCEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVkFBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVkFBEEe2Kw8YgMgGasw" id="HE747" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVkVBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVkVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_6R8ZkO_XEe28G7cKH-sJBw" mediniIdentifier="_6R8ZkO_XEe28G7cKH-sJBw" id="HE1015" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_6R8Zke_XEe28G7cKH-sJBw" mediniIdentifier="_6R8Zke_XEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_64NvYO_XEe28G7cKH-sJBw" mediniIdentifier="_64NvYO_XEe28G7cKH-sJBw" id="HE1016" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_64NvYe_XEe28G7cKH-sJBw" mediniIdentifier="_64NvYe_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_67tvUO_XEe28G7cKH-sJBw" mediniIdentifier="_67tvUO_XEe28G7cKH-sJBw" id="HE1017" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_67tvUe_XEe28G7cKH-sJBw" mediniIdentifier="_67tvUe_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_operationMode="" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kKNjsD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVlFBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVlFBEEe2Kw8YgMgGasw" id="HE749" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVlVBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVlVBEEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Ruk-wGcCEe2SPNjxy79kZw" mediniIdentifier="_Ruk-wGcCEe2SPNjxy79kZw" id="HE851" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Ruk-wWcCEe2SPNjxy79kZw" mediniIdentifier="_Ruk-wWcCEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Rz_qQGcCEe2SPNjxy79kZw" mediniIdentifier="_Rz_qQGcCEe2SPNjxy79kZw" id="HE852" effect="Battery gassing or TR possible, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="This can only occur in combination with temperature control related failures&#xD;&#xA;&#xD;&#xA;Underground parking, lifts, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Rz_qQWcCEe2SPNjxy79kZw" mediniIdentifier="_Rz_qQWcCEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_7uVfEO_XEe28G7cKH-sJBw" mediniIdentifier="_7uVfEO_XEe28G7cKH-sJBw" id="HE1018" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_7uVfEe_XEe28G7cKH-sJBw" mediniIdentifier="_7uVfEe_XEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_operationMode="" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8OHyYO_XEe28G7cKH-sJBw" mediniIdentifier="_8OHyYO_XEe28G7cKH-sJBw" id="HE1019" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8OHyYe_XEe28G7cKH-sJBw" mediniIdentifier="_8OHyYe_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_8R9wkO_XEe28G7cKH-sJBw" mediniIdentifier="_8R9wkO_XEe28G7cKH-sJBw" id="HE1020" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_8R9wke_XEe28G7cKH-sJBw" mediniIdentifier="_8R9wke_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kg_eQD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1Vj4ExwEe2Kw8YgMgGasw" mediniIdentifier="_R1Vj4ExwEe2Kw8YgMgGasw" id="HE108" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1Vj4UxwEe2Kw8YgMgGasw" mediniIdentifier="_R1Vj4UxwEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_nDQmsD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_mKPKoGcCEe2SPNjxy79kZw" mediniIdentifier="_mKPKoGcCEe2SPNjxy79kZw" id="HE853" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_mKPKoWcCEe2SPNjxy79kZw" mediniIdentifier="_mKPKoWcCEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_nDQmsD_ZEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVllBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVllBEEe2Kw8YgMgGasw" id="HE750" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVl1BEEe2Kw8YgMgGasw" mediniIdentifier="__MeVl1BEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_nDQmsD_ZEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dszVkEx6Ee2Kw8YgMgGasw" mediniIdentifier="_dszVkEx6Ee2Kw8YgMgGasw" id="HE173" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dszVkUx6Ee2Kw8YgMgGasw" mediniIdentifier="_dszVkUx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8F9YGcCEe2SPNjxy79kZw" mediniIdentifier="_t8F9YGcCEe2SPNjxy79kZw" id="HE854" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8F9YWcCEe2SPNjxy79kZw" mediniIdentifier="_t8F9YWcCEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_uIk6MGcCEe2SPNjxy79kZw" mediniIdentifier="_uIk6MGcCEe2SPNjxy79kZw" id="HE855" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_uIk6MWcCEe2SPNjxy79kZw" mediniIdentifier="_uIk6MWcCEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_-0xrkO_XEe28G7cKH-sJBw" mediniIdentifier="_-0xrkO_XEe28G7cKH-sJBw" id="HE1021" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_-0xrke_XEe28G7cKH-sJBw" mediniIdentifier="_-0xrke_XEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__Z7AAO_XEe28G7cKH-sJBw" mediniIdentifier="__Z7AAO_XEe28G7cKH-sJBw" id="HE1022" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__Z7AAe_XEe28G7cKH-sJBw" mediniIdentifier="__Z7AAe_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__bPOoO_XEe28G7cKH-sJBw" mediniIdentifier="__bPOoO_XEe28G7cKH-sJBw" id="HE1023" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__bPOoe_XEe28G7cKH-sJBw" mediniIdentifier="__bPOoe_XEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eIIUkExXEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1WK8ExwEe2Kw8YgMgGasw" mediniIdentifier="_R1WK8ExwEe2Kw8YgMgGasw" id="HE109" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1WK8UxwEe2Kw8YgMgGasw" mediniIdentifier="_R1WK8UxwEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVmlBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVmlBEEe2Kw8YgMgGasw" id="HE752" effect="Battery gassing, asphyxiation" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVm1BEEe2Kw8YgMgGasw" mediniIdentifier="__MeVm1BEEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVnFBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVnFBEEe2Kw8YgMgGasw" id="HE753" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVnVBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVnVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_AljssO_YEe28G7cKH-sJBw" mediniIdentifier="_AljssO_YEe28G7cKH-sJBw" id="HE1024" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Aljsse_YEe28G7cKH-sJBw" mediniIdentifier="_Aljsse_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_BQ5vwO_YEe28G7cKH-sJBw" mediniIdentifier="_BQ5vwO_YEe28G7cKH-sJBw" id="HE1025" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_BQ5vwe_YEe28G7cKH-sJBw" mediniIdentifier="_BQ5vwe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_BSg5UO_YEe28G7cKH-sJBw" mediniIdentifier="_BSg5UO_YEe28G7cKH-sJBw" id="HE1026" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_BSg5Ue_YEe28G7cKH-sJBw" mediniIdentifier="_BSg5Ue_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_IkQbsD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1WyAExwEe2Kw8YgMgGasw" mediniIdentifier="_R1WyAExwEe2Kw8YgMgGasw" id="HE110" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1WyAUxwEe2Kw8YgMgGasw" mediniIdentifier="_R1WyAUxwEe2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_zMBj8GcYEe2SPNjxy79kZw" mediniIdentifier="_zMBj8GcYEe2SPNjxy79kZw" id="HE857" effect="Battery gassing, asphyxiation, or TR" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_zMBj8WcYEe2SPNjxy79kZw" mediniIdentifier="_zMBj8WcYEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVnlBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVnlBEEe2Kw8YgMgGasw" id="HE754" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways&#xD;&#xA;&#xD;&#xA;Possible during Regen braking">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVn1BEEe2Kw8YgMgGasw" mediniIdentifier="__MeVn1BEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_C20ksO_YEe28G7cKH-sJBw" mediniIdentifier="_C20ksO_YEe28G7cKH-sJBw" id="HE1027" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_C20kse_YEe28G7cKH-sJBw" mediniIdentifier="_C20kse_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_DkLZ8O_YEe28G7cKH-sJBw" mediniIdentifier="_DkLZ8O_YEe28G7cKH-sJBw" id="HE1028" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_DkLZ8e_YEe28G7cKH-sJBw" mediniIdentifier="_DkLZ8e_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_DnsoAO_YEe28G7cKH-sJBw" mediniIdentifier="_DnsoAO_YEe28G7cKH-sJBw" id="HE1029" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_DnsoAe_YEe28G7cKH-sJBw" mediniIdentifier="_DnsoAe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_LTfCED_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_jfCZ8Ex6Ee2Kw8YgMgGasw" mediniIdentifier="_jfCZ8Ex6Ee2Kw8YgMgGasw" id="HE175" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lifts, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_jfCZ8Ux6Ee2Kw8YgMgGasw" mediniIdentifier="_jfCZ8Ux6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_OEWRQGcZEe2SPNjxy79kZw" mediniIdentifier="_OEWRQGcZEe2SPNjxy79kZw" id="HE858" effect="Battery gassing, asphyxiation, or TR" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_OEWRQWcZEe2SPNjxy79kZw" mediniIdentifier="_OEWRQWcZEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVoFBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVoFBEEe2Kw8YgMgGasw" id="HE755" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVoVBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVoVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_E9ogMO_YEe28G7cKH-sJBw" mediniIdentifier="_E9ogMO_YEe28G7cKH-sJBw" id="HE1030" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_E9ogMe_YEe28G7cKH-sJBw" mediniIdentifier="_E9ogMe_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_FvKDwO_YEe28G7cKH-sJBw" mediniIdentifier="_FvKDwO_YEe28G7cKH-sJBw" id="HE1031" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_FvKDwe_YEe28G7cKH-sJBw" mediniIdentifier="_FvKDwe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_F2sPIO_YEe28G7cKH-sJBw" mediniIdentifier="_F2sPIO_YEe28G7cKH-sJBw" id="HE1032" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_F2sPIe_YEe28G7cKH-sJBw" mediniIdentifier="_F2sPIe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_fuRrQD_bEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lO-GgEx6Ee2Kw8YgMgGasw" mediniIdentifier="_lO-GgEx6Ee2Kw8YgMgGasw" id="HE176" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lO-GgUx6Ee2Kw8YgMgGasw" mediniIdentifier="_lO-GgUx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_fKQpUGcZEe2SPNjxy79kZw" mediniIdentifier="_fKQpUGcZEe2SPNjxy79kZw" id="HE859" effect="Hazardous situation, battery fires or explosion, gassing possible " ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_fKQpUWcZEe2SPNjxy79kZw" mediniIdentifier="_fKQpUWcZEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__MeVolBEEe2Kw8YgMgGasw" mediniIdentifier="__MeVolBEEe2Kw8YgMgGasw" id="HE756" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__MeVo1BEEe2Kw8YgMgGasw" mediniIdentifier="__MeVo1BEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_HAP4MO_YEe28G7cKH-sJBw" mediniIdentifier="_HAP4MO_YEe28G7cKH-sJBw" id="HE1033" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_HAP4Me_YEe28G7cKH-sJBw" mediniIdentifier="_HAP4Me_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Hk4PQO_YEe28G7cKH-sJBw" mediniIdentifier="_Hk4PQO_YEe28G7cKH-sJBw" id="HE1034" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Hk4PQe_YEe28G7cKH-sJBw" mediniIdentifier="_Hk4PQe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_HodHsO_YEe28G7cKH-sJBw" mediniIdentifier="_HodHsO_YEe28G7cKH-sJBw" id="HE1035" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_HodHse_YEe28G7cKH-sJBw" mediniIdentifier="_HodHse_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_896G0D_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_m5w0YEx6Ee2Kw8YgMgGasw" mediniIdentifier="_m5w0YEx6Ee2Kw8YgMgGasw" id="HE177" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_m5w0YUx6Ee2Kw8YgMgGasw" mediniIdentifier="_m5w0YUx6Ee2Kw8YgMgGasw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_qbj-cGcZEe2SPNjxy79kZw" mediniIdentifier="_qbj-cGcZEe2SPNjxy79kZw" id="HE860" effect="Battery gassing, asphyxiation, or TR" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_qbj-cWcZEe2SPNjxy79kZw" mediniIdentifier="_qbj-cWcZEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="__Me8oFBEEe2Kw8YgMgGasw" mediniIdentifier="__Me8oFBEEe2Kw8YgMgGasw" id="HE757" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="__Me8oVBEEe2Kw8YgMgGasw" mediniIdentifier="__Me8oVBEEe2Kw8YgMgGasw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Jsv6sO_YEe28G7cKH-sJBw" mediniIdentifier="_Jsv6sO_YEe28G7cKH-sJBw" id="HE1036" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Jsv6se_YEe28G7cKH-sJBw" mediniIdentifier="_Jsv6se_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_operationMode="" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_OvWR4O_YEe28G7cKH-sJBw" mediniIdentifier="_OvWR4O_YEe28G7cKH-sJBw" id="HE1037" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_OvWR4e_YEe28G7cKH-sJBw" mediniIdentifier="_OvWR4e_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_O0Ox4O_YEe28G7cKH-sJBw" mediniIdentifier="_O0Ox4O_YEe28G7cKH-sJBw" id="HE1038" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_O0Ox4e_YEe28G7cKH-sJBw" mediniIdentifier="_O0Ox4e_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_operationMode="" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_gwmZYExcEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_94uP0GcbEe2SPNjxy79kZw" mediniIdentifier="_94uP0GcbEe2SPNjxy79kZw" id="HE861" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_94uP0WcbEe2SPNjxy79kZw" mediniIdentifier="_94uP0WcbEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_-ioIcGcbEe2SPNjxy79kZw" mediniIdentifier="_-ioIcGcbEe2SPNjxy79kZw" id="HE863" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_-ioIcWcbEe2SPNjxy79kZw" mediniIdentifier="_-ioIcWcbEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_-ecMAGcbEe2SPNjxy79kZw" mediniIdentifier="_-ecMAGcbEe2SPNjxy79kZw" id="HE862" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_-ecMAWcbEe2SPNjxy79kZw" mediniIdentifier="_-ecMAWcbEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QjtLcO_YEe28G7cKH-sJBw" mediniIdentifier="_QjtLcO_YEe28G7cKH-sJBw" id="HE1039" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_QjtLce_YEe28G7cKH-sJBw" mediniIdentifier="_QjtLce_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_RTNVwO_YEe28G7cKH-sJBw" mediniIdentifier="_RTNVwO_YEe28G7cKH-sJBw" id="HE1040" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_RTNVwe_YEe28G7cKH-sJBw" mediniIdentifier="_RTNVwe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_RXWO4O_YEe28G7cKH-sJBw" mediniIdentifier="_RXWO4O_YEe28G7cKH-sJBw" id="HE1041" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_RXWO4e_YEe28G7cKH-sJBw" mediniIdentifier="_RXWO4e_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_VWt6MD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Hq9l8GccEe2SPNjxy79kZw" mediniIdentifier="_Hq9l8GccEe2SPNjxy79kZw" id="HE865" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Hq9l8WccEe2SPNjxy79kZw" mediniIdentifier="_Hq9l8WccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_H_YWwGccEe2SPNjxy79kZw" mediniIdentifier="_H_YWwGccEe2SPNjxy79kZw" id="HE867" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_H_YWwWccEe2SPNjxy79kZw" mediniIdentifier="_H_YWwWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_H7G6wGccEe2SPNjxy79kZw" mediniIdentifier="_H7G6wGccEe2SPNjxy79kZw" id="HE866" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_H7G6wWccEe2SPNjxy79kZw" mediniIdentifier="_H7G6wWccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_S6KFcO_YEe28G7cKH-sJBw" mediniIdentifier="_S6KFcO_YEe28G7cKH-sJBw" id="HE1042" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_S6KFce_YEe28G7cKH-sJBw" mediniIdentifier="_S6KFce_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_U44b8O_YEe28G7cKH-sJBw" mediniIdentifier="_U44b8O_YEe28G7cKH-sJBw" id="HE1044" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_U44b8e_YEe28G7cKH-sJBw" mediniIdentifier="_U44b8e_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_operationMode="" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_U_T0EO_YEe28G7cKH-sJBw" mediniIdentifier="_U_T0EO_YEe28G7cKH-sJBw" id="HE1045" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_U_T0Ee_YEe28G7cKH-sJBw" mediniIdentifier="_U_T0Ee_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_hcziQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_N0VX8mccEe2SPNjxy79kZw" mediniIdentifier="_N0VX8mccEe2SPNjxy79kZw" id="HE869" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_N0VX82ccEe2SPNjxy79kZw" mediniIdentifier="_N0VX82ccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Oc-FQGccEe2SPNjxy79kZw" mediniIdentifier="_Oc-FQGccEe2SPNjxy79kZw" id="HE871" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Oc-FQWccEe2SPNjxy79kZw" mediniIdentifier="_Oc-FQWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_OVb54GccEe2SPNjxy79kZw" mediniIdentifier="_OVb54GccEe2SPNjxy79kZw" id="HE870" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_OVb54WccEe2SPNjxy79kZw" mediniIdentifier="_OVb54WccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_WTvQYO_YEe28G7cKH-sJBw" mediniIdentifier="_WTvQYO_YEe28G7cKH-sJBw" id="HE1046" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_WTvQYe_YEe28G7cKH-sJBw" mediniIdentifier="_WTvQYe_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_XZ6OQO_YEe28G7cKH-sJBw" mediniIdentifier="_XZ6OQO_YEe28G7cKH-sJBw" id="HE1047" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_XZ6OQe_YEe28G7cKH-sJBw" mediniIdentifier="_XZ6OQe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_XbZcAO_YEe28G7cKH-sJBw" mediniIdentifier="_XbZcAO_YEe28G7cKH-sJBw" id="HE1048" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_XbZcAe_YEe28G7cKH-sJBw" mediniIdentifier="_XbZcAe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_operationMode="" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_vZmNQD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_P0OzIGccEe2SPNjxy79kZw" mediniIdentifier="_P0OzIGccEe2SPNjxy79kZw" id="HE873" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_P0OzIWccEe2SPNjxy79kZw" mediniIdentifier="_P0OzIWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QEHpQGccEe2SPNjxy79kZw" mediniIdentifier="_QEHpQGccEe2SPNjxy79kZw" id="HE874" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_QEHpQWccEe2SPNjxy79kZw" mediniIdentifier="_QEHpQWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_QOYYgGccEe2SPNjxy79kZw" mediniIdentifier="_QOYYgGccEe2SPNjxy79kZw" id="HE875" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_QOYYgWccEe2SPNjxy79kZw" mediniIdentifier="_QOYYgWccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_YidxwO_YEe28G7cKH-sJBw" mediniIdentifier="_YidxwO_YEe28G7cKH-sJBw" id="HE1049" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Yidxwe_YEe28G7cKH-sJBw" mediniIdentifier="_Yidxwe_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_operationMode="" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ZLoqkO_YEe28G7cKH-sJBw" mediniIdentifier="_ZLoqkO_YEe28G7cKH-sJBw" id="HE1050" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ZLoqke_YEe28G7cKH-sJBw" mediniIdentifier="_ZLoqke_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ZNJGcO_YEe28G7cKH-sJBw" mediniIdentifier="_ZNJGcO_YEe28G7cKH-sJBw" id="HE1051" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ZNJGce_YEe28G7cKH-sJBw" mediniIdentifier="_ZNJGce_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_yxD4UD_eEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dbCnEGccEe2SPNjxy79kZw" mediniIdentifier="_dbCnEGccEe2SPNjxy79kZw" id="HE876" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dbCnEWccEe2SPNjxy79kZw" mediniIdentifier="_dbCnEWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_d3LwgGccEe2SPNjxy79kZw" mediniIdentifier="_d3LwgGccEe2SPNjxy79kZw" id="HE878" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_d3LwgWccEe2SPNjxy79kZw" mediniIdentifier="_d3LwgWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dqIL8GccEe2SPNjxy79kZw" mediniIdentifier="_dqIL8GccEe2SPNjxy79kZw" id="HE877" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dqIL8WccEe2SPNjxy79kZw" mediniIdentifier="_dqIL8WccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_aTC-kO_YEe28G7cKH-sJBw" mediniIdentifier="_aTC-kO_YEe28G7cKH-sJBw" id="HE1052" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_aTC-ke_YEe28G7cKH-sJBw" mediniIdentifier="_aTC-ke_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_a6PhcO_YEe28G7cKH-sJBw" mediniIdentifier="_a6PhcO_YEe28G7cKH-sJBw" id="HE1053" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_a6Phce_YEe28G7cKH-sJBw" mediniIdentifier="_a6Phce_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_a7p2sO_YEe28G7cKH-sJBw" mediniIdentifier="_a7p2sO_YEe28G7cKH-sJBw" id="HE1054" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_a7p2se_YEe28G7cKH-sJBw" mediniIdentifier="_a7p2se_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_Kzqk0ExYEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_sc9HEGccEe2SPNjxy79kZw" mediniIdentifier="_sc9HEGccEe2SPNjxy79kZw" id="HE880" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_sc9HEWccEe2SPNjxy79kZw" mediniIdentifier="_sc9HEWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_swGskGccEe2SPNjxy79kZw" mediniIdentifier="_swGskGccEe2SPNjxy79kZw" id="HE881" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_swGskWccEe2SPNjxy79kZw" mediniIdentifier="_swGskWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_tMpeoGccEe2SPNjxy79kZw" mediniIdentifier="_tMpeoGccEe2SPNjxy79kZw" id="HE882" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_tMpeoWccEe2SPNjxy79kZw" mediniIdentifier="_tMpeoWccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ckQzQO_YEe28G7cKH-sJBw" mediniIdentifier="_ckQzQO_YEe28G7cKH-sJBw" id="HE1055" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ckQzQe_YEe28G7cKH-sJBw" mediniIdentifier="_ckQzQe_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dFa_kO_YEe28G7cKH-sJBw" mediniIdentifier="_dFa_kO_YEe28G7cKH-sJBw" id="HE1056" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dFa_ke_YEe28G7cKH-sJBw" mediniIdentifier="_dFa_ke_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dG4_MO_YEe28G7cKH-sJBw" mediniIdentifier="_dG4_MO_YEe28G7cKH-sJBw" id="HE1057" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dG4_Me_YEe28G7cKH-sJBw" mediniIdentifier="_dG4_Me_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_M2CaUExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_vlas0mccEe2SPNjxy79kZw" mediniIdentifier="_vlas0mccEe2SPNjxy79kZw" id="HE883" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_vlas02ccEe2SPNjxy79kZw" mediniIdentifier="_vlas02ccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_v28hsGccEe2SPNjxy79kZw" mediniIdentifier="_v28hsGccEe2SPNjxy79kZw" id="HE884" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_v28hsWccEe2SPNjxy79kZw" mediniIdentifier="_v28hsWccEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_wfl2EGccEe2SPNjxy79kZw" mediniIdentifier="_wfl2EGccEe2SPNjxy79kZw" id="HE885" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_wfl2EWccEe2SPNjxy79kZw" mediniIdentifier="_wfl2EWccEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_es7I4O_YEe28G7cKH-sJBw" mediniIdentifier="_es7I4O_YEe28G7cKH-sJBw" id="HE1058" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_es7I4e_YEe28G7cKH-sJBw" mediniIdentifier="_es7I4e_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_fNyaQO_YEe28G7cKH-sJBw" mediniIdentifier="_fNyaQO_YEe28G7cKH-sJBw" id="HE1059" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_fNyaQe_YEe28G7cKH-sJBw" mediniIdentifier="_fNyaQe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_fPY8wO_YEe28G7cKH-sJBw" mediniIdentifier="_fPY8wO_YEe28G7cKH-sJBw" id="HE1060" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_fPY8we_YEe28G7cKH-sJBw" mediniIdentifier="_fPY8we_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_XpPeMExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hnutIGcgEe2SPNjxy79kZw" mediniIdentifier="_hnutIGcgEe2SPNjxy79kZw" id="HE886" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hnutIWcgEe2SPNjxy79kZw" mediniIdentifier="_hnutIWcgEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_h96YgGcgEe2SPNjxy79kZw" mediniIdentifier="_h96YgGcgEe2SPNjxy79kZw" id="HE887" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_h96YgWcgEe2SPNjxy79kZw" mediniIdentifier="_h96YgWcgEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_iBaYcGcgEe2SPNjxy79kZw" mediniIdentifier="_iBaYcGcgEe2SPNjxy79kZw" id="HE888" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_iBaYcWcgEe2SPNjxy79kZw" mediniIdentifier="_iBaYcWcgEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_gbN2sO_YEe28G7cKH-sJBw" mediniIdentifier="_gbN2sO_YEe28G7cKH-sJBw" id="HE1061" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_gbN2se_YEe28G7cKH-sJBw" mediniIdentifier="_gbN2se_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hKrkwO_YEe28G7cKH-sJBw" mediniIdentifier="_hKrkwO_YEe28G7cKH-sJBw" id="HE1062" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hKrkwe_YEe28G7cKH-sJBw" mediniIdentifier="_hKrkwe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hMC2sO_YEe28G7cKH-sJBw" mediniIdentifier="_hMC2sO_YEe28G7cKH-sJBw" id="HE1063" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hMC2se_YEe28G7cKH-sJBw" mediniIdentifier="_hMC2se_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZK7TYExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_i3IfgGcgEe2SPNjxy79kZw" mediniIdentifier="_i3IfgGcgEe2SPNjxy79kZw" id="HE889" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_i3IfgWcgEe2SPNjxy79kZw" mediniIdentifier="_i3IfgWcgEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_jPhxYGcgEe2SPNjxy79kZw" mediniIdentifier="_jPhxYGcgEe2SPNjxy79kZw" id="HE890" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_jPhxYWcgEe2SPNjxy79kZw" mediniIdentifier="_jPhxYWcgEe2SPNjxy79kZw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_jQvSUGcgEe2SPNjxy79kZw" mediniIdentifier="_jQvSUGcgEe2SPNjxy79kZw" id="HE891" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_jQvSUWcgEe2SPNjxy79kZw" mediniIdentifier="_jQvSUWcgEe2SPNjxy79kZw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ircM4O_YEe28G7cKH-sJBw" mediniIdentifier="_ircM4O_YEe28G7cKH-sJBw" id="HE1064" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ircM4e_YEe28G7cKH-sJBw" mediniIdentifier="_ircM4e_YEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_jkTHgO_YEe28G7cKH-sJBw" mediniIdentifier="_jkTHgO_YEe28G7cKH-sJBw" id="HE1065" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_jkTHge_YEe28G7cKH-sJBw" mediniIdentifier="_jkTHge_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_jltcwO_YEe28G7cKH-sJBw" mediniIdentifier="_jltcwO_YEe28G7cKH-sJBw" id="HE1066" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_jltcwe_YEe28G7cKH-sJBw" mediniIdentifier="_jltcwe_YEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_eKRiQExaEe2zRcf-1tDSGA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_LHXZUPCuEe28G7cKH-sJBw" mediniIdentifier="_LHXZUPCuEe28G7cKH-sJBw" id="HE1124" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S2" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries" ISO26262_exposure="E3" ISO26262_exposureComment="Removable batteries are taken into closed spaces once every 2 to 3 on an average (B.3)" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by drivers or nearby people (C3)" user_Assumptions="Underground parking, lift; removable / swappable battery charging in closed locations such as rooms or apartments, or any other closed spaces, smoking can cause asphysxiation or other respiratory issues to nearby people, specially in enclosed spaces from where escaping is difficult;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_LHXZUfCuEe28G7cKH-sJBw" mediniIdentifier="_LHXZUfCuEe28G7cKH-sJBw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_PCZEcPCuEe28G7cKH-sJBw" mediniIdentifier="_PCZEcPCuEe28G7cKH-sJBw" id="HE1125" effect="Hazardous situation, battery fires or explosion, gassing possible " ISO26262_severity="S1" ISO26262_severityComment="Light to moderate injuries possible in close proximity" ISO26262_exposure="E4" ISO26262_exposureComment="Vehicle stopped or charging " ISO26262_controllability="C2" ISO26262_controllabilityComment="People can run away / escape" user_Assumptions="Any space from where escape is not difficult; vehicle is stopped or recharging">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_PCZEcfCuEe28G7cKH-sJBw" mediniIdentifier="_PCZEcfCuEe28G7cKH-sJBw" ISO26262_location="any location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="children, elderly or disabled people" ISO26262_itemUsage="stopped or refuelling" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="not moving">
      <user_further_situation_properties>parking lot</user_further_situation_properties>
      <user_further_situation_properties>parking structure</user_further_situation_properties>
      <user_further_situation_properties>garage (general for service)</user_further_situation_properties>
      <user_further_situation_properties>gas station</user_further_situation_properties>
      <user_further_situation_properties>parking</user_further_situation_properties>
    </operationalSituation>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_RhincPCuEe28G7cKH-sJBw" mediniIdentifier="_RhincPCuEe28G7cKH-sJBw" id="HE1126" effect="Battery gassing, panic braking" ISO26262_severity="S1" ISO26262_severityComment="Panic braking might lead to topple over and minor injuries " ISO26262_exposure="E4" ISO26262_exposureComment="General driving condition" ISO26262_controllability="C1" ISO26262_controllabilityComment="Generally controllable by the largest part of target population" user_Assumptions="If gassing occurs when vehicle is at high speeds, it could lead to accidents due to panic, specially on highways">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_RhincfCuEe28G7cKH-sJBw" mediniIdentifier="_RhincfCuEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="any environmental condition" ISO26262_trafficAndPeople="high-density traffic" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-specific collision</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_RmQvYPCuEe28G7cKH-sJBw" mediniIdentifier="_RmQvYPCuEe28G7cKH-sJBw" id="HE1127" effect="Exposure to battery gases to passengers, rescue personnel, or nearby people" ISO26262_severity="S3" ISO26262_severityComment="Hazard occurring in difficult-to-escape spaces can cause &gt;AIS3 injuries. Passengers might try to jump out of running vehicle, causing collision or non-collision injuries (Case: 3 wheelers)" ISO26262_exposure="E1" ISO26262_exposureComment="Considered case is a very corner case / extreme case" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver could stop the vehicle by applying the mechanical brakes so its easy to evacuate." user_Assumptions="q1 Case: TR occurred in a moving L5 passenger vehicle with passengers onboard. Passengers might try to jump out of moving vehicle.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_RmQvYfCuEe28G7cKH-sJBw" mediniIdentifier="_RmQvYfCuEe28G7cKH-sJBw" ISO26262_location="normal road" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="persons in vehicle" ISO26262_itemUsage="general driving" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_R1WUQPCuEe28G7cKH-sJBw" mediniIdentifier="_R1WUQPCuEe28G7cKH-sJBw" id="HE1128" effect="Exposure to battery gases to the person sleeping, rescue personnel, or nearby people. Might cause gas inhalation or fire-related injuries." ISO26262_severity="S3" ISO26262_severityComment="Gassing / TR might lead to asphyxiation of the sleeping driver" ISO26262_exposure="E3" ISO26262_exposureComment="Drivers often sleep in their vehicles during day or night" ISO26262_controllability="C2" ISO26262_controllabilityComment="Person can wake up and run away. Assumption: LFP battery is used on L5 vehicles." user_Assumptions="q2 Case: Driver sleeping in L5 passenger or cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_R1WUQfCuEe28G7cKH-sJBw" mediniIdentifier="_R1WUQfCuEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="person sleeping in vehicle" ISO26262_itemUsage="stopped" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_UfbU4PCuEe28G7cKH-sJBw" mediniIdentifier="_UfbU4PCuEe28G7cKH-sJBw" id="HE1129" effect="DG might also catch fire, leading to even larger and/or uncontrollable fires and smoke" ISO26262_severity="S3" ISO26262_severityComment="Battery + DG fire combined" ISO26262_exposure="E2" ISO26262_exposureComment="Very low probability of both, the battery and the DG catching fire" ISO26262_controllability="C2" ISO26262_controllabilityComment="Driver ideally gets sufficient time to get out of the vehicle" user_Assumptions="q3 Case: DG being transported on L5 cargo vehicle">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_UfbU4fCuEe28G7cKH-sJBw" mediniIdentifier="_UfbU4fCuEe28G7cKH-sJBw" ISO26262_location="no impact by location" ISO26262_roadConditions="no impact by road condition" ISO26262_environment="no impact by environment conditions" ISO26262_trafficAndPeople="dangerous good transport" ISO26262_itemUsage="any item usage" ISO26262_defaultExposure="" ISO26262_defaultExposureComment="" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_GAzDoD_fEe2PnvlPKZ-oHA"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
    <user_accident_type>non-collision injury (inside of car or falling out)</user_accident_type>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
