<?xml version="1.1" encoding="UTF-8"?>
<de.ikv.analyze.checklist:Checklist xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:de.ikv.analyze.checklist="http:///de/ikv/analyze/checklist.ecore" xmi:id="_ogXQwG9IEeqG1abzinpicA" mediniIdentifier="_ogXQwG9IEeqG1abzinpicA" name="Checklist: Dependent Failure Analysis (ISO26262-2nd Ed.:Part11 -Table 21-26)" version="26/03/2020 11:00">
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_yecDcG9IEeqG1abzinpicA" mediniIdentifier="_yecDcG9IEeqG1abzinpicA" name="Dependent failure initiators due to random hardware faults of shared resources" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OsuBoG9KEeqG1abzinpicA" mediniIdentifier="_OsuBoG9KEeqG1abzinpicA" name="Failures in common clock elements (including PLL, clock trees, clock enable signals, etc.)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_TbBj0G9KEeqG1abzinpicA" mediniIdentifier="_TbBj0G9KEeqG1abzinpicA" name="Failures in common test logic including DFT (Design for Test) signals, scan chains etc., common debug logic including debug routing network (network that provides access to analogue or digital signals or enables reading of digital registers) and trace signals (mechanism to trace one or more signals synchronously, e.g. controlled by triggers or trace clocks and read the result afterwards)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_WDKDsG9KEeqG1abzinpicA" mediniIdentifier="_WDKDsG9KEeqG1abzinpicA" name="Failures in power supply elements including power distribution network, common voltage regulators, common references (e.g. band-gaps, bias generators and related network)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_bfvBIG9KEeqG1abzinpicA" mediniIdentifier="_bfvBIG9KEeqG1abzinpicA" name="Non simultaneous supply switch on, that can cause effects like latch up or high inrush current" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_cXH8IG9KEeqG1abzinpicA" mediniIdentifier="_cXH8IG9KEeqG1abzinpicA" name="Failures in common reset logic including reset signals" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_e2KxcG9KEeqG1abzinpicA" mediniIdentifier="_e2KxcG9KEeqG1abzinpicA" name="Failures in shared modules (e.g. RAM, Flash, ADC, Timers, DMA, Interrupt Controller, Busses, etc.)" user_Description=""/>
  </items>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kL5gAG9KEeqG1abzinpicA" mediniIdentifier="_kL5gAG9KEeqG1abzinpicA" name="Dependent failures initiators due to random physical root causes" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_m_MHAG9KEeqG1abzinpicA" mediniIdentifier="_m_MHAG9KEeqG1abzinpicA" name="Short circuits (e.g.: local defects, electro migration, via migration, contact migration, oxide break down)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_pqJRYG9KEeqG1abzinpicA" mediniIdentifier="_pqJRYG9KEeqG1abzinpicA" name="Latch up" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_z0gMkG9KEeqG1abzinpicA" mediniIdentifier="_z0gMkG9KEeqG1abzinpicA" name="Cross talk (substrate current, capacitive coupling) " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_tItC8G9KEeqG1abzinpicA" mediniIdentifier="_tItC8G9KEeqG1abzinpicA" name="Local heating caused e.g. by defective voltage regulators or output drivers" user_Description=""/>
  </items>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_5Nd1UG9KEeqG1abzinpicA" mediniIdentifier="_5Nd1UG9KEeqG1abzinpicA" name="Systematic dependent failure initiators due to environmental conditions" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_6CVn0G9KEeqG1abzinpicA" mediniIdentifier="_6CVn0G9KEeqG1abzinpicA" name="Temperature " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_9Gt-0G9KEeqG1abzinpicA" mediniIdentifier="_9Gt-0G9KEeqG1abzinpicA" name="Vibration Pressure" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_AQDuUG9LEeqG1abzinpicA" mediniIdentifier="_AQDuUG9LEeqG1abzinpicA" name=" Humidity/Condensation " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_BpFWwG9LEeqG1abzinpicA" mediniIdentifier="_BpFWwG9LEeqG1abzinpicA" name="Corrosion " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_DW3HMG9LEeqG1abzinpicA" mediniIdentifier="_DW3HMG9LEeqG1abzinpicA" name="EMI " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_E9nCkG9LEeqG1abzinpicA" mediniIdentifier="_E9nCkG9LEeqG1abzinpicA" name="Overvoltage applied from external " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_HQXvYG9LEeqG1abzinpicA" mediniIdentifier="_HQXvYG9LEeqG1abzinpicA" name="Mechanical stress " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_IuLKIG9LEeqG1abzinpicA" mediniIdentifier="_IuLKIG9LEeqG1abzinpicA" name="Wear " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_KNQXQG9LEeqG1abzinpicA" mediniIdentifier="_KNQXQG9LEeqG1abzinpicA" name="Aging " user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_LrFnMG9LEeqG1abzinpicA" mediniIdentifier="_LrFnMG9LEeqG1abzinpicA" name="Water and other fluids intrusion" user_Description=""/>
  </items>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Qfr-oG9LEeqG1abzinpicA" mediniIdentifier="_Qfr-oG9LEeqG1abzinpicA" name="Systematic dependent failure initiators due to development faults" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_RP1pMG9LEeqG1abzinpicA" mediniIdentifier="_RP1pMG9LEeqG1abzinpicA" name="Requirement faults" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_b2dCkG9LEeqG1abzinpicA" mediniIdentifier="_b2dCkG9LEeqG1abzinpicA" name="Specification errors" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_chLakG9LEeqG1abzinpicA" mediniIdentifier="_chLakG9LEeqG1abzinpicA" name="Implementation faults, i.e. incorrect implementation of functionality" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_d5rekG9LEeqG1abzinpicA" mediniIdentifier="_d5rekG9LEeqG1abzinpicA" name="Lack or insufficiency of design measures to avoid crosstalk" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_goi4kG9LEeqG1abzinpicA" mediniIdentifier="_goi4kG9LEeqG1abzinpicA" name="Lack or insufficiency of Latch up prevention measures" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_h8oWoG9LEeqG1abzinpicA" mediniIdentifier="_h8oWoG9LEeqG1abzinpicA" name="Wrong configuration" user_Description=""/>
  </items>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_jYyLkG9LEeqG1abzinpicA" mediniIdentifier="_jYyLkG9LEeqG1abzinpicA" name="Layout faults, such as incorrect routing e.g. over redundant blocks, insufficient insulation, insufficient separation or isolation, insufficient EMI shielding" user_Description=""/>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_lOqIEG9LEeqG1abzinpicA" mediniIdentifier="_lOqIEG9LEeqG1abzinpicA" name="Temperature due to heating of power consuming parts of the die Temperature gradients causing mismatches within sensitive measurement circuitry" user_Description=""/>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_mEgyAG9LEeqG1abzinpicA" mediniIdentifier="_mEgyAG9LEeqG1abzinpicA" name="Systematic dependent failure initiators due to manufacturing faults" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_oX1fgG9LEeqG1abzinpicA" mediniIdentifier="_oX1fgG9LEeqG1abzinpicA" name="Related to processes procedures and training" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_phdaAG9LEeqG1abzinpicA" mediniIdentifier="_phdaAG9LEeqG1abzinpicA" name="Faults in control plans and in monitoring of special characteristics" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_soW5gG9LEeqG1abzinpicA" mediniIdentifier="_soW5gG9LEeqG1abzinpicA" name="Related to software flashing and end-of-line programming (e.g. wrong versions or wrong programming conditions, protocols or timings)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_uyTBgG9LEeqG1abzinpicA" mediniIdentifier="_uyTBgG9LEeqG1abzinpicA" name="Mask misalignment" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_wnyjgG9LEeqG1abzinpicA" mediniIdentifier="_wnyjgG9LEeqG1abzinpicA" name="Incorrect End-of-Line trimming or fusing (e.g. Laser trimming, OTP or EEPROM programming of calibration coefficients or customization settings)" user_Description=""/>
  </items>
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_1Vr2AG9LEeqG1abzinpicA" mediniIdentifier="_1Vr2AG9LEeqG1abzinpicA" name="Systematic dependent failure initiators due to installation faults" user_Description="">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_1wY1AG9LEeqG1abzinpicA" mediniIdentifier="_1wY1AG9LEeqG1abzinpicA" name="Related to wiring harness routing" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_4D2scG9LEeqG1abzinpicA" mediniIdentifier="_4D2scG9LEeqG1abzinpicA" name="Related to the inter-changeability of parts" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_5YBDAG9LEeqG1abzinpicA" mediniIdentifier="_5YBDAG9LEeqG1abzinpicA" name="Failures of adjacent items or parts or elements. (e.g. wrong configuration of a connected interface delivering data to an input, or incorrect load on a driven output)" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_7NHjcG9LEeqG1abzinpicA" mediniIdentifier="_7NHjcG9LEeqG1abzinpicA" name="Wrong PCB connection" user_Description=""/>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_84dq8G9LEeqG1abzinpicA" mediniIdentifier="_84dq8G9LEeqG1abzinpicA" name="Wrong configuration (e.g. of spare memory usage)" user_Description=""/>
  </items>
</de.ikv.analyze.checklist:Checklist>
