<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_W4QMINfzEe-1u6dpesWcRg" mediniIdentifier="_W4QMINfzEe-1u6dpesWcRg" name="HARA F024 B 21.01.25">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kpWkgNfzEe-1u6dpesWcRg" mediniIdentifier="_kpWkgNfzEe-1u6dpesWcRg" id="HE71820" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kpWkgdfzEe-1u6dpesWcRg" mediniIdentifier="_kpWkgdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kphjoNfzEe-1u6dpesWcRg" mediniIdentifier="_kphjoNfzEe-1u6dpesWcRg" id="HE71821" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kphjodfzEe-1u6dpesWcRg" mediniIdentifier="_kphjodfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kpsiwNfzEe-1u6dpesWcRg" mediniIdentifier="_kpsiwNfzEe-1u6dpesWcRg" id="HE71822" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kpsiwdfzEe-1u6dpesWcRg" mediniIdentifier="_kpsiwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kp3h4NfzEe-1u6dpesWcRg" mediniIdentifier="_kp3h4NfzEe-1u6dpesWcRg" id="HE71823" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kp3h4dfzEe-1u6dpesWcRg" mediniIdentifier="_kp3h4dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kqChANfzEe-1u6dpesWcRg" mediniIdentifier="_kqChANfzEe-1u6dpesWcRg" id="HE71824" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kqChAdfzEe-1u6dpesWcRg" mediniIdentifier="_kqChAdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kqNgINfzEe-1u6dpesWcRg" mediniIdentifier="_kqNgINfzEe-1u6dpesWcRg" id="HE71825" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kqNgIdfzEe-1u6dpesWcRg" mediniIdentifier="_kqNgIdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kqX4MNfzEe-1u6dpesWcRg" mediniIdentifier="_kqX4MNfzEe-1u6dpesWcRg" id="HE71826" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kqX4MdfzEe-1u6dpesWcRg" mediniIdentifier="_kqX4MdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kqiQQNfzEe-1u6dpesWcRg" mediniIdentifier="_kqiQQNfzEe-1u6dpesWcRg" id="HE71827" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kqiQQdfzEe-1u6dpesWcRg" mediniIdentifier="_kqiQQdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kqtPYNfzEe-1u6dpesWcRg" mediniIdentifier="_kqtPYNfzEe-1u6dpesWcRg" id="HE71828" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kqtPYdfzEe-1u6dpesWcRg" mediniIdentifier="_kqtPYdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kq3ncNfzEe-1u6dpesWcRg" mediniIdentifier="_kq3ncNfzEe-1u6dpesWcRg" id="HE71829" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kq3ncdfzEe-1u6dpesWcRg" mediniIdentifier="_kq3ncdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_krB_gNfzEe-1u6dpesWcRg" mediniIdentifier="_krB_gNfzEe-1u6dpesWcRg" id="HE71830" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_krB_gdfzEe-1u6dpesWcRg" mediniIdentifier="_krB_gdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_krMXkNfzEe-1u6dpesWcRg" mediniIdentifier="_krMXkNfzEe-1u6dpesWcRg" id="HE71831" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_krMXkdfzEe-1u6dpesWcRg" mediniIdentifier="_krMXkdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_krWvoNfzEe-1u6dpesWcRg" mediniIdentifier="_krWvoNfzEe-1u6dpesWcRg" id="HE71832" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_krWvodfzEe-1u6dpesWcRg" mediniIdentifier="_krWvodfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_krhuwNfzEe-1u6dpesWcRg" mediniIdentifier="_krhuwNfzEe-1u6dpesWcRg" id="HE71833" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_krhuwdfzEe-1u6dpesWcRg" mediniIdentifier="_krhuwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_krsG0NfzEe-1u6dpesWcRg" mediniIdentifier="_krsG0NfzEe-1u6dpesWcRg" id="HE71834" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_krsG0dfzEe-1u6dpesWcRg" mediniIdentifier="_krsG0dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kr2e4NfzEe-1u6dpesWcRg" mediniIdentifier="_kr2e4NfzEe-1u6dpesWcRg" id="HE71835" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kr2e4dfzEe-1u6dpesWcRg" mediniIdentifier="_kr2e4dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ksA28NfzEe-1u6dpesWcRg" mediniIdentifier="_ksA28NfzEe-1u6dpesWcRg" id="HE71836" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ksA28dfzEe-1u6dpesWcRg" mediniIdentifier="_ksA28dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ksLPANfzEe-1u6dpesWcRg" mediniIdentifier="_ksLPANfzEe-1u6dpesWcRg" id="HE71837" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ksLPAdfzEe-1u6dpesWcRg" mediniIdentifier="_ksLPAdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ksVnENfzEe-1u6dpesWcRg" mediniIdentifier="_ksVnENfzEe-1u6dpesWcRg" id="HE71838" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ksVnEdfzEe-1u6dpesWcRg" mediniIdentifier="_ksVnEdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ksf_INfzEe-1u6dpesWcRg" mediniIdentifier="_ksf_INfzEe-1u6dpesWcRg" id="HE71839" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ksf_IdfzEe-1u6dpesWcRg" mediniIdentifier="_ksf_IdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ksqXMNfzEe-1u6dpesWcRg" mediniIdentifier="_ksqXMNfzEe-1u6dpesWcRg" id="HE71840" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ksqXMdfzEe-1u6dpesWcRg" mediniIdentifier="_ksqXMdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ks0vQNfzEe-1u6dpesWcRg" mediniIdentifier="_ks0vQNfzEe-1u6dpesWcRg" id="HE71841" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ks0vQdfzEe-1u6dpesWcRg" mediniIdentifier="_ks0vQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ks_HUNfzEe-1u6dpesWcRg" mediniIdentifier="_ks_HUNfzEe-1u6dpesWcRg" id="HE71842" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ks_HUdfzEe-1u6dpesWcRg" mediniIdentifier="_ks_HUdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ktJfYNfzEe-1u6dpesWcRg" mediniIdentifier="_ktJfYNfzEe-1u6dpesWcRg" id="HE71843" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ktJfYdfzEe-1u6dpesWcRg" mediniIdentifier="_ktJfYdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ktT3cNfzEe-1u6dpesWcRg" mediniIdentifier="_ktT3cNfzEe-1u6dpesWcRg" id="HE71844" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ktT3cdfzEe-1u6dpesWcRg" mediniIdentifier="_ktT3cdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ktePgNfzEe-1u6dpesWcRg" mediniIdentifier="_ktePgNfzEe-1u6dpesWcRg" id="HE71845" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ktePgdfzEe-1u6dpesWcRg" mediniIdentifier="_ktePgdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ktonkNfzEe-1u6dpesWcRg" mediniIdentifier="_ktonkNfzEe-1u6dpesWcRg" id="HE71846" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ktonkdfzEe-1u6dpesWcRg" mediniIdentifier="_ktonkdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kty_oNfzEe-1u6dpesWcRg" mediniIdentifier="_kty_oNfzEe-1u6dpesWcRg" id="HE71847" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kty_odfzEe-1u6dpesWcRg" mediniIdentifier="_kty_odfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_AD4aUNmREe-CqdlwzOt9UA" mediniIdentifier="_AD4aUNmREe-CqdlwzOt9UA" id="HE72735" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_AD4aUdmREe-CqdlwzOt9UA" mediniIdentifier="_AD4aUdmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_AdplMNmREe-CqdlwzOt9UA" mediniIdentifier="_AdplMNmREe-CqdlwzOt9UA" id="HE72736" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_AdplMdmREe-CqdlwzOt9UA" mediniIdentifier="_AdplMdmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_AqJJENmREe-CqdlwzOt9UA" mediniIdentifier="_AqJJENmREe-CqdlwzOt9UA" id="HE72737" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_AqJJEdmREe-CqdlwzOt9UA" mediniIdentifier="_AqJJEdmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_35RRcII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kt9XsNfzEe-1u6dpesWcRg" mediniIdentifier="_kt9XsNfzEe-1u6dpesWcRg" id="HE71848" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kt9XsdfzEe-1u6dpesWcRg" mediniIdentifier="_kt9XsdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kuHvwNfzEe-1u6dpesWcRg" mediniIdentifier="_kuHvwNfzEe-1u6dpesWcRg" id="HE71849" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kuHvwdfzEe-1u6dpesWcRg" mediniIdentifier="_kuHvwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kuSH0NfzEe-1u6dpesWcRg" mediniIdentifier="_kuSH0NfzEe-1u6dpesWcRg" id="HE71850" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kuSH0dfzEe-1u6dpesWcRg" mediniIdentifier="_kuSH0dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kucf4NfzEe-1u6dpesWcRg" mediniIdentifier="_kucf4NfzEe-1u6dpesWcRg" id="HE71851" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kucf4dfzEe-1u6dpesWcRg" mediniIdentifier="_kucf4dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kum38NfzEe-1u6dpesWcRg" mediniIdentifier="_kum38NfzEe-1u6dpesWcRg" id="HE71852" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kum38dfzEe-1u6dpesWcRg" mediniIdentifier="_kum38dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kuxQANfzEe-1u6dpesWcRg" mediniIdentifier="_kuxQANfzEe-1u6dpesWcRg" id="HE71853" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kuxQAdfzEe-1u6dpesWcRg" mediniIdentifier="_kuxQAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ku7oENfzEe-1u6dpesWcRg" mediniIdentifier="_ku7oENfzEe-1u6dpesWcRg" id="HE71854" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ku7oEdfzEe-1u6dpesWcRg" mediniIdentifier="_ku7oEdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kvGAINfzEe-1u6dpesWcRg" mediniIdentifier="_kvGAINfzEe-1u6dpesWcRg" id="HE71855" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kvGAIdfzEe-1u6dpesWcRg" mediniIdentifier="_kvGAIdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kvPxINfzEe-1u6dpesWcRg" mediniIdentifier="_kvPxINfzEe-1u6dpesWcRg" id="HE71856" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kvPxIdfzEe-1u6dpesWcRg" mediniIdentifier="_kvPxIdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kvaJMNfzEe-1u6dpesWcRg" mediniIdentifier="_kvaJMNfzEe-1u6dpesWcRg" id="HE71857" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kvaJMdfzEe-1u6dpesWcRg" mediniIdentifier="_kvaJMdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kvlIUNfzEe-1u6dpesWcRg" mediniIdentifier="_kvlIUNfzEe-1u6dpesWcRg" id="HE71858" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kvlIUdfzEe-1u6dpesWcRg" mediniIdentifier="_kvlIUdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kvvgYNfzEe-1u6dpesWcRg" mediniIdentifier="_kvvgYNfzEe-1u6dpesWcRg" id="HE71859" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kvvgYdfzEe-1u6dpesWcRg" mediniIdentifier="_kvvgYdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kv54cNfzEe-1u6dpesWcRg" mediniIdentifier="_kv54cNfzEe-1u6dpesWcRg" id="HE71860" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kv54cdfzEe-1u6dpesWcRg" mediniIdentifier="_kv54cdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kwDpcNfzEe-1u6dpesWcRg" mediniIdentifier="_kwDpcNfzEe-1u6dpesWcRg" id="HE71861" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kwDpcdfzEe-1u6dpesWcRg" mediniIdentifier="_kwDpcdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kwOBgNfzEe-1u6dpesWcRg" mediniIdentifier="_kwOBgNfzEe-1u6dpesWcRg" id="HE71862" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kwOBgdfzEe-1u6dpesWcRg" mediniIdentifier="_kwOBgdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kwYZkNfzEe-1u6dpesWcRg" mediniIdentifier="_kwYZkNfzEe-1u6dpesWcRg" id="HE71863" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kwYZkdfzEe-1u6dpesWcRg" mediniIdentifier="_kwYZkdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kwixoNfzEe-1u6dpesWcRg" mediniIdentifier="_kwixoNfzEe-1u6dpesWcRg" id="HE71864" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kwixodfzEe-1u6dpesWcRg" mediniIdentifier="_kwixodfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kwtwwNfzEe-1u6dpesWcRg" mediniIdentifier="_kwtwwNfzEe-1u6dpesWcRg" id="HE71865" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kwtwwdfzEe-1u6dpesWcRg" mediniIdentifier="_kwtwwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kw4I0NfzEe-1u6dpesWcRg" mediniIdentifier="_kw4I0NfzEe-1u6dpesWcRg" id="HE71866" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kw4I0dfzEe-1u6dpesWcRg" mediniIdentifier="_kw4I0dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kxCg4NfzEe-1u6dpesWcRg" mediniIdentifier="_kxCg4NfzEe-1u6dpesWcRg" id="HE71867" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kxCg4dfzEe-1u6dpesWcRg" mediniIdentifier="_kxCg4dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kxM48NfzEe-1u6dpesWcRg" mediniIdentifier="_kxM48NfzEe-1u6dpesWcRg" id="HE71868" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kxM48dfzEe-1u6dpesWcRg" mediniIdentifier="_kxM48dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kxXRANfzEe-1u6dpesWcRg" mediniIdentifier="_kxXRANfzEe-1u6dpesWcRg" id="HE71869" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kxXRAdfzEe-1u6dpesWcRg" mediniIdentifier="_kxXRAdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kxiQINfzEe-1u6dpesWcRg" mediniIdentifier="_kxiQINfzEe-1u6dpesWcRg" id="HE71870" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kxiQIdfzEe-1u6dpesWcRg" mediniIdentifier="_kxiQIdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kxtPQNfzEe-1u6dpesWcRg" mediniIdentifier="_kxtPQNfzEe-1u6dpesWcRg" id="HE71871" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kxtPQdfzEe-1u6dpesWcRg" mediniIdentifier="_kxtPQdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kx3nUNfzEe-1u6dpesWcRg" mediniIdentifier="_kx3nUNfzEe-1u6dpesWcRg" id="HE71872" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kx3nUdfzEe-1u6dpesWcRg" mediniIdentifier="_kx3nUdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kyB_YNfzEe-1u6dpesWcRg" mediniIdentifier="_kyB_YNfzEe-1u6dpesWcRg" id="HE71873" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kyB_YdfzEe-1u6dpesWcRg" mediniIdentifier="_kyB_YdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kyM-gNfzEe-1u6dpesWcRg" mediniIdentifier="_kyM-gNfzEe-1u6dpesWcRg" id="HE71874" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kyM-gdfzEe-1u6dpesWcRg" mediniIdentifier="_kyM-gdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kyXWkNfzEe-1u6dpesWcRg" mediniIdentifier="_kyXWkNfzEe-1u6dpesWcRg" id="HE71875" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kyXWkdfzEe-1u6dpesWcRg" mediniIdentifier="_kyXWkdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_b9PjUNmQEe-CqdlwzOt9UA" mediniIdentifier="_b9PjUNmQEe-CqdlwzOt9UA" id="HE72729" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E1" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_b9PjUdmQEe-CqdlwzOt9UA" mediniIdentifier="_b9PjUdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_cenLANmQEe-CqdlwzOt9UA" mediniIdentifier="_cenLANmQEe-CqdlwzOt9UA" id="HE72730" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_cenLAdmQEe-CqdlwzOt9UA" mediniIdentifier="_cenLAdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c4TdYNmQEe-CqdlwzOt9UA" mediniIdentifier="_c4TdYNmQEe-CqdlwzOt9UA" id="HE72731" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c4TdYdmQEe-CqdlwzOt9UA" mediniIdentifier="_c4TdYdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_xM0AgII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kyhuoNfzEe-1u6dpesWcRg" mediniIdentifier="_kyhuoNfzEe-1u6dpesWcRg" id="HE71876" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kyhuodfzEe-1u6dpesWcRg" mediniIdentifier="_kyhuodfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kysGsNfzEe-1u6dpesWcRg" mediniIdentifier="_kysGsNfzEe-1u6dpesWcRg" id="HE71877" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kysGsdfzEe-1u6dpesWcRg" mediniIdentifier="_kysGsdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ky2ewNfzEe-1u6dpesWcRg" mediniIdentifier="_ky2ewNfzEe-1u6dpesWcRg" id="HE71878" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ky2ewdfzEe-1u6dpesWcRg" mediniIdentifier="_ky2ewdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kzA20NfzEe-1u6dpesWcRg" mediniIdentifier="_kzA20NfzEe-1u6dpesWcRg" id="HE71879" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kzA20dfzEe-1u6dpesWcRg" mediniIdentifier="_kzA20dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kzLO4NfzEe-1u6dpesWcRg" mediniIdentifier="_kzLO4NfzEe-1u6dpesWcRg" id="HE71880" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kzLO4dfzEe-1u6dpesWcRg" mediniIdentifier="_kzLO4dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kzVm8NfzEe-1u6dpesWcRg" mediniIdentifier="_kzVm8NfzEe-1u6dpesWcRg" id="HE71881" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kzVm8dfzEe-1u6dpesWcRg" mediniIdentifier="_kzVm8dfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kzf_ANfzEe-1u6dpesWcRg" mediniIdentifier="_kzf_ANfzEe-1u6dpesWcRg" id="HE71882" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kzf_AdfzEe-1u6dpesWcRg" mediniIdentifier="_kzf_AdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kzpwANfzEe-1u6dpesWcRg" mediniIdentifier="_kzpwANfzEe-1u6dpesWcRg" id="HE71883" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kzpwAdfzEe-1u6dpesWcRg" mediniIdentifier="_kzpwAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kz0IENfzEe-1u6dpesWcRg" mediniIdentifier="_kz0IENfzEe-1u6dpesWcRg" id="HE71884" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kz0IEdfzEe-1u6dpesWcRg" mediniIdentifier="_kz0IEdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_kz-gINfzEe-1u6dpesWcRg" mediniIdentifier="_kz-gINfzEe-1u6dpesWcRg" id="HE71885" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_kz-gIdfzEe-1u6dpesWcRg" mediniIdentifier="_kz-gIdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k0I4MNfzEe-1u6dpesWcRg" mediniIdentifier="_k0I4MNfzEe-1u6dpesWcRg" id="HE71886" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k0I4MdfzEe-1u6dpesWcRg" mediniIdentifier="_k0I4MdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k0TQQNfzEe-1u6dpesWcRg" mediniIdentifier="_k0TQQNfzEe-1u6dpesWcRg" id="HE71887" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k0TQQdfzEe-1u6dpesWcRg" mediniIdentifier="_k0TQQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k0dBQNfzEe-1u6dpesWcRg" mediniIdentifier="_k0dBQNfzEe-1u6dpesWcRg" id="HE71888" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k0dBQdfzEe-1u6dpesWcRg" mediniIdentifier="_k0dBQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k0nZUNfzEe-1u6dpesWcRg" mediniIdentifier="_k0nZUNfzEe-1u6dpesWcRg" id="HE71889" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k0nZUdfzEe-1u6dpesWcRg" mediniIdentifier="_k0nZUdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k0xxYNfzEe-1u6dpesWcRg" mediniIdentifier="_k0xxYNfzEe-1u6dpesWcRg" id="HE71890" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k0xxYdfzEe-1u6dpesWcRg" mediniIdentifier="_k0xxYdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k08JcNfzEe-1u6dpesWcRg" mediniIdentifier="_k08JcNfzEe-1u6dpesWcRg" id="HE71891" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k08JcdfzEe-1u6dpesWcRg" mediniIdentifier="_k08JcdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k1F6cNfzEe-1u6dpesWcRg" mediniIdentifier="_k1F6cNfzEe-1u6dpesWcRg" id="HE71892" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k1F6cdfzEe-1u6dpesWcRg" mediniIdentifier="_k1F6cdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k1QSgNfzEe-1u6dpesWcRg" mediniIdentifier="_k1QSgNfzEe-1u6dpesWcRg" id="HE71893" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k1QSgdfzEe-1u6dpesWcRg" mediniIdentifier="_k1QSgdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k1aqkNfzEe-1u6dpesWcRg" mediniIdentifier="_k1aqkNfzEe-1u6dpesWcRg" id="HE71894" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k1aqkdfzEe-1u6dpesWcRg" mediniIdentifier="_k1aqkdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k1lCoNfzEe-1u6dpesWcRg" mediniIdentifier="_k1lCoNfzEe-1u6dpesWcRg" id="HE71895" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k1lCodfzEe-1u6dpesWcRg" mediniIdentifier="_k1lCodfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k1vasNfzEe-1u6dpesWcRg" mediniIdentifier="_k1vasNfzEe-1u6dpesWcRg" id="HE71896" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k1vasdfzEe-1u6dpesWcRg" mediniIdentifier="_k1vasdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k15ywNfzEe-1u6dpesWcRg" mediniIdentifier="_k15ywNfzEe-1u6dpesWcRg" id="HE71897" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k15ywdfzEe-1u6dpesWcRg" mediniIdentifier="_k15ywdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2DjwNfzEe-1u6dpesWcRg" mediniIdentifier="_k2DjwNfzEe-1u6dpesWcRg" id="HE71898" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2DjwdfzEe-1u6dpesWcRg" mediniIdentifier="_k2DjwdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2N70NfzEe-1u6dpesWcRg" mediniIdentifier="_k2N70NfzEe-1u6dpesWcRg" id="HE71899" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2N70dfzEe-1u6dpesWcRg" mediniIdentifier="_k2N70dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2YT4NfzEe-1u6dpesWcRg" mediniIdentifier="_k2YT4NfzEe-1u6dpesWcRg" id="HE71900" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2YT4dfzEe-1u6dpesWcRg" mediniIdentifier="_k2YT4dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2iE4NfzEe-1u6dpesWcRg" mediniIdentifier="_k2iE4NfzEe-1u6dpesWcRg" id="HE71901" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2iE4dfzEe-1u6dpesWcRg" mediniIdentifier="_k2iE4dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2sc8NfzEe-1u6dpesWcRg" mediniIdentifier="_k2sc8NfzEe-1u6dpesWcRg" id="HE71902" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2sc8dfzEe-1u6dpesWcRg" mediniIdentifier="_k2sc8dfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k2_-8NfzEe-1u6dpesWcRg" mediniIdentifier="_k2_-8NfzEe-1u6dpesWcRg" id="HE71903" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k2_-8dfzEe-1u6dpesWcRg" mediniIdentifier="_k2_-8dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_JG6hENmREe-CqdlwzOt9UA" mediniIdentifier="_JG6hENmREe-CqdlwzOt9UA" id="HE72738" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_JG6hEdmREe-CqdlwzOt9UA" mediniIdentifier="_JG6hEdmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_JwZi8NmREe-CqdlwzOt9UA" mediniIdentifier="_JwZi8NmREe-CqdlwzOt9UA" id="HE72739" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_JwZi8dmREe-CqdlwzOt9UA" mediniIdentifier="_JwZi8dmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_KSYOoNmREe-CqdlwzOt9UA" mediniIdentifier="_KSYOoNmREe-CqdlwzOt9UA" id="HE72740" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_KSYOodmREe-CqdlwzOt9UA" mediniIdentifier="_KSYOodmREe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_5-htwII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_Q5rL4N-pEe-CobyefWie2w"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k3K-ENfzEe-1u6dpesWcRg" mediniIdentifier="_k3K-ENfzEe-1u6dpesWcRg" id="HE71904" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k3K-EdfzEe-1u6dpesWcRg" mediniIdentifier="_k3K-EdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k3WkQNfzEe-1u6dpesWcRg" mediniIdentifier="_k3WkQNfzEe-1u6dpesWcRg" id="HE71905" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k3WkQdfzEe-1u6dpesWcRg" mediniIdentifier="_k3WkQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k3hjYNfzEe-1u6dpesWcRg" mediniIdentifier="_k3hjYNfzEe-1u6dpesWcRg" id="HE71906" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k3hjYdfzEe-1u6dpesWcRg" mediniIdentifier="_k3hjYdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k3sigNfzEe-1u6dpesWcRg" mediniIdentifier="_k3sigNfzEe-1u6dpesWcRg" id="HE71907" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k3sigdfzEe-1u6dpesWcRg" mediniIdentifier="_k3sigdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k33hoNfzEe-1u6dpesWcRg" mediniIdentifier="_k33hoNfzEe-1u6dpesWcRg" id="HE71908" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k33hodfzEe-1u6dpesWcRg" mediniIdentifier="_k33hodfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4DH0NfzEe-1u6dpesWcRg" mediniIdentifier="_k4DH0NfzEe-1u6dpesWcRg" id="HE71909" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4DH0dfzEe-1u6dpesWcRg" mediniIdentifier="_k4DH0dfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4Nf4NfzEe-1u6dpesWcRg" mediniIdentifier="_k4Nf4NfzEe-1u6dpesWcRg" id="HE71910" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4Nf4dfzEe-1u6dpesWcRg" mediniIdentifier="_k4Nf4dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4YfANfzEe-1u6dpesWcRg" mediniIdentifier="_k4YfANfzEe-1u6dpesWcRg" id="HE71911" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4YfAdfzEe-1u6dpesWcRg" mediniIdentifier="_k4YfAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4jeINfzEe-1u6dpesWcRg" mediniIdentifier="_k4jeINfzEe-1u6dpesWcRg" id="HE71912" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4jeIdfzEe-1u6dpesWcRg" mediniIdentifier="_k4jeIdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4udQNfzEe-1u6dpesWcRg" mediniIdentifier="_k4udQNfzEe-1u6dpesWcRg" id="HE71913" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4udQdfzEe-1u6dpesWcRg" mediniIdentifier="_k4udQdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k4_jANfzEe-1u6dpesWcRg" mediniIdentifier="_k4_jANfzEe-1u6dpesWcRg" id="HE71914" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k4_jAdfzEe-1u6dpesWcRg" mediniIdentifier="_k4_jAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k5KiINfzEe-1u6dpesWcRg" mediniIdentifier="_k5KiINfzEe-1u6dpesWcRg" id="HE71915" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k5KiIdfzEe-1u6dpesWcRg" mediniIdentifier="_k5KiIdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k5U6MNfzEe-1u6dpesWcRg" mediniIdentifier="_k5U6MNfzEe-1u6dpesWcRg" id="HE71916" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k5U6MdfzEe-1u6dpesWcRg" mediniIdentifier="_k5U6MdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k5fSQNfzEe-1u6dpesWcRg" mediniIdentifier="_k5fSQNfzEe-1u6dpesWcRg" id="HE71917" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k5fSQdfzEe-1u6dpesWcRg" mediniIdentifier="_k5fSQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k5pqUNfzEe-1u6dpesWcRg" mediniIdentifier="_k5pqUNfzEe-1u6dpesWcRg" id="HE71918" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k5pqUdfzEe-1u6dpesWcRg" mediniIdentifier="_k5pqUdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k50CYNfzEe-1u6dpesWcRg" mediniIdentifier="_k50CYNfzEe-1u6dpesWcRg" id="HE71919" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k50CYdfzEe-1u6dpesWcRg" mediniIdentifier="_k50CYdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k5_BgNfzEe-1u6dpesWcRg" mediniIdentifier="_k5_BgNfzEe-1u6dpesWcRg" id="HE71920" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k5_BgdfzEe-1u6dpesWcRg" mediniIdentifier="_k5_BgdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k6JZkNfzEe-1u6dpesWcRg" mediniIdentifier="_k6JZkNfzEe-1u6dpesWcRg" id="HE71921" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k6JZkdfzEe-1u6dpesWcRg" mediniIdentifier="_k6JZkdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k6TxoNfzEe-1u6dpesWcRg" mediniIdentifier="_k6TxoNfzEe-1u6dpesWcRg" id="HE71922" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k6TxodfzEe-1u6dpesWcRg" mediniIdentifier="_k6TxodfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k6eJsNfzEe-1u6dpesWcRg" mediniIdentifier="_k6eJsNfzEe-1u6dpesWcRg" id="HE71923" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k6eJsdfzEe-1u6dpesWcRg" mediniIdentifier="_k6eJsdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k6ohwNfzEe-1u6dpesWcRg" mediniIdentifier="_k6ohwNfzEe-1u6dpesWcRg" id="HE71924" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k6ohwdfzEe-1u6dpesWcRg" mediniIdentifier="_k6ohwdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k6ySwNfzEe-1u6dpesWcRg" mediniIdentifier="_k6ySwNfzEe-1u6dpesWcRg" id="HE71925" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k6ySwdfzEe-1u6dpesWcRg" mediniIdentifier="_k6ySwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k68q0NfzEe-1u6dpesWcRg" mediniIdentifier="_k68q0NfzEe-1u6dpesWcRg" id="HE71926" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k68q0dfzEe-1u6dpesWcRg" mediniIdentifier="_k68q0dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k7HC4NfzEe-1u6dpesWcRg" mediniIdentifier="_k7HC4NfzEe-1u6dpesWcRg" id="HE71927" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k7HC4dfzEe-1u6dpesWcRg" mediniIdentifier="_k7HC4dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k7Ra8NfzEe-1u6dpesWcRg" mediniIdentifier="_k7Ra8NfzEe-1u6dpesWcRg" id="HE71928" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k7Ra8dfzEe-1u6dpesWcRg" mediniIdentifier="_k7Ra8dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k7bzANfzEe-1u6dpesWcRg" mediniIdentifier="_k7bzANfzEe-1u6dpesWcRg" id="HE71929" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k7bzAdfzEe-1u6dpesWcRg" mediniIdentifier="_k7bzAdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k7mLENfzEe-1u6dpesWcRg" mediniIdentifier="_k7mLENfzEe-1u6dpesWcRg" id="HE71930" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k7mLEdfzEe-1u6dpesWcRg" mediniIdentifier="_k7mLEdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k7wjINfzEe-1u6dpesWcRg" mediniIdentifier="_k7wjINfzEe-1u6dpesWcRg" id="HE71931" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k7wjIdfzEe-1u6dpesWcRg" mediniIdentifier="_k7wjIdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_xVQpwNmQEe-CqdlwzOt9UA" mediniIdentifier="_xVQpwNmQEe-CqdlwzOt9UA" id="HE72732" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E1" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_xVQpwdmQEe-CqdlwzOt9UA" mediniIdentifier="_xVQpwdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_x-fM8NmQEe-CqdlwzOt9UA" mediniIdentifier="_x-fM8NmQEe-CqdlwzOt9UA" id="HE72733" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible while existing the vehicle during emergency." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_x-fM8dmQEe-CqdlwzOt9UA" mediniIdentifier="_x-fM8dmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_yV2kENmQEe-CqdlwzOt9UA" mediniIdentifier="_yV2kENmQEe-CqdlwzOt9UA" id="HE72734" ISO26262_severity="S2" ISO26262_severityComment="Severe Injury possible due to fire and toxic gas inhalation." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yGBSQIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_yV2kEdmQEe-CqdlwzOt9UA" mediniIdentifier="_yV2kEdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_1W8eoII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k767MNfzEe-1u6dpesWcRg" mediniIdentifier="_k767MNfzEe-1u6dpesWcRg" id="HE71932" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k767MdfzEe-1u6dpesWcRg" mediniIdentifier="_k767MdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k8FTQNfzEe-1u6dpesWcRg" mediniIdentifier="_k8FTQNfzEe-1u6dpesWcRg" id="HE71933" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k8FTQdfzEe-1u6dpesWcRg" mediniIdentifier="_k8FTQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k8PrUNfzEe-1u6dpesWcRg" mediniIdentifier="_k8PrUNfzEe-1u6dpesWcRg" id="HE71934" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k8PrUdfzEe-1u6dpesWcRg" mediniIdentifier="_k8PrUdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k8aDYNfzEe-1u6dpesWcRg" mediniIdentifier="_k8aDYNfzEe-1u6dpesWcRg" id="HE71935" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k8aDYdfzEe-1u6dpesWcRg" mediniIdentifier="_k8aDYdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k8j0YNfzEe-1u6dpesWcRg" mediniIdentifier="_k8j0YNfzEe-1u6dpesWcRg" id="HE71936" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k8j0YdfzEe-1u6dpesWcRg" mediniIdentifier="_k8j0YdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k8uMcNfzEe-1u6dpesWcRg" mediniIdentifier="_k8uMcNfzEe-1u6dpesWcRg" id="HE71937" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k8uMcdfzEe-1u6dpesWcRg" mediniIdentifier="_k8uMcdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k84kgNfzEe-1u6dpesWcRg" mediniIdentifier="_k84kgNfzEe-1u6dpesWcRg" id="HE71938" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k84kgdfzEe-1u6dpesWcRg" mediniIdentifier="_k84kgdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9C8kNfzEe-1u6dpesWcRg" mediniIdentifier="_k9C8kNfzEe-1u6dpesWcRg" id="HE71939" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9C8kdfzEe-1u6dpesWcRg" mediniIdentifier="_k9C8kdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9NUoNfzEe-1u6dpesWcRg" mediniIdentifier="_k9NUoNfzEe-1u6dpesWcRg" id="HE71940" ISO26262_severity="S2" ISO26262_severityComment="The severity is high due to the potential for a collision with other high-speed moving vehicles, leading to catastrophic consequences." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C2" ISO26262_controllabilityComment="Under power loss conditions at high speed is difficult to control and the driver will face difficulty in maneuvering to halt the vehicle " user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9NUodfzEe-1u6dpesWcRg" mediniIdentifier="_k9NUodfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9XssNfzEe-1u6dpesWcRg" mediniIdentifier="_k9XssNfzEe-1u6dpesWcRg" id="HE71941" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9XssdfzEe-1u6dpesWcRg" mediniIdentifier="_k9XssdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9iEwNfzEe-1u6dpesWcRg" mediniIdentifier="_k9iEwNfzEe-1u6dpesWcRg" id="HE71942" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9iEwdfzEe-1u6dpesWcRg" mediniIdentifier="_k9iEwdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9sc0NfzEe-1u6dpesWcRg" mediniIdentifier="_k9sc0NfzEe-1u6dpesWcRg" id="HE71943" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9sc0dfzEe-1u6dpesWcRg" mediniIdentifier="_k9sc0dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k9204NfzEe-1u6dpesWcRg" mediniIdentifier="_k9204NfzEe-1u6dpesWcRg" id="HE71944" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k9204dfzEe-1u6dpesWcRg" mediniIdentifier="_k9204dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-BM8NfzEe-1u6dpesWcRg" mediniIdentifier="_k-BM8NfzEe-1u6dpesWcRg" id="HE71945" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-BM8dfzEe-1u6dpesWcRg" mediniIdentifier="_k-BM8dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-LlANfzEe-1u6dpesWcRg" mediniIdentifier="_k-LlANfzEe-1u6dpesWcRg" id="HE71946" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-LlAdfzEe-1u6dpesWcRg" mediniIdentifier="_k-LlAdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-VWANfzEe-1u6dpesWcRg" mediniIdentifier="_k-VWANfzEe-1u6dpesWcRg" id="HE71947" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-VWAdfzEe-1u6dpesWcRg" mediniIdentifier="_k-VWAdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-fuENfzEe-1u6dpesWcRg" mediniIdentifier="_k-fuENfzEe-1u6dpesWcRg" id="HE71948" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-fuEdfzEe-1u6dpesWcRg" mediniIdentifier="_k-fuEdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-qGINfzEe-1u6dpesWcRg" mediniIdentifier="_k-qGINfzEe-1u6dpesWcRg" id="HE71949" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-qGIdfzEe-1u6dpesWcRg" mediniIdentifier="_k-qGIdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k-0eMNfzEe-1u6dpesWcRg" mediniIdentifier="_k-0eMNfzEe-1u6dpesWcRg" id="HE71950" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k-0eMdfzEe-1u6dpesWcRg" mediniIdentifier="_k-0eMdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k--PMNfzEe-1u6dpesWcRg" mediniIdentifier="_k--PMNfzEe-1u6dpesWcRg" id="HE71951" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k--PMdfzEe-1u6dpesWcRg" mediniIdentifier="_k--PMdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_InQNfzEe-1u6dpesWcRg" mediniIdentifier="_k_InQNfzEe-1u6dpesWcRg" id="HE71952" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_InQdfzEe-1u6dpesWcRg" mediniIdentifier="_k_InQdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_S_UNfzEe-1u6dpesWcRg" mediniIdentifier="_k_S_UNfzEe-1u6dpesWcRg" id="HE71953" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_86TUMIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_S_UdfzEe-1u6dpesWcRg" mediniIdentifier="_k_S_UdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_dXYNfzEe-1u6dpesWcRg" mediniIdentifier="_k_dXYNfzEe-1u6dpesWcRg" id="HE71954" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_dXYdfzEe-1u6dpesWcRg" mediniIdentifier="_k_dXYdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_oWgNfzEe-1u6dpesWcRg" mediniIdentifier="_k_oWgNfzEe-1u6dpesWcRg" id="HE71955" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_oWgdfzEe-1u6dpesWcRg" mediniIdentifier="_k_oWgdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_yukNfzEe-1u6dpesWcRg" mediniIdentifier="_k_yukNfzEe-1u6dpesWcRg" id="HE71956" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_yukdfzEe-1u6dpesWcRg" mediniIdentifier="_k_yukdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_k_9tsNfzEe-1u6dpesWcRg" mediniIdentifier="_k_9tsNfzEe-1u6dpesWcRg" id="HE71957" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_k_9tsdfzEe-1u6dpesWcRg" mediniIdentifier="_k_9tsdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lAIFwNfzEe-1u6dpesWcRg" mediniIdentifier="_lAIFwNfzEe-1u6dpesWcRg" id="HE71958" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lAIFwdfzEe-1u6dpesWcRg" mediniIdentifier="_lAIFwdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lATE4NfzEe-1u6dpesWcRg" mediniIdentifier="_lATE4NfzEe-1u6dpesWcRg" id="HE71959" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lATE4dfzEe-1u6dpesWcRg" mediniIdentifier="_lATE4dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_HeJB4NmQEe-CqdlwzOt9UA" mediniIdentifier="_HeJB4NmQEe-CqdlwzOt9UA" id="HE72726" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_HeJB4dmQEe-CqdlwzOt9UA" mediniIdentifier="_HeJB4dmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Jnc3wNmQEe-CqdlwzOt9UA" mediniIdentifier="_Jnc3wNmQEe-CqdlwzOt9UA" id="HE72727" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Normally Controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Jnc3wdmQEe-CqdlwzOt9UA" mediniIdentifier="_Jnc3wdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_KDNmsNmQEe-CqdlwzOt9UA" mediniIdentifier="_KDNmsNmQEe-CqdlwzOt9UA" id="HE72728" ISO26262_severity="S1" ISO26262_severityComment="Minor injuries possible due to sudden braking." ISO26262_exposure="E2" ISO26262_controllability="C1" ISO26262_controllabilityComment="Under power loss conditions, the driver can safely maneuver and halt the vehicle without significant difficulty." user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_84QFwIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_KDNmsdmQEe-CqdlwzOt9UA" mediniIdentifier="_KDNmsdmQEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_phHgIII9Ee-aNNVRVoOGvw"/>
    <user_accident_type>car2car collision (general)</user_accident_type>
    <user_accident_type>car2car collision head-to-rear</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lAdc8NfzEe-1u6dpesWcRg" mediniIdentifier="_lAdc8NfzEe-1u6dpesWcRg" id="HE71960" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lAdc8dfzEe-1u6dpesWcRg" mediniIdentifier="_lAdc8dfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8Jb0NfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lAocENfzEe-1u6dpesWcRg" mediniIdentifier="_lAocENfzEe-1u6dpesWcRg" id="HE71961" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lAocEdfzEe-1u6dpesWcRg" mediniIdentifier="_lAocEdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDAdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lAy0INfzEe-1u6dpesWcRg" mediniIdentifier="_lAy0INfzEe-1u6dpesWcRg" id="HE71962" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands&#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lAy0IdfzEe-1u6dpesWcRg" mediniIdentifier="_lAy0IdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDD9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lA9zQNfzEe-1u6dpesWcRg" mediniIdentifier="_lA9zQNfzEe-1u6dpesWcRg" id="HE71963" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver Sleeping &#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lA9zQdfzEe-1u6dpesWcRg" mediniIdentifier="_lA9zQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDFdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lBIyYNfzEe-1u6dpesWcRg" mediniIdentifier="_lBIyYNfzEe-1u6dpesWcRg" id="HE71964" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lBIyYdfzEe-1u6dpesWcRg" mediniIdentifier="_lBIyYdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC99fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lBTKcNfzEe-1u6dpesWcRg" mediniIdentifier="_lBTKcNfzEe-1u6dpesWcRg" id="HE71965" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lBTKcdfzEe-1u6dpesWcRg" mediniIdentifier="_lBTKcdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDC9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lBeJkNfzEe-1u6dpesWcRg" mediniIdentifier="_lBeJkNfzEe-1u6dpesWcRg" id="HE71966" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lBeJkdfzEe-1u6dpesWcRg" mediniIdentifier="_lBeJkdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC59fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lBohoNfzEe-1u6dpesWcRg" mediniIdentifier="_lBohoNfzEe-1u6dpesWcRg" id="HE71967" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lBohodfzEe-1u6dpesWcRg" mediniIdentifier="_lBohodfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lBzgwNfzEe-1u6dpesWcRg" mediniIdentifier="_lBzgwNfzEe-1u6dpesWcRg" id="HE71968" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lBzgwdfzEe-1u6dpesWcRg" mediniIdentifier="_lBzgwdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="High vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lB-f4NfzEe-1u6dpesWcRg" mediniIdentifier="_lB-f4NfzEe-1u6dpesWcRg" id="HE71969" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lB-f4dfzEe-1u6dpesWcRg" mediniIdentifier="_lB-f4dfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDCdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lCJfANfzEe-1u6dpesWcRg" mediniIdentifier="_lCJfANfzEe-1u6dpesWcRg" id="HE71970" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lCJfAdfzEe-1u6dpesWcRg" mediniIdentifier="_lCJfAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDB9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lCT3ENfzEe-1u6dpesWcRg" mediniIdentifier="_lCT3ENfzEe-1u6dpesWcRg" id="HE71971" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lCT3EdfzEe-1u6dpesWcRg" mediniIdentifier="_lCT3EdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC4dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lCe2MNfzEe-1u6dpesWcRg" mediniIdentifier="_lCe2MNfzEe-1u6dpesWcRg" id="HE71972" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lCe2MdfzEe-1u6dpesWcRg" mediniIdentifier="_lCe2MdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDE9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lCpOQNfzEe-1u6dpesWcRg" mediniIdentifier="_lCpOQNfzEe-1u6dpesWcRg" id="HE71973" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Driver/Conductor Sleeping Overnight &#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lCpOQdfzEe-1u6dpesWcRg" mediniIdentifier="_lCpOQdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDDdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lCzmUNfzEe-1u6dpesWcRg" mediniIdentifier="_lCzmUNfzEe-1u6dpesWcRg" id="HE71974" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lCzmUdfzEe-1u6dpesWcRg" mediniIdentifier="_lCzmUdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC89fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lC9-YNfzEe-1u6dpesWcRg" mediniIdentifier="_lC9-YNfzEe-1u6dpesWcRg" id="HE71975" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lC9-YdfzEe-1u6dpesWcRg" mediniIdentifier="_lC9-YdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC9dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lDIWcNfzEe-1u6dpesWcRg" mediniIdentifier="_lDIWcNfzEe-1u6dpesWcRg" id="HE71976" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lDIWcdfzEe-1u6dpesWcRg" mediniIdentifier="_lDIWcdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC7dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lDSugNfzEe-1u6dpesWcRg" mediniIdentifier="_lDSugNfzEe-1u6dpesWcRg" id="HE71977" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People Sleeping while bus is in Bus Stands&#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lDSugdfzEe-1u6dpesWcRg" mediniIdentifier="_lDSugdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDEdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lDcfgNfzEe-1u6dpesWcRg" mediniIdentifier="_lDcfgNfzEe-1u6dpesWcRg" id="HE71978" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lDcfgdfzEe-1u6dpesWcRg" mediniIdentifier="_lDcfgdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC79fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lDneoNfzEe-1u6dpesWcRg" mediniIdentifier="_lDneoNfzEe-1u6dpesWcRg" id="HE71979" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lDneodfzEe-1u6dpesWcRg" mediniIdentifier="_lDneodfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E1" ISO26262_defaultExposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDA9fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lDx2sNfzEe-1u6dpesWcRg" mediniIdentifier="_lDx2sNfzEe-1u6dpesWcRg" id="HE71980" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lDx2sdfzEe-1u6dpesWcRg" mediniIdentifier="_lDx2sdfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC8dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lD8OwNfzEe-1u6dpesWcRg" mediniIdentifier="_lD8OwNfzEe-1u6dpesWcRg" id="HE71981" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="People might sleep while charging &#xD;&#xA;It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lD8OwdfzEe-1u6dpesWcRg" mediniIdentifier="_lD8OwdfzEe-1u6dpesWcRg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC49fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lEGm0NfzEe-1u6dpesWcRg" mediniIdentifier="_lEGm0NfzEe-1u6dpesWcRg" id="HE71982" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lEGm0dfzEe-1u6dpesWcRg" mediniIdentifier="_lEGm0dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC6dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lEQX0NfzEe-1u6dpesWcRg" mediniIdentifier="_lEQX0NfzEe-1u6dpesWcRg" id="HE71983" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lEQX0dfzEe-1u6dpesWcRg" mediniIdentifier="_lEQX0dfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC69fCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lEav4NfzEe-1u6dpesWcRg" mediniIdentifier="_lEav4NfzEe-1u6dpesWcRg" id="HE71984" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lEav4dfzEe-1u6dpesWcRg" mediniIdentifier="_lEav4dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_speed="Low vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC_dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lElH8NfzEe-1u6dpesWcRg" mediniIdentifier="_lElH8NfzEe-1u6dpesWcRg" id="HE71985" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lElH8dfzEe-1u6dpesWcRg" mediniIdentifier="_lElH8dfzEe-1u6dpesWcRg" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC-dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lEvgANfzEe-1u6dpesWcRg" mediniIdentifier="_lEvgANfzEe-1u6dpesWcRg" id="HE71986" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lEvgAdfzEe-1u6dpesWcRg" mediniIdentifier="_lEvgAdfzEe-1u6dpesWcRg" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KDBdfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lE54ENfzEe-1u6dpesWcRg" mediniIdentifier="_lE54ENfzEe-1u6dpesWcRg" id="HE71987" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lE54EdfzEe-1u6dpesWcRg" mediniIdentifier="_lE54EdfzEe-1u6dpesWcRg" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_speed="Any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <template href="../commons/_JbMG4NMNEe-Sld_1EWpoOA.ha#_t8KC5dfCEe-7fd93EIJ22A"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_DDClANmPEe-CqdlwzOt9UA" mediniIdentifier="_DDClANmPEe-CqdlwzOt9UA" id="HE72723" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E1" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_DDClAdmPEe-CqdlwzOt9UA" mediniIdentifier="_DDClAdmPEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="No Occupant" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_Dtvu4NmPEe-CqdlwzOt9UA" mediniIdentifier="_Dtvu4NmPEe-CqdlwzOt9UA" id="HE72724" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_Dtvu4dmPEe-CqdlwzOt9UA" mediniIdentifier="_Dtvu4dmPEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_EIFhgNmPEe-CqdlwzOt9UA" mediniIdentifier="_EIFhgNmPEe-CqdlwzOt9UA" id="HE72725" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience, no impact on functionality." ISO26262_exposure="E2" ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="It is assumed that dual failures doesn't happen.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_yT6kUIx2Ee-lk9Yz7i8Jsg"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_EIFhgdmPEe-CqdlwzOt9UA" mediniIdentifier="_EIFhgdmPEe-CqdlwzOt9UA" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low temperature " ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="any vehicle speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_WE9CYII9Ee-aNNVRVoOGvw"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_D4I2sKM5Ee-cWLxwEtuALg"/>
    <user_accident_type>no accident</user_accident_type>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
