<?xml version="1.1" encoding="UTF-8"?>
<de.ikv.analyze.checklist:Checklist xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:de.ikv.analyze.checklist="http:///de/ikv/analyze/checklist.ecore" xmi:id="_kgSncJSmEeefbsnFgah_5Q" mediniIdentifier="_kgSncJSmEeefbsnFgah_5Q" name="Checklist: Dependent Failure Analysis (ISO26262-2nd Ed.:Part9 Annex C)" version="25/08/2017 15:13">
  <items xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgSncZSmEeefbsnFgah_5Q" mediniIdentifier="_kgSncZSmEeefbsnFgah_5Q" name="Coupling Factor Class">
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgYHAJSmEeefbsnFgah_5Q" mediniIdentifier="_kgYHAJSmEeefbsnFgah_5Q" name="System-level" user_Description="">
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgWR0JSmEeefbsnFgah_5Q" mediniIdentifier="_kgWR0JSmEeefbsnFgah_5Q" name="Shared Resources" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;g) failures of common external resources&#xD;&#xA;&#xD;&#xA;The same software, hardware, or system element instance used by the two elements which are therefore affected by the failure or unavailability of that shared resource, i.e. from a physical perspective.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_CJR3kMGMEeimSKDM1drJhw" mediniIdentifier="_CJR3kMGMEeimSKDM1drJhw" name="Shared Power Supply" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_GoktYMGMEeimSKDM1drJhw" mediniIdentifier="_GoktYMGMEeimSKDM1drJhw" name="Wiring harness" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Sfxk4MGMEeimSKDM1drJhw" mediniIdentifier="_Sfxk4MGMEeimSKDM1drJhw" name="Data and Communication busses" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_5Dap0MGMEeimSKDM1drJhw" mediniIdentifier="_5Dap0MGMEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_EfGvAMipEeiciPcxq-kTYA" mediniIdentifier="_EfGvAMipEeiciPcxq-kTYA" name="Shared Information Inputs" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;&#xD;&#xA;Same information consumed by the two functions even in absence of shared resources, i.e. from a functional perspective">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_PTUagMGNEeimSKDM1drJhw" mediniIdentifier="_PTUagMGNEeimSKDM1drJhw" name="External messages" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_TlxuMMGNEeimSKDM1drJhw" mediniIdentifier="_TlxuMMGNEeimSKDM1drJhw" name="External physical signals" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_V8RrgMGNEeimSKDM1drJhw" mediniIdentifier="_V8RrgMGNEeimSKDM1drJhw" name="Readings detected by capacitive/radar/optical sensors" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_aNb-sMGNEeimSKDM1drJhw" mediniIdentifier="_aNb-sMGNEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kge0sJSmEeefbsnFgah_5Q" mediniIdentifier="_kge0sJSmEeefbsnFgah_5Q" name="Insufficient Environmental Immunity" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;f) environmental factors&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Common external environmental disturbance affects both functions">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_EwnbUMGOEeimSKDM1drJhw" mediniIdentifier="_EwnbUMGOEeimSKDM1drJhw" name="Mechanical Coupling" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_ZaNVgMGOEeimSKDM1drJhw" mediniIdentifier="_ZaNVgMGOEeimSKDM1drJhw" name="Water Ingress" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_cZNdQMGOEeimSKDM1drJhw" mediniIdentifier="_cZNdQMGOEeimSKDM1drJhw" name="Flammable Material" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_fLO48MGOEeimSKDM1drJhw" mediniIdentifier="_fLO48MGOEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgkUQJSmEeefbsnFgah_5Q" mediniIdentifier="_kgkUQJSmEeefbsnFgah_5Q" name="Systematic Coupling" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;b) development faults&#xD;&#xA;c) manufacturing faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Failure of both elements due to a common systematic human or tool error">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_uk-0sMGPEeimSKDM1drJhw" mediniIdentifier="_uk-0sMGPEeimSKDM1drJhw" name="Identical production processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_wzzcsMGPEeimSKDM1drJhw" mediniIdentifier="_wzzcsMGPEeimSKDM1drJhw" name="Identical repair processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_zQfhkMGPEeimSKDM1drJhw" mediniIdentifier="_zQfhkMGPEeimSKDM1drJhw" name="Identical repair processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_z7HL4MGPEeimSKDM1drJhw" mediniIdentifier="_z7HL4MGPEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgpz0JSmEeefbsnFgah_5Q" mediniIdentifier="_kgpz0JSmEeefbsnFgah_5Q" name="Components of Identical Type" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;&#xD;&#xA;Identical components may fail with a probability higher than expected due to a common cause failure.&#xD;&#xA;Two functions both use a software, hardware, or system element instance of the same type. If these element instances both fail due to a common mode failure, both functions are affected.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2BQjkMGQEeimSKDM1drJhw" mediniIdentifier="_2BQjkMGQEeimSKDM1drJhw" name="Same type of actuator/power stage e.g. motor" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_4S4A4MGQEeimSKDM1drJhw" mediniIdentifier="_4S4A4MGQEeimSKDM1drJhw" name="Same type of sensors" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_7YS5sMGQEeimSKDM1drJhw" mediniIdentifier="_7YS5sMGQEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kguFQJSmEeefbsnFgah_5Q" mediniIdentifier="_kguFQJSmEeefbsnFgah_5Q" name="Communication" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;i) ageing and wear&#xD;&#xA;&#xD;&#xA;The receiving element is affected by information that is false,  lost, sent multiple times, or in the wrong order, etc. from the sender.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_rABOQMGREeimSKDM1drJhw" mediniIdentifier="_rABOQMGREeimSKDM1drJhw" name="Failure of the application or protocol layer of the communication" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_xO6ZcMGREeimSKDM1drJhw" mediniIdentifier="_xO6ZcMGREeimSKDM1drJhw" name="CAN connection between two ECUs of the same system" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_yoZ78MGREeimSKDM1drJhw" mediniIdentifier="_yoZ78MGREeimSKDM1drJhw" name="Communication between two microcontrollers within the same ECU" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_z32KkMGREeimSKDM1drJhw" mediniIdentifier="_z32KkMGREeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgyWsJSmEeefbsnFgah_5Q" mediniIdentifier="_kgyWsJSmEeefbsnFgah_5Q" name="Unintended Interface" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Two elements affecting each other directly via an unanticipated interface, or with unanticipated effects.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Xg_NQMGSEeimSKDM1drJhw" mediniIdentifier="_Xg_NQMGSEeimSKDM1drJhw" name="Thermal impact of one actuator to the other" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_ZNvqAMGSEeimSKDM1drJhw" mediniIdentifier="_ZNvqAMGSEeimSKDM1drJhw" name="One functionality overruling the other because of missing synchronization" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_a3l8sMGSEeimSKDM1drJhw" mediniIdentifier="_a3l8sMGSEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
    </subItems>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgYuEJSmEeefbsnFgah_5Q" mediniIdentifier="_kgYuEJSmEeefbsnFgah_5Q" name="Software-level">
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_bCy7MMilEeiciPcxq-kTYA" mediniIdentifier="_bCy7MMilEeiciPcxq-kTYA" name="Shared Resources" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;g) failures of common external resources&#xD;&#xA;&#xD;&#xA;The same software, hardware, or system element instance used by the two elements which are therefore affected by the failure or unavailability of that shared resource, i.e. from a physical perspective.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_apTQwMGMEeimSKDM1drJhw" mediniIdentifier="_apTQwMGMEeimSKDM1drJhw" name="SW component used by  other SW component" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_hFAv8MGMEeimSKDM1drJhw" mediniIdentifier="_hFAv8MGMEeimSKDM1drJhw" name="Shared Libraries or maths" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kwva0MGMEeimSKDM1drJhw" mediniIdentifier="_kwva0MGMEeimSKDM1drJhw" name="Shared I/O routines, drivers" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_pDtE0MGMEeimSKDM1drJhw" mediniIdentifier="_pDtE0MGMEeimSKDM1drJhw" name="Shared Hardware resource" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_7s2xQMGMEeimSKDM1drJhw" mediniIdentifier="_7s2xQMGMEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_EWj3AMipEeiciPcxq-kTYA" mediniIdentifier="_EWj3AMipEeiciPcxq-kTYA" name="Shared Information Inputs" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;&#xD;&#xA;Same information consumed by the two functions even in absence of shared resources, i.e. from a functional perspective">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_cn_8oMGNEeimSKDM1drJhw" mediniIdentifier="_cn_8oMGNEeimSKDM1drJhw" name="Constants, or variables, being global to the invesitigated elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_jstVgMGNEeimSKDM1drJhw" mediniIdentifier="_jstVgMGNEeimSKDM1drJhw" name="Data/function parameter arguments/messages shared by investigated elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_rQHckMGNEeimSKDM1drJhw" mediniIdentifier="_rQHckMGNEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_D4DOsMisEeiciPcxq-kTYA" mediniIdentifier="_D4DOsMisEeiciPcxq-kTYA" name="Systematic Coupling" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;b) development faults&#xD;&#xA;c) manufacturing faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Failure of both elements due to a common systematic human or tool error">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_clDEYMGPEeimSKDM1drJhw" mediniIdentifier="_clDEYMGPEeimSKDM1drJhw" name="Same software tools e.g. IDE, compiler, linker, software configurator" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_fD7hoMGPEeimSKDM1drJhw" mediniIdentifier="_fD7hoMGPEeimSKDM1drJhw" name="Same programming and/or modelling language" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_hA_EMMGPEeimSKDM1drJhw" mediniIdentifier="_hA_EMMGPEeimSKDM1drJhw" name="Same compiler/linker" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kBzw4MGPEeimSKDM1drJhw" mediniIdentifier="_kBzw4MGPEeimSKDM1drJhw" name="Same algorithms" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_nbiFwMGPEeimSKDM1drJhw" mediniIdentifier="_nbiFwMGPEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Y23yAMisEeiciPcxq-kTYA" mediniIdentifier="_Y23yAMisEeiciPcxq-kTYA" name="Components of Identical Type" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;&#xD;&#xA;Identical components may fail with a probability higher than expected due to a common cause failure.&#xD;&#xA;Two functions both use a software, hardware, or system element instance of the same type. If these element instances both fail due to a common mode failure, both functions are affected.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_9t6GMMGQEeimSKDM1drJhw" mediniIdentifier="_9t6GMMGQEeimSKDM1drJhw" name="Same source code expanded twice, e.g. by usage of C macros" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_EQ6gMMGREeimSKDM1drJhw" mediniIdentifier="_EQ6gMMGREeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_-fFJcMisEeiciPcxq-kTYA" mediniIdentifier="_-fFJcMisEeiciPcxq-kTYA" name="Communication" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;i) ageing and wear&#xD;&#xA;&#xD;&#xA;The receiving element is affected by information that is false, lost, sent multiple times, or in the wrong order, etc. from the sender.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2tPDUMGREeimSKDM1drJhw" mediniIdentifier="_2tPDUMGREeimSKDM1drJhw" name="Data flow via global variables" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_4S1IIMGREeimSKDM1drJhw" mediniIdentifier="_4S1IIMGREeimSKDM1drJhw" name="Messaging" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_6D3A4MGREeimSKDM1drJhw" mediniIdentifier="_6D3A4MGREeimSKDM1drJhw" name="Function calls with arguments passed" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_7UUjMMGREeimSKDM1drJhw" mediniIdentifier="_7UUjMMGREeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_O5gfEMiuEeiciPcxq-kTYA" mediniIdentifier="_O5gfEMiuEeiciPcxq-kTYA" name="Unintended Interface" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Two elements affecting each other directly via an unanticipated interface, or with unanticipated effects.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_fVfrYMGSEeimSKDM1drJhw" mediniIdentifier="_fVfrYMGSEeimSKDM1drJhw" name="Same memory space which means a potential of wrong memory allocation or memory leaks" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_gXWxAMGSEeimSKDM1drJhw" mediniIdentifier="_gXWxAMGSEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
    </subItems>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgYuEZSmEeefbsnFgah_5Q" mediniIdentifier="_kgYuEZSmEeefbsnFgah_5Q" name="Hardware-level">
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_bI7_cMilEeiciPcxq-kTYA" mediniIdentifier="_bI7_cMilEeiciPcxq-kTYA" name="Shared Resources" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;g) failures of common external resources&#xD;&#xA;&#xD;&#xA;The same software, hardware, or system element instance used by the two elements which are therefore affected by the failure or unavailability of that shared resource, i.e. from a physical perspective.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_t9Sp8MGMEeimSKDM1drJhw" mediniIdentifier="_t9Sp8MGMEeimSKDM1drJhw" name="Common clock" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_ziXcEMGMEeimSKDM1drJhw" mediniIdentifier="_ziXcEMGMEeimSKDM1drJhw" name="Shared H-Bridge" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_15wxQMGMEeimSKDM1drJhw" mediniIdentifier="_15wxQMGMEeimSKDM1drJhw" name="Shared Sockets or Connectors" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_850ToMGMEeimSKDM1drJhw" mediniIdentifier="_850ToMGMEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_ELHcAMipEeiciPcxq-kTYA" mediniIdentifier="_ELHcAMipEeiciPcxq-kTYA" name="Shared Information Inputs" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;&#xD;&#xA;Same information consumed by the two functions even in absence of shared resources, i.e. from a functional perspective">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_udGV8MGNEeimSKDM1drJhw" mediniIdentifier="_udGV8MGNEeimSKDM1drJhw" name="Shared  sources of raw physical digital or analogous signals" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_z-vZkMGNEeimSKDM1drJhw" mediniIdentifier="_z-vZkMGNEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_hf2r8MiqEeiciPcxq-kTYA" mediniIdentifier="_hf2r8MiqEeiciPcxq-kTYA" name="Insufficient Environmental Immunity" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;f) environmental factors&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Common external environmental disturbance affects both functions">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_pFJkYMGOEeimSKDM1drJhw" mediniIdentifier="_pFJkYMGOEeimSKDM1drJhw" name="Sensitivity to electrical effects - e.g. suffering from e.g. EMI, ESD" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_xboHIMGOEeimSKDM1drJhw" mediniIdentifier="_xboHIMGOEeimSKDM1drJhw" name="Proximity of HW elements - e.g. suffering from dust, particles" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_5lPSkMGOEeimSKDM1drJhw" mediniIdentifier="_5lPSkMGOEeimSKDM1drJhw" name="Same housing- e.g. suffering from e.g. water entry, humidity" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="__YHQIMGOEeimSKDM1drJhw" mediniIdentifier="__YHQIMGOEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_FRtwUMisEeiciPcxq-kTYA" mediniIdentifier="_FRtwUMisEeiciPcxq-kTYA" name="Systematic Coupling" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;b) development faults&#xD;&#xA;c) manufacturing faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Failure of both elements due to a common systematic human or tool error">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2EesIcGPEeimSKDM1drJhw" mediniIdentifier="_2EesIcGPEeimSKDM1drJhw" name="Identical production processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2EesIsGPEeimSKDM1drJhw" mediniIdentifier="_2EesIsGPEeimSKDM1drJhw" name="Identical repair processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2EesI8GPEeimSKDM1drJhw" mediniIdentifier="_2EesI8GPEeimSKDM1drJhw" name="Identical repair processes used for multiple elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_2EesJMGPEeimSKDM1drJhw" mediniIdentifier="_2EesJMGPEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OiTqkMivEeiciPcxq-kTYA" mediniIdentifier="_OiTqkMivEeiciPcxq-kTYA" name="Components of Identical Type" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;&#xD;&#xA;Identical components may fail with a probability higher than expected due to a common cause failure.&#xD;&#xA;Two functions both use a software, hardware, or system element instance of the same type. If these element instances both fail due to a common mode failure, both functions are affected.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OiTqkcivEeiciPcxq-kTYA" mediniIdentifier="_OiTqkcivEeiciPcxq-kTYA" name="Same type of actuator/power stage e.g. motor" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OiTqksivEeiciPcxq-kTYA" mediniIdentifier="_OiTqksivEeiciPcxq-kTYA" name="Same type of sensors" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OiTqk8ivEeiciPcxq-kTYA" mediniIdentifier="_OiTqk8ivEeiciPcxq-kTYA" name="Other DFI?" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_H6QlccGREeimSKDM1drJhw" mediniIdentifier="_H6QlccGREeimSKDM1drJhw" name="Same type of HW parts and components" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_MyXj4MGREeimSKDM1drJhw" mediniIdentifier="_MyXj4MGREeimSKDM1drJhw" name="Same power supply ICs for different microcontrollers" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_OwxKQMGREeimSKDM1drJhw" mediniIdentifier="_OwxKQMGREeimSKDM1drJhw" name="Same microcontroller" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Qe5gAMGREeimSKDM1drJhw" mediniIdentifier="_Qe5gAMGREeimSKDM1drJhw" name="Same ASICs" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_H6QlcsGREeimSKDM1drJhw" mediniIdentifier="_H6QlcsGREeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="__bRr8MisEeiciPcxq-kTYA" mediniIdentifier="__bRr8MisEeiciPcxq-kTYA" name="Communication" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;i) ageing and wear&#xD;&#xA;&#xD;&#xA;The receiving element is affected by information that is false,  lost, sent multiple times, or in the wrong order, etc. from the sender.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_94eiAMGREeimSKDM1drJhw" mediniIdentifier="_94eiAMGREeimSKDM1drJhw" name="Electrical connection between two HW elements" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="__hUvIMGREeimSKDM1drJhw" mediniIdentifier="__hUvIMGREeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_WawqAMiuEeiciPcxq-kTYA" mediniIdentifier="_WawqAMiuEeiciPcxq-kTYA" name="Unintended Interface" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Two elements affecting each other directly via an unanticipated interface, or with unanticipated effects.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_1n7ysMGSEeimSKDM1drJhw" mediniIdentifier="_1n7ysMGSEeimSKDM1drJhw" name="Proximity of HW elements, creating the potential of crosstalk between signal lines, heat impact, interference etc." user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_4cSJoMGSEeimSKDM1drJhw" mediniIdentifier="_4cSJoMGSEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
    </subItems>
    <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgZVIJSmEeefbsnFgah_5Q" mediniIdentifier="_kgZVIJSmEeefbsnFgah_5Q" name="Semiconductor-level">
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_voPDQMinEeiciPcxq-kTYA" mediniIdentifier="_voPDQMinEeiciPcxq-kTYA" name="Shared Resources" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;g) failures of common external resources&#xD;&#xA;&#xD;&#xA;The same software, hardware, or system element instance used by the two elements which are therefore affected by the failure or unavailability of that shared resource, i.e. from a physical perspective.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="__tsJcMGMEeimSKDM1drJhw" mediniIdentifier="__tsJcMGMEeimSKDM1drJhw" name="Failure of Shared resources" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_Gs7zgMGNEeimSKDM1drJhw" mediniIdentifier="_Gs7zgMGNEeimSKDM1drJhw" name="Single physical root cause" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_-7nzUMGMEeimSKDM1drJhw" mediniIdentifier="_-7nzUMGMEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgajQJSmEeefbsnFgah_5Q" mediniIdentifier="_kgajQJSmEeefbsnFgah_5Q" name="Shared Information Inputs" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;&#xD;&#xA;Same information consumed by the two functions even in absence of shared resources, i.e. from a functional perspective">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_3meVQMGNEeimSKDM1drJhw" mediniIdentifier="_3meVQMGNEeimSKDM1drJhw" name="Failure of Shared resources" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgeNoJSmEeefbsnFgah_5Q" mediniIdentifier="_kgeNoJSmEeefbsnFgah_5Q" name="Other DFI?"/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_ijdeAMiqEeiciPcxq-kTYA" mediniIdentifier="_ijdeAMiqEeiciPcxq-kTYA" name="Insufficient Environmental Immunity" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;f) environmental factors&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Common external environmental disturbance affects both functions">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_D3LccMGPEeimSKDM1drJhw" mediniIdentifier="_D3LccMGPEeimSKDM1drJhw" name="Environmental faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgjtMJSmEeefbsnFgah_5Q" mediniIdentifier="_kgjtMJSmEeefbsnFgah_5Q" name="Other DFI?"/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_GdK20MisEeiciPcxq-kTYA" mediniIdentifier="_GdK20MisEeiciPcxq-kTYA" name="Systematic Coupling" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;b) development faults&#xD;&#xA;c) manufacturing faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Failure of both elements due to a common systematic human or tool error">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_DMg5YMGQEeimSKDM1drJhw" mediniIdentifier="_DMg5YMGQEeimSKDM1drJhw" name="Development faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_FL3iAMGQEeimSKDM1drJhw" mediniIdentifier="_FL3iAMGQEeimSKDM1drJhw" name="Manufacturing faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_IC71wMGQEeimSKDM1drJhw" mediniIdentifier="_IC71wMGQEeimSKDM1drJhw" name="Installation faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_KvQSEMGQEeimSKDM1drJhw" mediniIdentifier="_KvQSEMGQEeimSKDM1drJhw" name="Repair faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgolsJSmEeefbsnFgah_5Q" mediniIdentifier="_kgolsJSmEeefbsnFgah_5Q" name="Other DFI?"/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_akEToMisEeiciPcxq-kTYA" mediniIdentifier="_akEToMisEeiciPcxq-kTYA" name="Components of Identical Type" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;&#xD;&#xA;Identical components may fail with a probability higher than expected due to a common cause failure.&#xD;&#xA;Two functions both use a software, hardware, or system element instance of the same type. If these element instances both fail due to a common mode failure, both functions are affected.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_TQSpkMGREeimSKDM1drJhw" mediniIdentifier="_TQSpkMGREeimSKDM1drJhw" name="Development faults" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgteMJSmEeefbsnFgah_5Q" mediniIdentifier="_kgteMJSmEeefbsnFgah_5Q" name="Other DFI?"/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_AvwLkMitEeiciPcxq-kTYA" mediniIdentifier="_AvwLkMitEeiciPcxq-kTYA" name="Communication" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;e) repair faults&#xD;&#xA;i) ageing and wear&#xD;&#xA;&#xD;&#xA;The receiving element is affected by information that is false,  lost, sent multiple times, or in the wrong order, etc. from the sender.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_BtwKcMGSEeimSKDM1drJhw" mediniIdentifier="_BtwKcMGSEeimSKDM1drJhw" name="Failure of shared resources" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_E56kcMGSEeimSKDM1drJhw" mediniIdentifier="_E56kcMGSEeimSKDM1drJhw" name="Single physical root cause" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_kgxIkJSmEeefbsnFgah_5Q" mediniIdentifier="_kgxIkJSmEeefbsnFgah_5Q" name="Other DFI?"/>
      </subItems>
      <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_XgC3EMiuEeiciPcxq-kTYA" mediniIdentifier="_XgC3EMiuEeiciPcxq-kTYA" name="Unintended Interface" user_Description="Consider these Dependent Failure Indicators  for &#xD;&#xA;a) random hardware failures&#xD;&#xA;b) development faults&#xD;&#xA;d) installation faults&#xD;&#xA;h) stress due to specific situation&#xD;&#xA;&#xD;&#xA;Two elements affecting each other directly via an unanticipated interface, or with unanticipated effects.">
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_6W74cMGSEeimSKDM1drJhw" mediniIdentifier="_6W74cMGSEeimSKDM1drJhw" name="Single physical root cause" user_Description=""/>
        <subItems xsi:type="de.ikv.analyze.checklist:StaticChecklistItem" xmi:id="_89-MIMGSEeimSKDM1drJhw" mediniIdentifier="_89-MIMGSEeimSKDM1drJhw" name="Other DFI?" user_Description=""/>
      </subItems>
    </subItems>
  </items>
</de.ikv.analyze.checklist:Checklist>
