<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_JbMG4NMNEe-Sld_1EWpoOA" mediniIdentifier="_JbMG4NMNEe-Sld_1EWpoOA" name="VEC EV BUSES 21/01/25">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDE9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KDE9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle is expected to require service or maintenance only a few times per year, resulting in an E2 exposure due to the limited frequency of exposure." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDFNfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDFNfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Service " user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDDdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDDdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events." user_Assumptions="Driver/Conductor Sleeping Overnight ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDDtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDDtfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDD9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KDD9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Bus parking in various locations and conditions results in an E4 exposure due to the high frequency of potential hazardous events. xx  in cities " user_Assumptions="People Sleeping while bus is in Bus Stands">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDENfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDENfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Any Occupant + High traffic density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDEdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDEdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Parking in paved wet conditions during rain results in an E3 exposure due to the moderate likelihood of hazardous events in such scenarios." user_Assumptions="People Sleeping while bus is in Bus Stands">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDEtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDEtfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Paved Wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Occupant + Any traffic density" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDFdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDFdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Trucks and buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations. High traffic is worse condition." user_Assumptions="Driver Sleeping ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDFtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDFtfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8Jb0NfCEe-7fd93EIJ22A" mediniIdentifier="_t8Jb0NfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC4NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC4NfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC4dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC4dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Buses undergo charging frequently, resulting in an E4 exposure due to the high frequency of potential exposure during these operations." user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC4tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC4tfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC49fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC49fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Charging under wet and rainy conditions at various locations is moderately frequent in India, resulting in an E3 exposure." user_Assumptions="People might sleep while charging ">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC5NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC5NfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC5dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC5dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with any road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC5tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC5tfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC59fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC59fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with off road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC6NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC6NfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC6dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC6dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Rains in the city occurs only during certain months of the year, regardless of traffic density and off road , resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC6tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC6tfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC69fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC69fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Driving in city conditions with paved road type and environmental factors results in an E4 exposure due to the high frequency of potential hazardous events in such scenarios xx" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC7NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC7NfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Paved" ISO26262_environment="Any Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC7dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC7dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E1" ISO26262_exposureComment="Driving in waterlogged city conditions during rain, with both driver and goods onboard and any traffic density, results in an E1 exposure due to the low likelihood of hazardous events under these conditions" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC7tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC7tfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Water Logged" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC79fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC79fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in city areas, resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC8NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC8NfCEe-7fd93EIJ22A" ISO26262_location="City" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC8dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC8dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Any speed driving on expressways in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC8tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC8tfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC89fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC89fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Off-road patches on the expressway, commonly present due to ongoing construction, occur frequently even with low traffic density, resulting in an E3 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC9NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC9NfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC9dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC9dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E1" ISO26262_exposureComment="Rain on the expressway occurs only during certain months of the year, coupled with low traffic density and off road resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC9tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC9tfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC99fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC99fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC-NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC-NfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC-dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC-dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Rains occur only a few times a year in expressway areas, resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC-tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC-tfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC-9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC-9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="High-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC_NfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC_NfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" user_speed="High vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC_dfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC_dfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Low-speed driving on paved expressways in any temperature results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KC_tfCEe-7fd93EIJ22A" mediniIdentifier="_t8KC_tfCEe-7fd93EIJ22A" ISO26262_location="Expressway" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" user_speed="Low vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KC_9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KC_9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Any speed driving on mountains in any enviroment results in an E4 exposure due to the high likelihood of hazardous events under these conditions" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDANfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDANfCEe-7fd93EIJ22A" ISO26262_location="Mountain" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any Environment " ISO26262_trafficAndPeople="Only Driver + Any density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDAdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDAdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDAtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDAtfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Low density traffic" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDA9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KDA9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E1" ISO26262_exposureComment="Bus travel through tunnels occurs only a few times during a journey, as tunnels are infrequent, even with low traffic density. considering the expesswasy tunnels." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDBNfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDBNfCEe-7fd93EIJ22A" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + High traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDBdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDBdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Off-road patches on the mountains, commonly present due to ongoing construction, occur frequently regardless of traffic density, resulting in an E3 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDBtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDBtfCEe-7fd93EIJ22A" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDB9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KDB9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDCNfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDCNfCEe-7fd93EIJ22A" ISO26262_location="Mountain" ISO26262_roadConditions="Off-road / potholes" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDCdfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDCdfCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Driving on paved mountain roads at any speed and temperature results in an E4 exposure due to the high likelihood of hazardous events in these conditions." user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDCtfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDCtfCEe-7fd93EIJ22A" ISO26262_location="Mountain" ISO26262_roadConditions="Paved" ISO26262_environment="Any temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_t8KDC9fCEe-7fd93EIJ22A" mediniIdentifier="_t8KDC9fCEe-7fd93EIJ22A" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Rains occur only a few times a year in mountainous areas, resulting in an E2 exposure" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_t8KDDNfCEe-7fd93EIJ22A" mediniIdentifier="_t8KDDNfCEe-7fd93EIJ22A" ISO26262_location="Mountain" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_MhmZ8Ni6Ee-uTpMTea_uCA" mediniIdentifier="_MhmZ8Ni6Ee-uTpMTea_uCA" id="-" ISO26262_exposure="E1" user_Assumptions="Parked for long in low temperatures">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_MhsgkNi6Ee-uTpMTea_uCA" mediniIdentifier="_MhsgkNi6Ee-uTpMTea_uCA" ISO26262_location="Any Location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low Temperature" ISO26262_trafficAndPeople="No occupant" ISO26262_itemUsage="Parked " user_speed="Not moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_fwIrYNi6Ee-uTpMTea_uCA" mediniIdentifier="_fwIrYNi6Ee-uTpMTea_uCA" id="-" ISO26262_exposure="E2" user_Assumptions="Parked short period of time.">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_fwIrYdi6Ee-uTpMTea_uCA" mediniIdentifier="_fwIrYdi6Ee-uTpMTea_uCA" ISO26262_location="Any Location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low Temperature" ISO26262_trafficAndPeople="Any occupant + Any Traffic Density" ISO26262_itemUsage="Parked " user_speed="Not moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_dlPhINi6Ee-uTpMTea_uCA" mediniIdentifier="_dlPhINi6Ee-uTpMTea_uCA" id="-" ISO26262_exposure="E2" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_dlPhIdi6Ee-uTpMTea_uCA" mediniIdentifier="_dlPhIdi6Ee-uTpMTea_uCA" ISO26262_location="Any Location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Low Temperature" ISO26262_trafficAndPeople="Driver + Peoples Including Elderly, children, Disabled + Any traffic density" ISO26262_itemUsage="Drive" user_speed="Any vehicle speed"/>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
