<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_apm7cCuFEfCMc_2Esfz5fQ" mediniIdentifier="_apm7cCuFEfCMc_2Esfz5fQ" name="HARA 2W F020">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lO10wCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lO10wCuFEfCMc_2Esfz5fQ" id="HE2429" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lO10wSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lO10wSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lPFFUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPFFUCuFEfCMc_2Esfz5fQ" id="HE2430" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lPFFUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPFFUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lPSgsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPSgsCuFEfCMc_2Esfz5fQ" id="HE2431" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="This case only applicable for spontaneous thermal runaway in which BMS will not be protect battery and persons in the vicinity.">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lPSgsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPSgsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lPet8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPet8CuFEfCMc_2Esfz5fQ" id="HE2432" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lPet8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPet8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lPulkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPulkCuFEfCMc_2Esfz5fQ" id="HE2433" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lPulkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lPulkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lP_rUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lP_rUCuFEfCMc_2Esfz5fQ" id="HE2434" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lP_rUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lP_rUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQL4kCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQL4kCuFEfCMc_2Esfz5fQ" id="HE2435" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQL4kSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQL4kSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQVpkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQVpkCuFEfCMc_2Esfz5fQ" id="HE2436" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQVpkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQVpkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQid4CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQid4CuFEfCMc_2Esfz5fQ" id="HE2437" ISO26262_severity="S2" ISO26262_severityComment="Thermal runaway can result in moderate harm (e.g., smoke, fire); serious outcomes unlikely with basic safety measures in place." ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;&#xD;&#xA;Change Severity to S1 for LFP">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQid4SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQid4SuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQrn0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQrn0CuFEfCMc_2Esfz5fQ" id="HE2438" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQrn0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQrn0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQ31ECuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQ31ECuFEfCMc_2Esfz5fQ" id="HE2439" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQ31ESuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQ31ESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lQ_J0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQ_J0CuFEfCMc_2Esfz5fQ" id="HE2440" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lQ_J0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lQ_J0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lRITwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRITwCuFEfCMc_2Esfz5fQ" id="HE2441" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lRITwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRITwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lRRdsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRRdsCuFEfCMc_2Esfz5fQ" id="HE2442" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lRRdsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRRdsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lRYycCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRYycCuFEfCMc_2Esfz5fQ" id="HE2443" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lRYycSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRYycSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lRgHMCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRgHMCuFEfCMc_2Esfz5fQ" id="HE2444" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lRgHMSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lRgHMSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_tMJ_UExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lTfEMCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTfEMCuFEfCMc_2Esfz5fQ" id="HE2461" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lTfEMSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTfEMSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lTmY8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTmY8CuFEfCMc_2Esfz5fQ" id="HE2462" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lTmY8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTmY8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lTttsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTttsCuFEfCMc_2Esfz5fQ" id="HE2463" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lTttsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lTttsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lT1CcCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lT1CcCuFEfCMc_2Esfz5fQ" id="HE2464" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lT1CcSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lT1CcSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lT9lUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lT9lUCuFEfCMc_2Esfz5fQ" id="HE2465" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lT9lUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lT9lUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUE6ECuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUE6ECuFEfCMc_2Esfz5fQ" id="HE2466" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUE6ESuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUE6ESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lULnwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lULnwCuFEfCMc_2Esfz5fQ" id="HE2467" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lULnwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lULnwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUTjkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUTjkCuFEfCMc_2Esfz5fQ" id="HE2468" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUTjkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUTjkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUbfYCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUbfYCuFEfCMc_2Esfz5fQ" id="HE2469" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUbfYSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUbfYSuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUi0ICuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUi0ICuFEfCMc_2Esfz5fQ" id="HE2470" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUi0ISuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUi0ISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUph0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUph0CuFEfCMc_2Esfz5fQ" id="HE2471" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUph0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUph0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lUxdoCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUxdoCuFEfCMc_2Esfz5fQ" id="HE2472" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lUxdoSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lUxdoSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lU5ZcCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lU5ZcCuFEfCMc_2Esfz5fQ" id="HE2473" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lU5ZcSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lU5ZcSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVAHICuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVAHICuFEfCMc_2Esfz5fQ" id="HE2474" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVAHISuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVAHISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVIqACuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVIqACuFEfCMc_2Esfz5fQ" id="HE2475" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVIqASuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVIqASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVQl0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVQl0CuFEfCMc_2Esfz5fQ" id="HE2476" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVQl0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVQl0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_wWJ2IExVEe2zRcf-1tDSGA"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVX6kCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVX6kCuFEfCMc_2Esfz5fQ" id="HE2477" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVX6kSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVX6kSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVgdcCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVgdcCuFEfCMc_2Esfz5fQ" id="HE2478" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVgdcSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVgdcSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVnyMCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVnyMCuFEfCMc_2Esfz5fQ" id="HE2479" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVnyMSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVnyMSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lVvG8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVvG8CuFEfCMc_2Esfz5fQ" id="HE2480" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lVvG8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lVvG8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lV2bsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lV2bsCuFEfCMc_2Esfz5fQ" id="HE2481" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lV2bsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lV2bsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lV--kCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lV--kCuFEfCMc_2Esfz5fQ" id="HE2482" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lV--kSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lV--kSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWGTUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWGTUCuFEfCMc_2Esfz5fQ" id="HE2483" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWGTUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWGTUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWNoECuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWNoECuFEfCMc_2Esfz5fQ" id="HE2484" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWNoESuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWNoESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWU80CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWU80CuFEfCMc_2Esfz5fQ" id="HE2485" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWU80SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWU80SuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWdfsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWdfsCuFEfCMc_2Esfz5fQ" id="HE2486" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C1" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWdfsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWdfsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWk0cCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWk0cCuFEfCMc_2Esfz5fQ" id="HE2487" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWk0cSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWk0cSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWriICuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWriICuFEfCMc_2Esfz5fQ" id="HE2488" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWriISuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWriISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lWzd8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWzd8CuFEfCMc_2Esfz5fQ" id="HE2489" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lWzd8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lWzd8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lW8n4CuFEfCMc_2Esfz5fQ" mediniIdentifier="_lW8n4CuFEfCMc_2Esfz5fQ" id="HE2490" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lW8n4SuFEfCMc_2Esfz5fQ" mediniIdentifier="_lW8n4SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lXDVkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lXDVkCuFEfCMc_2Esfz5fQ" id="HE2491" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C2" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lXDVkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lXDVkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_lXKqUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_lXKqUCuFEfCMc_2Esfz5fQ" id="HE2492" ISO26262_severity="S0" ISO26262_severityComment="No safety risk; only minor inconvenience." ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_lXKqUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_lXKqUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_mdxTYExjEe2Kw8YgMgGasw"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c4-aEH2XEfCJDp8kareSBg" mediniIdentifier="_c4-aEH2XEfCJDp8kareSBg" id="HE145" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c4-aEX2XEfCJDp8kareSBg" mediniIdentifier="_c4-aEX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5FHwH2XEfCJDp8kareSBg" mediniIdentifier="_c5FHwH2XEfCJDp8kareSBg" id="HE146" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" ISO26262_controllability="C1" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5FHwX2XEfCJDp8kareSBg" mediniIdentifier="_c5FHwX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5JZMH2XEfCJDp8kareSBg" mediniIdentifier="_c5JZMH2XEfCJDp8kareSBg" id="HE147" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5JZMX2XEfCJDp8kareSBg" mediniIdentifier="_c5JZMX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5ORsH2XEfCJDp8kareSBg" mediniIdentifier="_c5ORsH2XEfCJDp8kareSBg" id="HE148" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5ORsX2XEfCJDp8kareSBg" mediniIdentifier="_c5ORsX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5TKMH2XEfCJDp8kareSBg" mediniIdentifier="_c5TKMH2XEfCJDp8kareSBg" id="HE149" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5TKMX2XEfCJDp8kareSBg" mediniIdentifier="_c5TKMX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5YCsH2XEfCJDp8kareSBg" mediniIdentifier="_c5YCsH2XEfCJDp8kareSBg" id="HE150" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5YCsX2XEfCJDp8kareSBg" mediniIdentifier="_c5YCsX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5c7MH2XEfCJDp8kareSBg" mediniIdentifier="_c5c7MH2XEfCJDp8kareSBg" id="HE151" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5c7MX2XEfCJDp8kareSBg" mediniIdentifier="_c5c7MX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5hzsH2XEfCJDp8kareSBg" mediniIdentifier="_c5hzsH2XEfCJDp8kareSBg" id="HE152" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5hzsX2XEfCJDp8kareSBg" mediniIdentifier="_c5hzsX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5nTQH2XEfCJDp8kareSBg" mediniIdentifier="_c5nTQH2XEfCJDp8kareSBg" id="HE153" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" ISO26262_controllability="C1" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5nTQX2XEfCJDp8kareSBg" mediniIdentifier="_c5nTQX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5sLwH2XEfCJDp8kareSBg" mediniIdentifier="_c5sLwH2XEfCJDp8kareSBg" id="HE154" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5sLwX2XEfCJDp8kareSBg" mediniIdentifier="_c5sLwX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5xEQH2XEfCJDp8kareSBg" mediniIdentifier="_c5xEQH2XEfCJDp8kareSBg" id="HE155" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5xEQX2XEfCJDp8kareSBg" mediniIdentifier="_c5xEQX2XEfCJDp8kareSBg" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c518wH2XEfCJDp8kareSBg" mediniIdentifier="_c518wH2XEfCJDp8kareSBg" id="HE156" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c518wX2XEfCJDp8kareSBg" mediniIdentifier="_c518wX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c561QH2XEfCJDp8kareSBg" mediniIdentifier="_c561QH2XEfCJDp8kareSBg" id="HE157" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c561QX2XEfCJDp8kareSBg" mediniIdentifier="_c561QX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c5_twH2XEfCJDp8kareSBg" mediniIdentifier="_c5_twH2XEfCJDp8kareSBg" id="HE158" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_1na5QDsvEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c5_twX2XEfCJDp8kareSBg" mediniIdentifier="_c5_twX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c6FNUH2XEfCJDp8kareSBg" mediniIdentifier="_c6FNUH2XEfCJDp8kareSBg" id="HE159" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c6FNUX2XEfCJDp8kareSBg" mediniIdentifier="_c6FNUX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c6KF0H2XEfCJDp8kareSBg" mediniIdentifier="_c6KF0H2XEfCJDp8kareSBg" id="HE160" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c6KF0X2XEfCJDp8kareSBg" mediniIdentifier="_c6KF0X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_HC9JQHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c8iEYH2XEfCJDp8kareSBg" mediniIdentifier="_c8iEYH2XEfCJDp8kareSBg" id="HE193" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c8iEYX2XEfCJDp8kareSBg" mediniIdentifier="_c8iEYX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c8m84H2XEfCJDp8kareSBg" mediniIdentifier="_c8m84H2XEfCJDp8kareSBg" id="HE194" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" ISO26262_controllability="C1" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c8m84X2XEfCJDp8kareSBg" mediniIdentifier="_c8m84X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c8rOUH2XEfCJDp8kareSBg" mediniIdentifier="_c8rOUH2XEfCJDp8kareSBg" id="HE195" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c8rOUX2XEfCJDp8kareSBg" mediniIdentifier="_c8rOUX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c8wG0H2XEfCJDp8kareSBg" mediniIdentifier="_c8wG0H2XEfCJDp8kareSBg" id="HE196" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c8wG0X2XEfCJDp8kareSBg" mediniIdentifier="_c8wG0X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c80_UH2XEfCJDp8kareSBg" mediniIdentifier="_c80_UH2XEfCJDp8kareSBg" id="HE197" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c80_UX2XEfCJDp8kareSBg" mediniIdentifier="_c80_UX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c85QwH2XEfCJDp8kareSBg" mediniIdentifier="_c85QwH2XEfCJDp8kareSBg" id="HE198" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c85QwX2XEfCJDp8kareSBg" mediniIdentifier="_c85QwX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c8-JQH2XEfCJDp8kareSBg" mediniIdentifier="_c8-JQH2XEfCJDp8kareSBg" id="HE199" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c8-JQX2XEfCJDp8kareSBg" mediniIdentifier="_c8-JQX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9CasH2XEfCJDp8kareSBg" mediniIdentifier="_c9CasH2XEfCJDp8kareSBg" id="HE200" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9CasX2XEfCJDp8kareSBg" mediniIdentifier="_c9CasX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9HTMH2XEfCJDp8kareSBg" mediniIdentifier="_c9HTMH2XEfCJDp8kareSBg" id="HE201" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" ISO26262_controllability="C1" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9HTMX2XEfCJDp8kareSBg" mediniIdentifier="_c9HTMX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9LkoH2XEfCJDp8kareSBg" mediniIdentifier="_c9LkoH2XEfCJDp8kareSBg" id="HE202" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9LkoX2XEfCJDp8kareSBg" mediniIdentifier="_c9LkoX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9QdIH2XEfCJDp8kareSBg" mediniIdentifier="_c9QdIH2XEfCJDp8kareSBg" id="HE203" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9QdIX2XEfCJDp8kareSBg" mediniIdentifier="_c9QdIX2XEfCJDp8kareSBg" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9UukH2XEfCJDp8kareSBg" mediniIdentifier="_c9UukH2XEfCJDp8kareSBg" id="HE204" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9UukX2XEfCJDp8kareSBg" mediniIdentifier="_c9UukX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9ZAAH2XEfCJDp8kareSBg" mediniIdentifier="_c9ZAAH2XEfCJDp8kareSBg" id="HE205" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9ZAAX2XEfCJDp8kareSBg" mediniIdentifier="_c9ZAAX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9d4gH2XEfCJDp8kareSBg" mediniIdentifier="_c9d4gH2XEfCJDp8kareSBg" id="HE206" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" ISO26262_controllability="C2" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9d4gX2XEfCJDp8kareSBg" mediniIdentifier="_c9d4gX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9ixAH2XEfCJDp8kareSBg" mediniIdentifier="_c9ixAH2XEfCJDp8kareSBg" id="HE207" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9ixAX2XEfCJDp8kareSBg" mediniIdentifier="_c9ixAX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_c9npgH2XEfCJDp8kareSBg" mediniIdentifier="_c9npgH2XEfCJDp8kareSBg" id="HE208" ISO26262_severity="S1" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_un_tEDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_c9npgX2XEfCJDp8kareSBg" mediniIdentifier="_c9npgX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_MS28oHgWEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
