<?xml version="1.1" encoding="UTF-8"?>
<safegoals:SafetyRequirementsModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safegoals="http://www.ikv.de/analyze/metamodels/SafetyGoals/1.0" xmi:id="_wCDisHVYEeSHJr9dJxG-Iw" mediniIdentifier="_wCDisHVYEeSHJr9dJxG-Iw" name="HW Safety Requirements">
  <reqRelations xsi:type="safegoals:SafetyReqRelation" xmi:id="_pj5kcBbUEfCJh5s3y1LNtw" mediniIdentifier="_pj5kcBbUEfCJh5s3y1LNtw" target="_gfDf0BbUEfCJh5s3y1LNtw" source="_j9mqUBbUEfCJh5s3y1LNtw"/>
  <reqRelations xsi:type="safegoals:SafetyReqRelation" xmi:id="_p-TogBbUEfCJh5s3y1LNtw" mediniIdentifier="_p-TogBbUEfCJh5s3y1LNtw" source="_gfDf0BbUEfCJh5s3y1LNtw">
    <target xsi:type="safegoals:SafetyRequirement" href="_qdRrgHVYEeSHJr9dJxG-Iw.safetygoal#_7svKUAO9Ee-mCMiklR9HrQ"/>
  </reqRelations>
  <reqRelations xsi:type="safegoals:SafetyReqRelation" xmi:id="_qanxEBbUEfCJh5s3y1LNtw" mediniIdentifier="_qanxEBbUEfCJh5s3y1LNtw" source="_dq2S0BbUEfCJh5s3y1LNtw">
    <target xsi:type="safegoals:SafetyRequirement" href="_qdRrgHVYEeSHJr9dJxG-Iw.safetygoal#_7svKUAO9Ee-mCMiklR9HrQ"/>
  </reqRelations>
  <requirements xsi:type="safegoals:SafetyRequirement" xmi:id="_dq2S0BbUEfCJh5s3y1LNtw" mediniIdentifier="_dq2S0BbUEfCJh5s3y1LNtw" name="Add RC filter of xxx ms at the signal input" identifier="SR777" kind="HARDWARE" ISO26262_asil="B" user_Time_constraint="" user_Physical_constraint=""/>
  <requirements xsi:type="safegoals:SafetyRequirement" xmi:id="_gfDf0BbUEfCJh5s3y1LNtw" mediniIdentifier="_gfDf0BbUEfCJh5s3y1LNtw" name="Provide ESD protection of xxx " identifier="SR778" kind="HARDWARE" ISO26262_asil="B" user_Time_constraint="" user_Physical_constraint=""/>
  <requirements xsi:type="safegoals:SafetyRequirement" xmi:id="_j9mqUBbUEfCJh5s3y1LNtw" mediniIdentifier="_j9mqUBbUEfCJh5s3y1LNtw" name="The ESD protection shall be placed within xxx mm of the input of the signal connector" identifier="SR779" kind="HARDWARE" ISO26262_asil="B" user_Time_constraint="" user_Physical_constraint=""/>
  <requirements xsi:type="safegoals:SafetyRequirement" xmi:id="_AhI8QBbVEfCJh5s3y1LNtw" mediniIdentifier="_AhI8QBbVEfCJh5s3y1LNtw" name="[X&#x5d; CAN lines must be protected against spikes of upto xxx" identifier="SR780" kind="TECHNICAL" ISO26262_asil="B" user_Time_constraint="" user_Physical_constraint=""/>
</safegoals:SafetyRequirementsModel>
