<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_It9FIAX3Eeq4AMRV0u5rew" mediniIdentifier="_It9FIAX3Eeq4AMRV0u5rew" name="P-11 Table 51 - PLD: Logic-Block">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gAAYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gAAYBEeq4AMRV0u5rew" id="ISO26262-11: Table 51" name="Mix of spatial and temporal redundancy by means of reconfiguration" description="No default typical DC given in ISO26262" notes="none"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gAQYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gAQYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.1" name="Self-test by software: limited number of patterns (one channel)" maxDC="MEDIUM" notes="Depends on the quality of the self test"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gAgYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gAgYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.3" name="Self-test by software cross exchange between two independent units" maxDC="MEDIUM" notes="Depends of the quality of the self test"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gAwYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gAwYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.2" name="Self-test supported by hardware (one-channel)" maxDC="MEDIUM" notes="Depends on the quality of the self test"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gBAYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gBAYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.4" name="Software diversified redundancy (one hardware channel)" maxDC="HIGH" notes="Depends of the quality of the diversification. Common  mode failures can reduce diagnostic coverage"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gBQYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gBQYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.5" name="Reciprocal comparison by software" maxDC="HIGH" notes="Depends of the quality of the comparison"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gBgYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gBgYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.6" name="HW redundancy (e.g. Dual Core Lockstep, asymmetric redundancy, coded processing)" maxDC="HIGH" notes="It depends on the quality of redundancy. Common mode failures can reduce diagnostic coverage"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gBwYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gBwYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.7" name="Configuration Register Test" maxDC="HIGH" notes="Configuration Registers only"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gCAYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gCAYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.8" name="Stack over/under flow Detection" maxDC="LOW" notes="Stack boundary test only"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gCQYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gCQYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.9" name="Integrated Hardware consistency monitoring" maxDC="HIGH" notes="Coverage for illegal hardware exceptions only"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gCgYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gCgYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.1" name="Self-test by software" maxDC="MEDIUM" notes="-"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Gq8gCwYBEeq4AMRV0u5rew" mediniIdentifier="_Gq8gCwYBEeq4AMRV0u5rew" id="ISO26262-5: D.2.3.2" name="Self-test supported by hardware (one-channel)" maxDC="MEDIUM" notes="Higher coverage is possible, depending on effectiveness of test. Gate level is an appropriate level for this test."/>
</safety:MeasureCatalog>
