<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_rSuvoCseEfCMc_2Esfz5fQ" mediniIdentifier="_rSuvoCseEfCMc_2Esfz5fQ" name="2W Operational Cases">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmsCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmsCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmsStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmsStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" user_speed="High speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmsitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmsitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmsytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmsytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" user_speed="Low speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmtCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmtCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmtStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmtStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" user_speed="High speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmtitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmtitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmtytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmtytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" user_speed="High speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmuCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmuCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmuStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmuStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" user_speed="Low speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmuitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmuitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmuytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmuytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" user_speed="High speed"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmvCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmvCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmvStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmvStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmvitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmvitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmvytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmvytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmwCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmwCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmwStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmwStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmwitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmwitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmwytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmwytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmxCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmxCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmxStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmxStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmxitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmxitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmxytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmxytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmyCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmyCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmyStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmyStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmyitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmyitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E2" ISO26262_exposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" user_Assumptions="">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmyytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmyytLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmzCtLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmzCtLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmzStLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmzStLEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_2kPmzitLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmzitLEfCMc_2Esfz5fQ" id="-" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_2kPmzytLEfCMc_2Esfz5fQ" mediniIdentifier="_2kPmzytLEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" user_speed="Not Moving"/>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
