<?xml version="1.1" encoding="UTF-8"?>
<safety:MeasureCatalog xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:safety="http://www.ikv.de/medini/metamodels/SafetyModel/1.0" xmi:id="_8H8DsOUkEemDKMXKazwdEA" mediniIdentifier="_8H8DsOUkEemDKMXKazwdEA" name="P-11 Table 40 - Analogue/Mixed Signal: AD converter">
  <collectionType href="http://www.ikv.de/medini/metamodels/SafetyModel/1.0#//SafetyMechanism"/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_Af8lwOUlEemDKMXKazwdEA" mediniIdentifier="_Af8lwOUlEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.12" name="ADC attenuation detection" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit controlled by a digital circuit that validates the ADC conversion path by measuring a known and stable signal value."/>
  <measures xsi:type="safety:SafetyMechanism" xmi:id="_AnzhQOUlEemDKMXKazwdEA" mediniIdentifier="_AnzhQOUlEemDKMXKazwdEA" id="ISO26262-11: 5.2.4.13" name="Stuck on ADC channel detection" description="NOTE 1 It is not possible to give a general guidance on the DC because it strongly depends on the specific technology, type of circuit, use case etc." notes="Typically an analogue circuit controlled by a digital circuit that validates the ADC conversion path by measuring a known and stable signal value."/>
</safety:MeasureCatalog>
