<?xml version="1.1" encoding="UTF-8"?>
<hazardmodel:HazardAnalysisModel xmi:version="2.0" xmlns:xmi="http://www.omg.org/XMI" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:hazardmodel="http://www.ikv.de/analyze/metamodels/HazardAnalysis/1.0" xmi:id="_ZhdAkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ZhdAkCuFEfCMc_2Esfz5fQ" name="HARA 2W F019">
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_neSH0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_neSH0CuFEfCMc_2Esfz5fQ" id="HE2509" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_neSH0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_neSH0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nedG8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nedG8CuFEfCMc_2Esfz5fQ" id="HE2510" ISO26262_severity="S2" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nedG8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nedG8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_neuMsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_neuMsCuFEfCMc_2Esfz5fQ" id="HE2511" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_neuMsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_neuMsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ne7oECuFEfCMc_2Esfz5fQ" mediniIdentifier="_ne7oECuFEfCMc_2Esfz5fQ" id="HE2512" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ne7oESuFEfCMc_2Esfz5fQ" mediniIdentifier="_ne7oESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nfMt0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfMt0CuFEfCMc_2Esfz5fQ" id="HE2513" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nfMt0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfMt0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nfZiICuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfZiICuFEfCMc_2Esfz5fQ" id="HE2514" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nfZiISuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfZiISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nflvYCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nflvYCuFEfCMc_2Esfz5fQ" id="HE2515" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nflvYSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nflvYSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nfxVkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfxVkCuFEfCMc_2Esfz5fQ" id="HE2516" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nfxVkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nfxVkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nf9i0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nf9i0CuFEfCMc_2Esfz5fQ" id="HE2517" ISO26262_severity="S1" ISO26262_severityComment="Thermal runaway can result in moderate harm (e.g., smoke, fire); serious outcomes unlikely with basic safety measures in place." ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nf9i0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nf9i0SuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ngGFsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngGFsCuFEfCMc_2Esfz5fQ" id="HE2518" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ngGFsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngGFsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ngQdwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngQdwCuFEfCMc_2Esfz5fQ" id="HE2519" ISO26262_severity="S2" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ngQdwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngQdwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ngaOwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngaOwCuFEfCMc_2Esfz5fQ" id="HE2520" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ngaOwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngaOwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ngjYsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngjYsCuFEfCMc_2Esfz5fQ" id="HE2521" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ngjYsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngjYsSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ngr7kCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngr7kCuFEfCMc_2Esfz5fQ" id="HE2522" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ngr7kSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ngr7kSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ng1FgCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ng1FgCuFEfCMc_2Esfz5fQ" id="HE2523" ISO26262_severity="S2" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ng1FgSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ng1FgSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ng9BUCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ng9BUCuFEfCMc_2Esfz5fQ" id="HE2524" ISO26262_severity="S1" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ng9BUSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ng9BUSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_kSaOQFs5Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhFkMCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhFkMCuFEfCMc_2Esfz5fQ" id="HE2525" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhFkMSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhFkMSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhNgACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhNgACuFEfCMc_2Esfz5fQ" id="HE2526" ISO26262_severity="S2" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhNgASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhNgASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhU0wCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhU0wCuFEfCMc_2Esfz5fQ" id="HE2527" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhU0wSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhU0wSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhcJgCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhcJgCuFEfCMc_2Esfz5fQ" id="HE2528" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhcJgSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhcJgSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhksYCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhksYCuFEfCMc_2Esfz5fQ" id="HE2529" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhksYSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhksYSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nhsoMCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhsoMCuFEfCMc_2Esfz5fQ" id="HE2530" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nhsoMSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nhsoMSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nh0kACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nh0kACuFEfCMc_2Esfz5fQ" id="HE2531" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nh0kASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nh0kASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nh8f0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nh8f0CuFEfCMc_2Esfz5fQ" id="HE2532" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nh8f0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nh8f0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_niFpwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_niFpwCuFEfCMc_2Esfz5fQ" id="HE2533" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_niFpwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_niFpwSuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_niNlkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_niNlkCuFEfCMc_2Esfz5fQ" id="HE2534" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Simply controllable: The sudden power-loss produces only mild deceleration; nearly all riders can keep balance with normal steering/braking and pull over safely.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_niNlkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_niNlkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_niWvgCuFEfCMc_2Esfz5fQ" mediniIdentifier="_niWvgCuFEfCMc_2Esfz5fQ" id="HE2535" ISO26262_severity="S2" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_niWvgSuFEfCMc_2Esfz5fQ" mediniIdentifier="_niWvgSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nieEQCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nieEQCuFEfCMc_2Esfz5fQ" id="HE2536" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nieEQSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nieEQSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nimnICuFEfCMc_2Esfz5fQ" mediniIdentifier="_nimnICuFEfCMc_2Esfz5fQ" id="HE2537" ISO26262_severity="S1" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nimnISuFEfCMc_2Esfz5fQ" mediniIdentifier="_nimnISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nivKACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nivKACuFEfCMc_2Esfz5fQ" id="HE2538" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nivKASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nivKASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ni3s4CuFEfCMc_2Esfz5fQ" mediniIdentifier="_ni3s4CuFEfCMc_2Esfz5fQ" id="HE2539" ISO26262_severity="S2" ISO26262_severityComment="Sudden power loss can cause abrupt deceleration or a brief skid, risking minor, reversible injuries—e.g., bruises or whiplash—from a slip or a low-speed rear-end impact.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Normally controllable: At high  speeds, an abrupt loss of drive torque demands quick rider input; most riders can brake and stabilise, but a portion will find control difficult.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ni3s4SuFEfCMc_2Esfz5fQ" mediniIdentifier="_ni3s4SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_ni_osCuFEfCMc_2Esfz5fQ" mediniIdentifier="_ni_osCuFEfCMc_2Esfz5fQ" id="HE2540" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_ni_osSuFEfCMc_2Esfz5fQ" mediniIdentifier="_ni_osSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_ZJB7gFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njIyoCuFEfCMc_2Esfz5fQ" mediniIdentifier="_njIyoCuFEfCMc_2Esfz5fQ" id="HE2541" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njIyoSuFEfCMc_2Esfz5fQ" mediniIdentifier="_njIyoSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njQucCuFEfCMc_2Esfz5fQ" mediniIdentifier="_njQucCuFEfCMc_2Esfz5fQ" id="HE2542" ISO26262_severity="S2" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njQucSuFEfCMc_2Esfz5fQ" mediniIdentifier="_njQucSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njYqQCuFEfCMc_2Esfz5fQ" mediniIdentifier="_njYqQCuFEfCMc_2Esfz5fQ" id="HE2543" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njYqQSuFEfCMc_2Esfz5fQ" mediniIdentifier="_njYqQSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njgmECuFEfCMc_2Esfz5fQ" mediniIdentifier="_njgmECuFEfCMc_2Esfz5fQ" id="HE2544" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njgmESuFEfCMc_2Esfz5fQ" mediniIdentifier="_njgmESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njpI8CuFEfCMc_2Esfz5fQ" mediniIdentifier="_njpI8CuFEfCMc_2Esfz5fQ" id="HE2545" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njpI8SuFEfCMc_2Esfz5fQ" mediniIdentifier="_njpI8SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_njxEwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_njxEwCuFEfCMc_2Esfz5fQ" id="HE2546" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_njxEwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_njxEwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nj4ZgCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nj4ZgCuFEfCMc_2Esfz5fQ" id="HE2547" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nj4ZgSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nj4ZgSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkA8YCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkA8YCuFEfCMc_2Esfz5fQ" id="HE2548" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkA8YSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkA8YSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkJfQCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkJfQCuFEfCMc_2Esfz5fQ" id="HE2549" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkJfQSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkJfQSuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkRbECuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkRbECuFEfCMc_2Esfz5fQ" id="HE2550" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkRbESuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkRbESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkZ98CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkZ98CuFEfCMc_2Esfz5fQ" id="HE2551" ISO26262_severity="S2" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkZ98SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkZ98SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkig0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkig0CuFEfCMc_2Esfz5fQ" id="HE2552" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkig0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkig0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkqcoCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkqcoCuFEfCMc_2Esfz5fQ" id="HE2553" ISO26262_severity="S2" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkqcoSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkqcoSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nkyYcCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkyYcCuFEfCMc_2Esfz5fQ" id="HE2554" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nkyYcSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nkyYcSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nk67UCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nk67UCuFEfCMc_2Esfz5fQ" id="HE2555" ISO26262_severity="S2" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nk67USuFEfCMc_2Esfz5fQ" mediniIdentifier="_nk67USuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlC3ICuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlC3ICuFEfCMc_2Esfz5fQ" id="HE2556" ISO26262_severity="S1" ISO26262_severityComment="No safety risk involved" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_eajUkDswEe2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlC3ISuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlC3ISuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_OovzoFs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlLaACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlLaACuFEfCMc_2Esfz5fQ" id="HE2557" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlLaASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlLaASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlT84CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlT84CuFEfCMc_2Esfz5fQ" id="HE2558" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlT84SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlT84SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlb4sCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlb4sCuFEfCMc_2Esfz5fQ" id="HE2559" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlb4sSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlb4sSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlj0gCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlj0gCuFEfCMc_2Esfz5fQ" id="HE2560" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="The vehicle remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlj0gSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlj0gSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nlrJQCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlrJQCuFEfCMc_2Esfz5fQ" id="HE2561" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens every day for city riders → high probability ⇒ E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nlrJQSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nlrJQSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nl06QCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nl06QCuFEfCMc_2Esfz5fQ" id="HE2562" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nl06QSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nl06QSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nl8PACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nl8PACuFEfCMc_2Esfz5fQ" id="HE2563" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nl8PASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nl8PASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmEK0CuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmEK0CuFEfCMc_2Esfz5fQ" id="HE2564" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmEK0SuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmEK0SuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmMtsCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmMtsCuFEfCMc_2Esfz5fQ" id="HE2565" ISO26262_severity="S0" ISO26262_severityComment="Thermal runaway can result in moderate harm (e.g., smoke, fire); serious outcomes unlikely with basic safety measures in place." ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmMtsSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmMtsSuFEfCMc_2Esfz5fQ" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmV3oCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmV3oCuFEfCMc_2Esfz5fQ" id="HE2566" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Rider notices a hot or smoky battery in time, retains full control, decelerates safely, parks, and steps away before the situation escalates.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmV3oSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmV3oSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmdMYCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmdMYCuFEfCMc_2Esfz5fQ" id="HE2567" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmdMYSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmdMYSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmlvQCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmlvQCuFEfCMc_2Esfz5fQ" id="HE2568" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmlvQSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmlvQSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nmtrECuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmtrECuFEfCMc_2Esfz5fQ" id="HE2569" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nmtrESuFEfCMc_2Esfz5fQ" mediniIdentifier="_nmtrESuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nm21ACuFEfCMc_2Esfz5fQ" mediniIdentifier="_nm21ACuFEfCMc_2Esfz5fQ" id="HE2570" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nm21ASuFEfCMc_2Esfz5fQ" mediniIdentifier="_nm21ASuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
    <ISO26262_safetyGoal href="../goals/_zGRBwLryEeG74PAEAJO_Uw.safetygoal#_CzelwFB3Ee2Kw8YgMgGasw"/>
    <user_accident_type>fire/explosion</user_accident_type>
    <user_accident_type>gas inhalation</user_accident_type>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nm-JwCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nm-JwCuFEfCMc_2Esfz5fQ" id="HE2571" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3." ISO26262_controllability="C3" ISO26262_controllabilityComment="Heat or smoke becomes noticeable only shortly before escalation; most riders can still brake and pull over, but prompt, coordinated action is needed—some may wobble or tip before coming to a safe stop.&#xD;&#xA;" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nm-JwSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nm-JwSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_nnGFkCuFEfCMc_2Esfz5fQ" mediniIdentifier="_nnGFkCuFEfCMc_2Esfz5fQ" id="HE2572" ISO26262_severity="S0" ISO26262_severityComment="Light injuries (e.g., minor bruises or sprains) may occur during emergency egress from the vehicle.&#xD;&#xA;" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2." ISO26262_controllability="C3" ISO26262_controllabilityComment="Not controllable by the driver or any person in the vicinity" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_nnGFkSuFEfCMc_2Esfz5fQ" mediniIdentifier="_nnGFkSuFEfCMc_2Esfz5fQ" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_W-ZP8Fs4Ee2fU5b5rzhp9A"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hk1sQH2XEfCJDp8kareSBg" mediniIdentifier="_hk1sQH2XEfCJDp8kareSBg" id="HE209" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Could result in false positive ">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hk1sQX2XEfCJDp8kareSBg" mediniIdentifier="_hk1sQX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Overnight charging in a confined indoor space (regardless of weather) happens  every day for city riders → high probability ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hk7L0H2XEfCJDp8kareSBg" mediniIdentifier="_hk7L0H2XEfCJDp8kareSBg" id="HE210" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hk7L0X2XEfCJDp8kareSBg" mediniIdentifier="_hk7L0X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + High traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Carrying a pillion through stop-and-go city traffic is routine for office commutes and school drops; it occurs on most urban journeys → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlArYH2XEfCJDp8kareSBg" mediniIdentifier="_hlArYH2XEfCJDp8kareSBg" id="HE211" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming Multiple battery at same place charging simultaneouly [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlArYX2XEfCJDp8kareSBg" mediniIdentifier="_hlArYX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Re-charging inside hot, confined spaces (small repair kiosks, home garages) is a daily event in warm Indian climates → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlFj4H2XEfCJDp8kareSBg" mediniIdentifier="_hlFj4H2XEfCJDp8kareSBg" id="HE212" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlFj4X2XEfCJDp8kareSBg" mediniIdentifier="_hlFj4X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Riders still top-up at public chargers during rain (covered sheds, petrol pumps); with daily charging needs, the overall exposure stays high → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlJ1UH2XEfCJDp8kareSBg" mediniIdentifier="_hlJ1UH2XEfCJDp8kareSBg" id="HE213" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming that the battery has been plugged in to fast charge at High Temperatures after rapid Discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlJ1UX2XEfCJDp8kareSBg" mediniIdentifier="_hlJ1UX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Charging in a confined, hot garage occurs every charging cycle in hot climates; most riders charge daily → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmvCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlPU4H2XEfCJDp8kareSBg" mediniIdentifier="_hlPU4H2XEfCJDp8kareSBg" id="HE214" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlPU4X2XEfCJDp8kareSBg" mediniIdentifier="_hlPU4X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Indoor parking (basement/garage) with people nearby is part of nearly every trip end, so the scenario exists most of the time the vehicle is stationary ⇒ E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlTmUH2XEfCJDp8kareSBg" mediniIdentifier="_hlTmUH2XEfCJDp8kareSBg" id="HE215" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlTmUX2XEfCJDp8kareSBg" mediniIdentifier="_hlTmUX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Rain-soaked highway travel with pillion is limited to the rainy season and long-distance rides, giving low annual frequency ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmuitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlZF4H2XEfCJDp8kareSBg" mediniIdentifier="_hlZF4H2XEfCJDp8kareSBg" id="HE216" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlZF4X2XEfCJDp8kareSBg" mediniIdentifier="_hlZF4X2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Outdoor fast-charging in high temperature is daily routine in many Tier-2 cities from March to June; summer charging is therefore a high-probability scenario → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmxCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hld-YH2XEfCJDp8kareSBg" mediniIdentifier="_hld-YH2XEfCJDp8kareSBg" id="HE217" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hld-YX2XEfCJDp8kareSBg" mediniIdentifier="_hld-YX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + High Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Crawling through dense city traffic on hot paved roads is an everyday commute for most riders in metros such as Mumbai or Bengaluru; the scenario is present on most trips → E4.&#xD;&#xA;" user_speed="Low speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlkFAH2XEfCJDp8kareSBg" mediniIdentifier="_hlkFAH2XEfCJDp8kareSBg" id="HE218" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlkFAX2XEfCJDp8kareSBg" mediniIdentifier="_hlkFAX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved wet" ISO26262_environment="Rain" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Very wet paved road at high speed requires both rain and highway use—conditions that arise only on some rainy days, i.e., few operating conditions per year ⇒ E2.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hloWcH2XEfCJDp8kareSBg" mediniIdentifier="_hloWcH2XEfCJDp8kareSBg" id="HE219" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Swappable battery charging at home [S&#x5d;">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hloWcX2XEfCJDp8kareSBg" mediniIdentifier="_hloWcX2XEfCJDp8kareSBg" ISO26262_location="Home" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Plug-in at home every night in a closed garage is the dominant charging routine for Indian owners; hence the hazard is present on most days → E4.&#xD;&#xA;&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmzitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hludEH2XEfCJDp8kareSBg" mediniIdentifier="_hludEH2XEfCJDp8kareSBg" id="HE220" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="Assuming that the battery has been Fast Charge in High Temperatures and then discharge">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hludEX2XEfCJDp8kareSBg" mediniIdentifier="_hludEX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Only Driver + Low Traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="High-speed riding in hot weather during inter-city trips is common in summer months and happens multiple times per year for a typical rider → E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmsCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hlzVkH2XEfCJDp8kareSBg" mediniIdentifier="_hlzVkH2XEfCJDp8kareSBg" id="HE221" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E4" ISO26262_exposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hlzVkX2XEfCJDp8kareSBg" mediniIdentifier="_hlzVkX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Charging" ISO26262_defaultExposure="E4" ISO26262_defaultExposureComment="Normal charging—irrespective of environment—accompanies each duty cycle (often nightly), meaning the situation exists on most days → E4.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hl4OEH2XEfCJDp8kareSBg" mediniIdentifier="_hl4OEH2XEfCJDp8kareSBg" id="HE222" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E3" ISO26262_exposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hl4OEX2XEfCJDp8kareSBg" mediniIdentifier="_hl4OEX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Paved" ISO26262_environment="High temperature" ISO26262_trafficAndPeople="Driver+Pillion + Low traffic" ISO26262_itemUsage="Drive" ISO26262_defaultExposure="E3" ISO26262_defaultExposureComment="Two-up, hot-weather highway riding is typical for weekend outings and vacations; occurs several times each season ⇒ E3.&#xD;&#xA;" user_speed="High speed"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmtitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hl9GkH2XEfCJDp8kareSBg" mediniIdentifier="_hl9GkH2XEfCJDp8kareSBg" id="HE223" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hl9GkX2XEfCJDp8kareSBg" mediniIdentifier="_hl9GkX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Any Road Condition" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Parked" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="The bike remains parked outdoors and unattended only during shopping trips or office hours, which form a small slice of total operating time → E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmyitLEfCMc_2Esfz5fQ"/>
  </hazardElements>
  <hazardElements xsi:type="hazardmodel:HazardousEvent" xmi:id="_hmBYAH2XEfCJDp8kareSBg" mediniIdentifier="_hmBYAH2XEfCJDp8kareSBg" id="HE224" ISO26262_severity="S0" ISO26262_severityComment="" ISO26262_exposure="E2" ISO26262_exposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" ISO26262_controllability="C3" user_Assumptions="">
    <hazard href="../failures/_$Hazards$_RzcHQaljEeCaHInwqwM1Vg.failures#_wgT5kDo_Ee2fTugI974vXw"/>
    <operationalSituation xsi:type="hazardmodel:OperationalSituation" xmi:id="_hmBYAX2XEfCJDp8kareSBg" mediniIdentifier="_hmBYAX2XEfCJDp8kareSBg" ISO26262_location="Any location" ISO26262_roadConditions="Confined spaces" ISO26262_environment="Any environment" ISO26262_trafficAndPeople="Any Person in Vicinity +Any traffic" ISO26262_itemUsage="Service / breakdown" ISO26262_defaultExposure="E2" ISO26262_defaultExposureComment="Service or breakdown situations (puncture repair, workshop visits) surface only a handful of times over the scooter’s life → low probability ⇒ E2.&#xD;&#xA;" user_speed="Not Moving"/>
    <malfunctions href="../sysml/_NLA9YG3hEeGyZ5eYlZakUA.sysml#_qIfoQHgZEfCLxJ6MsRw7Dg"/>
    <template href="../commons/_rSuvoCseEfCMc_2Esfz5fQ.ha#_2kPmwCtLEfCMc_2Esfz5fQ"/>
  </hazardElements>
</hazardmodel:HazardAnalysisModel>
